;dvb7700all.INF --  Copyright 2000 YUAN

[Version]
signature	= "$CHICAGO$"
Class		= Media
ClassGUID	= {4d36e96c-e325-11ce-bfc1-08002be10318}
Provider	= %Dibcom%
DriverVer	= 05/22/2009,2.3.3.31
CatalogFile.ntamd64  = dvb7700all.cat


[Manufacturer]
%MfgName% = DIBCOM,NTamd64

[DIBCOM.NTamd64]
%MC872.DeviceDesc%     = MOD7000.Device,USB\VID_1164&PID_1E8C          ; B(C) version + 2260 dual
%MC872_1D.DeviceDesc%  = MOD7000.Device,USB\VID_1164&PID_2EDC          ; C version + 2260 single
%MC770A.DeviceDesc%    = MOD7000.Device,USB\VID_1164&PID_1F08          ; C version + 843 + 3028, WITH AV S & WITH FM
%MC770A.DeviceDesc%    = MOD7000.Device,USB\VID_1164&PID_1F06          ; C version + 843 + 3028, WITH FM
%MC770A.DeviceDesc%    = MOD7000.Device,USB\VID_1164&PID_1EFE          ; C version + 843 + 3028, WITH AV S
%MC770A.DeviceDesc%    = MOD7000.Device,USB\VID_1164&PID_1EFC          ; C version + 843 + 3028
%MC570QA.DeviceDesc%   = MOD7000.Device,USB\VID_1164&PID_2F08          ; ATSC + 843 + 5000, WITH AV S & WITH FM
%MC570QA.DeviceDesc%   = MOD7000.Device,USB\VID_1164&PID_2F06          ; ATSC + 843 + 5000, WITH FM
%MC570QA.DeviceDesc%   = MOD7000.Device,USB\VID_1164&PID_2EFC          ; ATSC + 843 + 5000
%MC570QA.DeviceDesc%   = MOD7000.Device,USB\VID_1164&PID_2EFE          ; ATSC + 843 + 5000, WITH AV S
%MC378H.DeviceDesc%    = MOD7000.Device,USB\VID_1164&PID_3EDC          ; DVBT   MC378 / PD378 Series
%PD770A.DeviceDesc%    = MOD7000.Device,USB\VID_1164&PID_4EFC          ; DVBT + 843 + 4000, NO AV S & NO FM
%PD770A.DeviceDesc%    = MOD7000.Device,USB\VID_1164&PID_4EFE          ; DVBT + 843 + 4000, WITH AV S & NO FM
%PD770A.DeviceDesc%    = MOD7000.Device,USB\VID_1164&PID_4F06          ; DVBT + 843 + 4000, NO AV S & WITH FM
%PD770A.DeviceDesc%    = MOD7000.Device,USB\VID_1164&PID_4F08          ; DVBT + 843 + 4000, WITH AV S & WITH FM
%MC770B.DeviceDesc%    = MOD7000.Device,USB\VID_1164&PID_6EFC          ; DVBT + 4910 + 4000, NO AV S & NO FM
%MC770B.DeviceDesc%    = MOD7000.Device,USB\VID_1164&PID_6EFE          ; DVBT + 4910 + 4000, WITH AV S & NO FM
%MC770B.DeviceDesc%    = MOD7000.Device,USB\VID_1164&PID_6F06          ; DVBT + 4910 + 4000, NO AV S & WITH FM
%MC770B.DeviceDesc%    = MOD7000.Device,USB\VID_1164&PID_6F08          ; DVBT + 4910 + 4000, WITH AV S & WITH FM
%MC470.DeviceDesc%     = MOD7000.Device,USB\VID_1164&PID_2F0A          ; ATSC Only, mxl5007 + 1411



[DestinationDirs]
MOD7000.CopyDrivers = 10,System32\Drivers 
MOD7000.CopyDll = 11


[SourceDisksNames]
1 = %INSTALLATION_DISK%,,

[SourceDisksFiles]
dvb7700all.sys = 1
avfcp.ax=1

[ControlFlags]
ExcludeFromSelect    = *
ExcludeFromSelect.NT = *

[MOD7000.Device.NT]
Include    = ks.inf, kscaptur.inf, bda.inf, wdmaudio.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = MOD7000.AddReg
CopyFiles  = MOD7000.CopyDrivers,MOD7000.CopyDll
RegisterDlls = MOD7000.RegAX

[MOD7000.Device.NT.HW]
AddReg = MOD7000_DEVICE_AddReg


[MOD7000.Device.NT.Services]
Addservice = mod7700, 0x00000002, MOD7000.AddService


[MOD7000.AddService]
DisplayName    = %MOD7000.FriendlyName%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\dvb7700all.sys
LoadOrderGroup = Base
AddReg         = MOD7000.Service.AddReg


[MOD7000.Service.AddReg]
HKR,,DigitalJmp,0x00010001,0x00


[MOD7000.CopyDrivers]
dvb7700all.sys

[MOD7000.CopyDll]
avfcp.ax

[MOD7000.RegAX]
11,,avfcp.ax,1


[MOD7000.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,dvb7700all.sys
HKR,,PageOutWhenUnopened,3,01
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D}
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D},Name,,"Tuner Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F}
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F},Name,,"Demodulator Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81}
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81},Name,,"Antenna In Pin"
;avfcp.ax
HKLM,System\CurrentControlSet\Control\MediaInterfaces\{868de3d7-1ed1-4698-af07-0a4b57662572},,,"Notify Copy Protect Filter"
HKLM,System\CurrentControlSet\Control\MediaInterfaces\{868de3d7-1ed1-4698-af07-0a4b57662572},IID,1,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00

[MOD7000_DEVICE_AddReg]
HKR,,"ProductId",0x00010001,0x00000000
HKR,,"MaskDevicePath",0x00010001,0x00000000
HKR,,"BdaDigCaptureFilterName",0,"DiBcom BDA Digital Capture"
HKR,,"BdaDigTunerFilterName",0,"DiBcom BDA Digital Tuner"
HKR,,"AnlgTunerFilterName",0,"DiBcom BDA Analog TV Tuner"
HKR,,"AnlgCaptureFilterName",0,"DiBcom BDA Analog Capture"
HKR,,"AnlgXBarFilterName",0,"DiBcom BDA Analog Xbar"
HKR,,"AnlgTVAudioFilterName",0,"DiBcom BDA Analog TV Audio"
HKR,,"ControlFilterName",0,"DiBcom Control Filter"


[Strings]

Dibcom               	= "YUAN"
MfgName              	= "YUAN"
MOD7000.FriendlyName 	= "DiBcom DIB7700 based TV tuner device"
INSTALLATION_DISK    	= "YUAN Installation Disk"
MC872.DeviceDesc        = "YUAN MC872 Dual DVB-T Tuner"
MC872_1D.DeviceDesc     = "YUAN MC872-1D/MC872 DVB-T Tuner"
MC770A.DeviceDesc       = "YUAN MC770A DVB-T/Analog Hybrid Tuner"
PD770A.DeviceDesc       = "YUAN PD770A DVB-T/Analog Hybrid Tuner"
MC770B.DeviceDesc       = "YUAN MC770B DVB-T/Analog Hybrid Tuner"
MC570QA.DeviceDesc      = "YUAN MC570QA ATSC/Analog Hybrid Tuner"
MC378H.DeviceDesc       = "YUAN MC378/PD378S Series DVB-T Tuner"
MC470.DeviceDesc        = "YUAN MC470/PD470 Series ATSC Tuner"
;
; The following items should be moved to KS_registration - TCP
;

MediaCategories         = "SYSTEM\CurrentControlSet\Control\MediaCategories"
    

;
; ServiceType values
SERVICE_KERNEL_DRIVER			= 0x00000001
SERVICE_FILE_SYSTEM_DRIVER		= 0x00000002
SERVICE_ADAPTER				= 0x00000004
SERVICE_RECOGNIZER_DRIVER		= 0x00000008
SERVICE_WIN32_OWN_PROCESS		= 0x00000010
SERVICE_WIN32_SHARE_PROCESS		= 0x00000020
SERVICE_INTERACTIVE_PROCESS		= 0x00000100
SERVICE_INTERACTIVE_SHARE_PROCESS	= 0x00000120

; StartType values
SERVICE_BOOT_START          = 0x00000000
SERVICE_SYSTEM_START        = 0x00000001
SERVICE_AUTO_START          = 0x00000002
SERVICE_DEMAND_START        = 0x00000003
SERVICE_DISABLED            = 0x00000004

; ErrorControl values
SERVICE_ERROR_IGNORE        = 0x00000000
SERVICE_ERROR_NORMAL        = 0x00000001
SERVICE_ERROR_SEVERE        = 0x00000002
SERVICE_ERROR_CRITICAL      = 0x00000003

; Characteristic flags
NCF_VIRTUAL                 = 0x0001
NCF_WRAPPER                 = 0x0002
NCF_PHYSICAL                = 0x0004
NCF_HIDDEN                  = 0x0008
NCF_NO_SERVICE              = 0x0010
NCF_NOT_USER_REMOVABLE      = 0x0020
NCF_HAS_UI                  = 0x0080
NCF_MODEM                   = 0x0100

; Registry types
REG_MULTI_SZ                = 0x10000
REG_EXPAND_SZ               = 0x20000
REG_DWORD                   = 0x10001

; Win9x Compatible Types
REG_BINARY                  = 17
REG_SZ                      = 0

; Service install flags
SPSVCINST_TAGTOFRONT        = 0x1
SPSVCINST_ASSOCSERVICE      = 0x2
