> Intel® Rapid Storage Technology 9.5.6.1001 Production Version

> Release Notes

> > 4 January 2009
> > DISCLAIMER: Information in this document is provided in connection with Intel products. No license, express or implied, by estoppels or otherwise, to any intellectual property rights is granted by this document. Except as provided in Intel’s Terms and Conditions of Sale for such products, Intel assumes no liability whatsoever, and Intel disclaims any express or implied warranty relating to sale and/or use of Intel products, including liability or warranties relating to fitness for a particular purpose, merchantability or infringement of any patent, copyright or other intellectual property right. Intel products are not intended for use in medical, lifesaving, or life-sustaining applications.

> > Intel may make changes to specifications and product descriptions at any time, without notice.

> > Contact your local Intel sales office or your distributor to obtain the latest specifications and before placing your product order.
> > * Other names and brands may be claimed as the property of others.
> > Copyright © Intel Corporation 2000-2009

> > NOTE: This release is a combination of 9.5.6.1001 driver and 9.5.6.1002 UI. The UI version will show as 9.5.6.1002 and the driver version is shown as 9.5.6.1002 driver

> > Supported Operating Systems

> > Microsoft Windows 7*

> > Microsoft Windows 7 x64 Edition*

> > Microsoft Windows Vista*
> > Microsoft Windows Vista x64 Edition*
> > Microsoft Windows XP Home Edition*
> > Microsoft Windows XP Professional*
> > Microsoft Windows XP x64 Edition

> > Microsoft Windows Server 2008* ++
> > Microsoft Windows Server 2008 x64 Edition*++
> > Microsoft Windows Server 2003* ++
> > Microsoft Windows Server 2003 x64 Edition*++

> > Microsoft Windows Media Center Edition*

> > > ++ Not available on mobile platforms

> > > Revision History

> > > Date | Driver Revision | Build Number
> > > 4 January 2009 | 9.5.6.1001 Production Version | 1001

> > > Notes:

> > > 1. A Vista OS Installation using a Matrix RAID Array on a system with a 9.5 or newer OROM requires the user to F6 a 9.5 driver.

> > > 2. Possible issue where RST is slow to start on Windows XP or Vista with .NET 3.0

> > > Issue description: Under certain network conditions, on systems with .NET 3.0, the RST application and notification icon (a.k.a. tray icon) may take about a minute to start.

> > > Resolution: Contact Microsoft* to receive the hot fix described by KB article 936707 or upgrade to .NET 3.5.

> > > 3. Possible Issue regarding File writes on Windows XP with Service Pack 2

> > > Issue description: System hangs, ERROR_NO_SYSTEM_RESOURCES or ERROR_NOT_ENOUGH_QUOTA observed when writing large numbers of files on Windows XP with Service Pack 2.

> > > Resolution: Contact Microsoft* to receive the hot fix described by KB article 888413.

Resolved Issues

Resolved Issues in 9.5.6.1001 Production Version
Reference No | Description | Affected OS's
3005294 | ESATA HDD is not detected in the second hot attach | Vista, Vista-64, Win7, Win7-64
3005389 | UI displayed incorrect UI for Chinese HK | Vista, Vista-64, Win7, Win7-64
3005358 | BSOD D1, 7E on iaStor when hot unplug particular eSATA drives | Vista-64, Win7
3005360 | 0xD1 BSOD seen intermittently during S4/S3 power cycling | Vista, Vista-64, Win7, Win7-64
3005350 | RST Driver fails with F6 install using specific Hard Drive | Win7
3005363 | BSOD 0xCC during DTM Common Scenario Stress Test | Vista, Vista-64, Win7, Win7-64
3005347 | WHQL: 0x70860002 BSOD on legacy platform RAID configurations | Vista, Vista-64, Windows2003, Windows2003-64, Windows2008, Windows2008-64, Windows XP, Windows XP-64
3004782 | With UAC enabled in Vista/Win7 if you select 'Cancel' after launching RST UI a Failure pop-up appears instead of graceful discontinue | Vista, Vista-64, Win7, Win7-64,
3005106 | 0x70860002 BSOD occurred during reboots | Vista, Vista-64, Win7, Win7-64,
3005163 | No C6 state maintained after ejecting ODD | Vista, Vista-64, Win7, Win7-64,
3005209 | For IRRT system, cannot rebuild to another disk (non-RAID HDD) with dock drive | Vista, Vista-64
3005211 | When in the RST UI, an error message pops up when clicking the Intel download center link | Vista, Vista-64, Win7, Win7-64, Windows 2003, Windows 2003-64, Windows 2008, Windows XP
3005251 | 0x9F BSOD during Passmark HD stress test | Vista
3005261 | 0cD1 BSOD when running Passmark HD stress test | Win7, Win7-64,
3005271 | 0x0A and 0xD1 BSOD appear during system imaging process | Win7
3005296 | Multiple BSODs and hangs (0xC5, 0xCC and others) occur running stress tests | Vista, Vista-64, Win7, Win7-64, Win-XP
3005325 | 0x3B BSOD when running Passmark HD stress test and verifier | Win7, Win7-64,
Resolved Issues in 9.5.0.1037 Production Candidate
Reference No | Description | Affected OS's
3005025 | RST 9.5 install to Matrix RAID results in OS loss, OROM reports HDDs as Incompatible – platform specific (ICH8R, ICH8MR and ESB2) | Vista, Vista-64, Win7, Win7-64, Windows 2003, Windows 2003-64, Windows 2008, Windows 2008-64, Windows XP, Windows XP-64
3005049 | RAID Option ROM loses disk info with specific hard disk drives | N/A
3005058 | Peforming hot plug events while IO flood to RAID1/RAID1 matrix arrays with mirror drives missing sometimes results in a 0x9086 BSOD | Vista-32
3005064 | System will hang up with Norton Internet Security Installed | Win7-64
3005072 | 0xD1 BSOD observed sporadically during extended hibernation (S4) testing | Windows XP
3005083 | SCSI Compliance commands stall against RAID pass-through | Vista-32, Vista-64, Windows 2008, Windows 2008-64
3005084 | RAID Option ROM does not recognize RAID volumes on auto-reboot following system crash | Vista, Vista-64, Win7, Win7-64, Windows 2003, Windows 2003-64, Windows 2008, Windows 2008-64, Windows XP, Windows XP-64
Resolved Issues in 9.5.0.1034 Production Candidate
Reference No | Description | Affected OS's
3005042 | Driver incorrectly setting RAID1 attribute in metadata for a RAID10 volume and an IRRT volume | Vista-64
3004556 | Bad Block I/O timeout (and data miscompare) during VERFIY 24-25% | Win7
2723864 | Data miscompare during bad block raid1 error injection test | Vista, Windows 2003, Windows 2008
3004713 | Disk selection not shown when attempting to add disk to 2 RAID 5 volumes on the same array | Vista
3004780 | When hot swapping HDD for ODD, the HDD is detected as a 'Removable Disk' and is not usable | Win7, Windows XP
3004809 | Intel® RST drops and detects SATA ports after S3 resume | Vista, Vista-64, Win7, Win7-64
2688344 | Removdrv.txt states that the mobile platform does not support RAID | Vista
3005049 | OROM losing disk info with Hitachi Deskstar DLA | None
3004886 | IRST driver needs to implement a "busy" state during device enumeration | Vista, Vista-64, Win7, Win7-64
3004889 | WHQL: Storage Query Property testing failing during StorageAdapterProperty query (BLOCKING) | Vista, Vista-64, Win7, Win7-64, Windows 2008, Windows 2008-64
3004910 | Intel® RST UI shows status of "Unknown" for continuous BrokenClone IRRT Volume | Win7
3004937 | Spanned RAID1 Volume not setting all disks to incompatible in RAID OROM | N/A
3004939 | Error Injection Causes Drive to Appear Failed, Appear Removed, or BSOD | Vista
3004952 | 0xC4 BSOD intermittently seen while running the test of System-Common Scenario Stress with IO overnight | Vista
3004956 | SGPIO: System locks up while doing a rebuilding of a Raid 5 Volume | Vista-64
3004967 | UI does not detect driver "busy" state | Vista, Win7, Windows XP
3004975 | BSOD 0xC9 (0x224) during WLK 1.4 Common Scenario Stress when booting to 3rd party controller | Win7
3004497 | WHQL: BSOD (StopCode 0x50) during Dynamic Partitioning Hot-Add CPU testing | Windows 2008-64
3004665 | DLAE and ATAPI bits aren't set for the port connected with ODD. | Vista
3004771 | Multiple hot-plugs of disks in same volume in between hardware scans causes 0x7E BSOD | Vista, Win7, Win7-64
3004897 | RaidCfg32 does not allow creation of a volume to span internal and external ports when the BCFS bits are configured to support/allow it | Vista
3004812 | RAID 1 creation with NTFS partition on one of the disks fails | Windows XP
3004654 | 0xD5 BSOD when hot unplugging E-SATA device | Win7, Win7-64
3004801 | IRRT allows invalid config but then gives an error message when trying to create. | Windows XP
3004852 | Managing a RAID 0 volume with available pass thru disks crashes the UI | Vista, Vista-64, Win7, Win7-64, Windows XP, Windows XP-64
3004611 | ODD drive does not display Serial number in mouse over tool tip for some ODDs | Vista, Vista-64
3004668 | UI displays an ‘add disk’ option when it should not be displayed. | Vista
3004688 | Unknown error occurs when creating an IRRT vol using 1.5TB drives | Vista, Win7
3004715 | UI allows attempt to change a RAID 1 volume to an IRST volume with another RAID volume present. | Vista
3004572 | UI allows entering 5 invalid passwords for Locked drives when 3 is the Max. | Vista
3004695 | BSOD 0x8086 occurred when open Roxio/ Creator Business DVD. | Win7
3004709 | Manage Disk does not refresh usage if Swap master and recovery disks pressed and Manage Disk is checked immediately | Vista, Win7
3004716 | UI should prevent disk actions on an array disk when the array is busy | Vista
3004735 | Recovery volume that recovers its master to a new disk shows 3 disks in the volume the master, recovery, and a missing disk | Win7-64
2553818 | ISDI returns success after failing to mark a disk as pass-thru after volume deletion | Vista
2688638 | Intel(R)RST: NAI Informational Balloon Message is Erroneous for device addition and removal | Windows XP
2724309 | BSOD 0x50 on XP32 | Windows XP
3004419 | With disc inserted, ATAPI device shows no memory usage or availability | Win7
3004492 | UI graphic for a disk removed from a volume is a green circle with a white checkmark | Win7, Win7-64
3004534 | UI graphic for a failed disk is a yellow bang with exclamation mark | Win7-64
3004550 | Drive icons do not update dynamically when disk fails or is reset | Win7
3004474 | WHQL: INF Test failure due to format of date captured in Driver Verifier | Vista, Vista-64, Win7, Win7-64, Windows 2003, Windows 2003-64, Windows 2008, Windows 2008-64, Windows XP, Windows XP-64
3004545 | BSOD occurs when unlocking drives from the UI | Vista, Win7
3004562 | Clicking Search button twice displays different information | Win7
3004573 | Cannot unlock drives in the UI after entering Max invalid passwords and rebooting | Vista
3004575 | UI displays "Update Mode: Continuous" incorrectly after hot unplugging Master disk from Intel® RRT | Vista-64,Win7,Windows XP
3004618 | UI allows the user to set the master and recovery disk as the same disk | Vista, Vista-64
3004675 | Moving internal drive to external drive on IbexPeak mobile causes UI failure | Vista-64
Resolved Issues in 9.5.0.1023 Beta
Reference No | Description | Affected OS's
2552010 | CSMI Smart IOCTL sent only to port 0 from middleware | WindowsXP
2662621 | A bootable 6 disk RAID10 can be created using ‘Create RAID Volume from Existing Hard Drive’ | WindowsXP
2688583 | Intel® RST User Interface Password Protected Status is Shown as Unknown | Vista, WindowsXP-64
2688650 | User Interface system report does not show password protected Hardware Information | Vista, WindowsXP-64
2724483 | Many Modal dialogs do not respond to Escape key to close dialog | WindowsXP
2724074 | The Preference Screen in the UI does not warn of changes if UI is closed | WindowsXP
2724243 | User Interface Tray Icon Shows Busy Icon When a Locked Volume is Present | Vista
2724264 | User Interface is not showing lock icon on locked volume | Vista
2724334 | Intel® RST UI does not prevent the user from attempting to create a spanned volume | Vista, Win7 & WindowsXP
2724368 | Driver does not set the LPM.ASP bit correctly when SALP=0 | WindowsXP
2724388 | Intel® Rapid Storage Technology UI takes about one minute to open in Win 7 | Win7-64
2724444 | Unable to create a RAID 0 or 1 volume from existing disks in the UI when one is an SSD | Vista
2724474 | User Interface does not allow user continue volume creation if disks are selected in descending order when attempting to create a RAID0 or 1 | Win7
2724480 | Help-the Customizing Notifications link in Notification Area content closes the entire App | Vista
2688357 | SATA LPM Issue: Seagate HDD and PHY Calibration | Vista, WindowsXP
2688714 | RAIDCPLY tool fails tests 6.1 and 6.3 even though the RAID OROM is loaded | DOS
2724029 | S4 causing BSOD 9086 after removal of eSATA HDD | Vista, Win7-32&64
2724065 | BSODs with S3/S4 and/or hot plug | Vista
2724083 | Graphic is cut in the Help file Volume type page | Vista
2724110 | Intel® RRT is unable to boot from recovery drive (when enabled in OROM) after mounting partner disk in UI | Vista, Win7
2724230 | Set SGPIO LED defaults to off | Vista, Windows2003
2724232 | Multiple Interrupts and missed hot plug insertion | Vista
2724239 | SATA transfer mode for ATAPI device does not display in Mbyte/sec | Vista
2724312 | No improvement seen on boot time with Braidwood | Vista
2724330 | When disks are connected through Internal PM, info tip displays internal PM as internal | Vista, Win7 & WindowsXP
2724346 | Volume Graphic Shows an Incorrect Capacity Representation for Various RAID Levels | Vista
3004337 | User Interface should not allow Recovery Disk Creation from a Maximized-Mode cached volume | Vista, Win7
3004358 | Driver AHCI bugcheck when booting on a non-PCH system | Vista, WindowsXP
2688484 | Middleware doesn't check for error when converting between IRRT and RAID1 | WindowsXP
2723544 | Intel® MSM driver not updating previous task file register values | WindowsXP
2723555 | User Interface does not warn user about exceeding 2TB limit when RAID Option ROM does not include that support | Vista
3004395 | Add 2 TB limit/warning to create page | Vista-32&64, Win7-32&64, Windows 2003-32&64, Windows 2008-32&64, WindowsXP-32&64
2723816 | User Interface error shown when attempting to unlock a disk | Vista, WindowsXP
2724014 | ODD doesn't consistently get detected w/Warm Swap during S3 and platform fails to enter S3 anymore afterwards | WindowsXP
2724060 | Recovery volume is not visible when Access Recovery Volume selected in Win7. | Win7
2724270 | Save button for System Report is difficult to see | Vista-32&64, Win7-32&64, Windows 2003-32&64, Windows 2008-32&64, WindowsXP-32&64
3004401 | User Interface Help Section is missing how to Synchronize Maximized disks/volumes using OROM UI | Vista
3004462 | "adding a disk" link in "managing volumes" section in help file does not work properly | Win7
3004411 | OROM does not support two digit major/minor version numbers (ie: 8.10, 10.0, etc) | N/A
3004425 | Strip size drop down should not display for RAID1 in Create Configure Volume and Change Type dialog | Vista, Win7 & WindowsXP
3004428 | OROM loses bad block log when initiating rebuild | Vista
3004473 | IO timeout followed by a sync section IO can result in system hang | Vista
2724382 | User Interface mishandles serial numbers that are longer than 15 characters | Win7-64
3004370 | Hot plugging of multiple HDDs results in system lock up and return a 9086 BSOD | Win7
3004403 | System Report shows "RAID" info when in "AHCI" mode | Vista
3004465 | The "Accessing Disk Files" in Index section of help page contains the Link “Accessing Disk Files” | Win7
3004468 | In the help window, the "Degraded Volumes" page has a link "Failed Volumes" which is a link back to "Degraded Volumes" | Win7
3004458 | Removdrv.txt file needs to be updated with Ibexpeak controller names | Vista, Win7 & WindowsXP
3004490 | User Interface Displays “None” Under “Password Protected:” | Win7
3004482 | Help page contents is missing an "online support section" in left contents tree | Win7
2724318 | C9 BSOD When trying to access files from an On Request Recovery volume | Win7-64
3004363 | BSOD occurs when the head unload in HDD occurs while entering hibernation | WindowsXP, Vista-32&64
3004459 | Delayed OROM log processing affects boot performance | Vista
3004499 | System Hang / Crash (BSOD Stop Code 0x3B) during SCSI Compliance testing | Vista-32&64, Win7-32&64, Windows 2003-32&64, Windows 2008-32&64
3004503 | User Interface allows R1 rebuild to a disk that is too small | Vista
3004571 | 0xD1 BSOD on system boot | Win7

Known Issues

Known Issues in 9.5.6.1001 Production Version |
Reference No | Description | Affected OS's
3004935 | 0xD1 BSOD observed at times when performing S4 extended cycling | Win7-64
3004995 | Access violation seen at times when running WHQL Common Stress Scenario w/IO test overnight | Win7
3005020 | ODD disappears when the media eject button is pressed | Win7
3005036 | Running stress tests cause one hard drive to fail and cause RAID1 volume to degrade | Vista
2554217 | IOMeter sequential writes on 6-disk R5 slow with WBC disabled | Vista,Vista-64,Win2000,Win7,Win7-64,Windows 2003,Windows 2003-64,Windows Media Center,Windows XP,Windows XP-64
2556715 | Intel® Rapid Recover Technology: sync does not automatically re-start upon re-plugging the master disk into a system with a degraded recovery volume that was in the middle of syncing the data on the master and recovery drives while in manual sync mode | Vista-64
2556766 | Modification of one volume fails during migration of a different volume | Vista,Vista-64,Windows 2003,Windows XP,Windows XP-64
2556799 | Intel(R) Rapid Recover Technology: Fast sync log is corrupt if no data is written to the master drive of the IRRT volume | Vista-64
2557006 | Marking mounted recovery disk as spare is allowed when it should not be | Windows XP
2688459 | HDDPWD-BSOD 0xD5 After Disconnecting Unlocked PWD Drive During Rebuild | Vista-64
2688463 | HDDPWD-After Entering BIOS Password for Locked Disk During Resume from S4 Disk/Volume is still Locked | Windows XP-64
2688466 | HDDPWD-After Disconnecting Locked Disk From Redundant RAID Volume the Volume is Shown as Degraded But is Not Exported to OS | Windows XP-64
2688483 | Driver proceeds with volume creation if disk is missing | Windows XP
2688639 | Splash Screen Not Shown When UI is Started For the First Time During a Login Session | Vista-64,Windows XP-64
2688691 | Metadata is stored on target HDD when the UI blocks creation of IRRT volume | Vista
2724057 | Creation of a RAID 1 volume from OS drive hangs then fails the source drive and on reboot if you mark the failed disk as normal the rebuild will complete and work as expected. | Vista,Win7
2724103 | 0x7B BSOD when attempting to boot from a RAID-boot volume with a locked drive | Vista,Vista-64,Win7,Win7-64,Windows XP
3004463 | The AHCI register (PxSctrl) is being written without a read first. | Vista
3005048 | Inf strings remains in English until going through Name translation process | Vista
2723619 | Help file Index is not alphabetizing correctly in CHS, CHT | Vista- 32&64
2723625 | JPN, KOR, CHS, CHT characters are displayed as if they are Bolded throughout UI & Help in XP | WindowsXP
2723856 | ARA/HEB Help page Arrow icon is not following the correct layout | Vista
3004750 | Event Viewer - Service started successfully txt is not localized on localized XP | Windows XP
3004690 | OROM doesn't always destroy metadata | Vista,Vista-64,Win7,Win7-64,Windows XP,Windows XP-64
3004874 | Two disk RAID 0 with one disk password protected and lock, shows as three disks in Disk Manager | Win7
3004898 | BSOD when running raidcfg32 from batch file. Issue occurs after immediately deleting an IRRT volume after the volume creation completes | Vista
3004899 | IRST displays incorrect error message when booted in Safe Mode | Win7,Win7-64
3004902 | When True E-SATA drive is connected, erratic disk behavior is present in UI and disk manager | Windows XP,Windows XP-64
3004911 | Automatically, Rebuild from Continuous Degraded Normal IRRT State when Master Disk attached begins | Win7
3004916 | Master disk is incorrectly set as Smart error after rebuild if recovery disk has smart error | Win7
3004944 | Manage Volume status does not update from Add Disk if more help is launched from Add Disk dialog | Windows XP
3004982 | Master Disk Fails during RAID volume creation (R1/R5/IRRTC) | Vista,Vista-64,Windows XP,Windows XP-64
3004992 | Drive Information of Hover windows is incomplete once Drive is a member of any Raid Volume | Vista,Vista-64
3004994 | UI Does Not Display Correct String when Invalid Password Entered 5 Times Or More on Locked Drive | Win7
3005002 | 0x70860002 BSOD intermittently seen when performing multiple hot plug insertions/removals of drive while performing extended S3 cycling | Vista
3005026 | 0x9F BSOD intermittently when running extended S3 cycling and IO | Win7
3005033 | 0x7E BSOD observed sporadically when hot unplugging E-SATA drive multiple times | Win7
3005058 | BSOD 0x9086 intermittently seen when hot plugging while IO flood to RAID1/RAID1 matrix arrays with mirror drives missing | Vista
2688162 | DISABLE WRITE CACHE is sent to ATAPI device during hardware scan. | Vista,Vista-64
2688381 | RAID F6 driver install twice issue | ,Vista
2688481 | Errors seen after volume data verification on expanded RAID volumes | Windows XP,Vista
2688495 | Flush Cache is sent to ATAPI device when it shouldn't | Vista,Vista-64
2688509 | Automatically DVD playing fail to start with showing Windows error Dialog. | Vista
2723901 | SGPIO defaults not functioning as described in the Intel® Matrix Storage Manager 8.5 PRD and OEM Technical Guide | Windows 2008
2723967 | iaStor System event log, event id 9 seen under various scenarios | Windows XP
2724026 | Event ID 9 "iaStor" error in the system log | Windows XP,Vista
2724125 | Event ID 9 of iastor occurs during heavy IO on AHCI system. | Windows 2003
2724413 | SATA ODD intermittently disappears from Intel Matrix Storage Console upon resuming from S3 on ICH9M | Vista
2724524 | Hot plug removals of eSATA devices are sometimes not detected | Vista
3004378 | 9.5.0.1016 default for cache is disabled | Vista
2688533 | 0x7E BSOD occurs after hotplug event with disks from different IRRT volumes | Vista
2688639 | Splash Screen Not Shown When UI is Started For the First Time During a Login Session | Vista-64,Windows XP-64
2688648 | RAID10 fail to rebuild after recovery from a 2 disk failed state | Vista,Vista-64
2688756 | Removdrv.txt Not Shown When Uninstalling Intel® RST | Vista,Vista-64,Windows XP,Windows XP-64
2723557 | Full array expansion w/ new disk fails while doing IO | Vista,Vista-64,Windows XP-64
2723575 | ‘Intel’ Start menu folder not deleted after uninstall of Intel® RST | Vista,Vista-64,Windows XP,Windows XP-64
2723591 | Driver doesn't delete partition after deleting volume during migration | Windows 2008
2723596 | 0x7E BSOD when hot plugging Intel(R) RRT member disk during volume update. | Vista
2723632 | Installer displays incorrect string "Intel(R) ESB2 SATA RAID Controller" when overwriting newer driver | Vista
2723634 | System BSOD if middleware transfer buffer is smaller than requested driver parameter table. | Vista
2723557 | Full array expansion w/ new disk fails while doing IO | Vista,Vista-64,Windows XP-64
2723869 | >2TB single disk passthru support does not work properly | Vista-64
2723887 | Disk goes into unknown state when expanding volume | Vista-64,Windows XP
2723982 | Volume is Stuck in a Verifying and Repairing Loop While PATIN Runs Following Dirty Shutdown | Windows XP
2723990 | System Hangs While Performing Volume Expansion | Windows XP,Windows XP-64
2724018 | Restart after capacity expansion fails on 2TB testing | Win7
2724020 | PCH Desktop System locks up during migration and expansion | Windows XP
2724072 | PCH Desktop fails transition from MIGRATING TO NORMAL after RAID Expansion | Win7
2724082 | After S3/S4 a Previously Unlocked Volume is Shown as Locked But is Exported to OS | Win7-64
2724182 | Iastor needs to backpocket address spaces to use in low memory conditions | Vista,Vista-64,Win7,Win7-64
3004418 | Flash memory module is randomly no longer seen by the Intel® RST OROM | Vista
3004477 | WHQL: 0x50 BSOD upon reboot when Driver Verifier is enabled against iastor.sys | Windows XP
3004479 | Platform BSOD 0x9086 while entering S3/S4 (SI-3726*) | Vista
3004484 | System BSOD after Hot plugging a raid member drive with code of D1 (SI 3726*) | Win7-64
3004485 | Performance on a 4-disk RAID 5 with one disk failed is poor | Vista
3004567 | Driver sending ATA commands to devices which don’t support the commands | Vista