;Autogenerated INF
;
; Intel Wireless WiFi Link Adapters
; Installation Script for WinT
;
; Copyright (C) 1997-2024 Intel Corporation. All rights reserved.
;
; The information and source code contained herein is the exclusive
; property of Intel Corporation and may not be disclosed, examined
; or reproduced in whole or in part without explicit written authorization
; from the company.
;
;------------------------------------------------------------------------------
;
;******************************************************************************
; Version Section
;------------------------------------------------------------------------------

[Version]
Signature            = "$Windows NT$"
Compatible           = 1
Class                = net
ClassGUID            = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider             = %PROVIDER_NAME%
DriverVer            = 05/01/2024,23.60.1.2 ;DATE HAS TO BE IN FOLLOWING FORMAT MM/DD/YYYY
PnPLockdown          = 1
CatalogFile          = Netwtw08.cat


[Manufacturer]
%COMPANY_NAME%       = Device, NTamd64.10.0...17735


[Device.NTamd64.10.0...17735]
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F0&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F0&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F0&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F0&SUBSYS_007C8086 ; AX
%NIC_101_1x1_AX_no_160% = Install_GEN_SLR_HrP1_101_AX_no_160_1x1_WinT_non_6e , PCI\VEN_8086&DEV_51F0&SUBSYS_02448086 ; AX_no_160
%NIC_203_2x2_AX_no_160% = Install_GEN_SLR_JnP_203_AX_no_160_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F0&SUBSYS_02748086 ; AX_no_160
%NIC_1650s_2x2_AX%      = Install_RIV_SLR_HrP2_1650s_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F0&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%      = Install_RIV_SLR_HrP2_1650i_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F0&SUBSYS_16521A56 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F0&SUBSYS_20748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F0&SUBSYS_40708086 ; AX
%NIC_101_1x1_AX_no_160% = Install_GEN_SLR_HrP1_101_AX_no_160_1x1_WinT_non_6e , PCI\VEN_8086&DEV_51F0&SUBSYS_42448086 ; AX_no_160
%NIC_203_2x2_AX_no_160% = Install_GEN_SLR_JnP_203_AX_no_160_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F0&SUBSYS_42748086 ; AX_no_160
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F0&SUBSYS_60748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F1&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F1&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F1&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F1&SUBSYS_007C8086 ; AX
%NIC_101_1x1_AX_no_160% = Install_GEN_SLR_HrP1_101_AX_no_160_1x1_WinT_non_6e , PCI\VEN_8086&DEV_51F1&SUBSYS_02448086 ; AX_no_160
%NIC_203_2x2_AX_no_160% = Install_GEN_SLR_JnP_203_AX_no_160_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F1&SUBSYS_02748086 ; AX_no_160
%NIC_1650s_2x2_AX%      = Install_RIV_SLR_HrP2_1650s_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F1&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%      = Install_RIV_SLR_HrP2_1650i_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F1&SUBSYS_16521A56 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F1&SUBSYS_20748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F1&SUBSYS_40708086 ; AX
%NIC_101_1x1_AX_no_160% = Install_GEN_SLR_HrP1_101_AX_no_160_1x1_WinT_non_6e , PCI\VEN_8086&DEV_51F1&SUBSYS_42448086 ; AX_no_160
%NIC_203_2x2_AX_no_160% = Install_GEN_SLR_JnP_203_AX_no_160_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F1&SUBSYS_42748086 ; AX_no_160
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_51F1&SUBSYS_60748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_54F0&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_54F0&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_54F0&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_54F0&SUBSYS_007C8086 ; AX
%NIC_101_1x1_AX_no_160% = Install_GEN_SLR_HrP1_101_AX_no_160_1x1_WinT_non_6e , PCI\VEN_8086&DEV_54F0&SUBSYS_02448086 ; AX_no_160
%NIC_203_2x2_AX_no_160% = Install_GEN_SLR_JnP_203_AX_no_160_2x2_WinT_non_6e , PCI\VEN_8086&DEV_54F0&SUBSYS_02748086 ; AX_no_160
%NIC_1650s_2x2_AX%      = Install_RIV_SLR_HrP2_1650s_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_54F0&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%      = Install_RIV_SLR_HrP2_1650i_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_54F0&SUBSYS_16521A56 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_54F0&SUBSYS_20748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_54F0&SUBSYS_40708086 ; AX
%NIC_101_1x1_AX_no_160% = Install_GEN_SLR_HrP1_101_AX_no_160_1x1_WinT_non_6e , PCI\VEN_8086&DEV_54F0&SUBSYS_42448086 ; AX_no_160
%NIC_203_2x2_AX_no_160% = Install_GEN_SLR_JnP_203_AX_no_160_2x2_WinT_non_6e , PCI\VEN_8086&DEV_54F0&SUBSYS_42748086 ; AX_no_160
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_54F0&SUBSYS_60748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7A70&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7A70&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7A70&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7A70&SUBSYS_007C8086 ; AX
%NIC_101_1x1_AX_no_160% = Install_GEN_SLR_HrP1_101_AX_no_160_1x1_WinT_non_6e , PCI\VEN_8086&DEV_7A70&SUBSYS_02448086 ; AX_no_160
%NIC_203_2x2_AX_no_160% = Install_GEN_SLR_JnP_203_AX_no_160_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7A70&SUBSYS_02748086 ; AX_no_160
%NIC_1650s_2x2_AX%      = Install_RIV_SLR_HrP2_1650s_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7A70&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%      = Install_RIV_SLR_HrP2_1650i_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7A70&SUBSYS_16521A56 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7A70&SUBSYS_20748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7A70&SUBSYS_40708086 ; AX
%NIC_101_1x1_AX_no_160% = Install_GEN_SLR_HrP1_101_AX_no_160_1x1_WinT_non_6e , PCI\VEN_8086&DEV_7A70&SUBSYS_42448086 ; AX_no_160
%NIC_203_2x2_AX_no_160% = Install_GEN_SLR_JnP_203_AX_no_160_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7A70&SUBSYS_42748086 ; AX_no_160
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7A70&SUBSYS_60748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7AF0&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7AF0&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7AF0&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7AF0&SUBSYS_007C8086 ; AX
%NIC_101_1x1_AX_no_160% = Install_GEN_SLR_HrP1_101_AX_no_160_1x1_WinT_non_6e , PCI\VEN_8086&DEV_7AF0&SUBSYS_02448086 ; AX_no_160
%NIC_203_2x2_AX_no_160% = Install_GEN_SLR_JnP_203_AX_no_160_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7AF0&SUBSYS_02748086 ; AX_no_160
%NIC_1650s_2x2_AX%      = Install_RIV_SLR_HrP2_1650s_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7AF0&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%      = Install_RIV_SLR_HrP2_1650i_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7AF0&SUBSYS_16521A56 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7AF0&SUBSYS_20748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7AF0&SUBSYS_40708086 ; AX
%NIC_101_1x1_AX_no_160% = Install_GEN_SLR_HrP1_101_AX_no_160_1x1_WinT_non_6e , PCI\VEN_8086&DEV_7AF0&SUBSYS_42448086 ; AX_no_160
%NIC_203_2x2_AX_no_160% = Install_GEN_SLR_JnP_203_AX_no_160_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7AF0&SUBSYS_42748086 ; AX_no_160
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7AF0&SUBSYS_60748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_MAG_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7E40&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_MAG_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7E40&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_MAG_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7E40&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_MAG_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7E40&SUBSYS_007C8086 ; AX
%NIC_101_1x1_AX_no_160% = Install_GEN_MAG_HrP1_101_AX_no_160_1x1_WinT_non_6e , PCI\VEN_8086&DEV_7E40&SUBSYS_02448086 ; AX_no_160
%NIC_203_2x2_AX_no_160% = Install_GEN_MAG_JnP_203_AX_no_160_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7E40&SUBSYS_02748086 ; AX_no_160
%NIC_1650s_2x2_AX%      = Install_RIV_MAG_HrP2_1650s_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7E40&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%      = Install_RIV_MAG_HrP2_1650i_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7E40&SUBSYS_16521A56 ; AX
%NIC_201_2x2_AX%        = Install_GEN_MAG_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7E40&SUBSYS_20748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_MAG_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7E40&SUBSYS_40708086 ; AX
%NIC_101_1x1_AX_no_160% = Install_GEN_MAG_HrP1_101_AX_no_160_1x1_WinT_non_6e , PCI\VEN_8086&DEV_7E40&SUBSYS_42448086 ; AX_no_160
%NIC_203_2x2_AX_no_160% = Install_GEN_MAG_JnP_203_AX_no_160_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7E40&SUBSYS_42748086 ; AX_no_160
%NIC_201_2x2_AX%        = Install_GEN_MAG_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7E40&SUBSYS_60748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7F70&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7F70&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7F70&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7F70&SUBSYS_007C8086 ; AX
%NIC_101_1x1_AX_no_160% = Install_GEN_SLR_HrP1_101_AX_no_160_1x1_WinT_non_6e , PCI\VEN_8086&DEV_7F70&SUBSYS_02448086 ; AX_no_160
%NIC_203_2x2_AX_no_160% = Install_GEN_SLR_JnP_203_AX_no_160_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7F70&SUBSYS_02748086 ; AX_no_160
%NIC_1650s_2x2_AX%      = Install_RIV_SLR_HrP2_1650s_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7F70&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%      = Install_RIV_SLR_HrP2_1650i_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7F70&SUBSYS_16521A56 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7F70&SUBSYS_20748086 ; AX
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7F70&SUBSYS_40708086 ; AX
%NIC_101_1x1_AX_no_160% = Install_GEN_SLR_HrP1_101_AX_no_160_1x1_WinT_non_6e , PCI\VEN_8086&DEV_7F70&SUBSYS_42448086 ; AX_no_160
%NIC_203_2x2_AX_no_160% = Install_GEN_SLR_JnP_203_AX_no_160_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7F70&SUBSYS_42748086 ; AX_no_160
%NIC_201_2x2_AX%        = Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e , PCI\VEN_8086&DEV_7F70&SUBSYS_60748086 ; AX

%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_00648086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_007C8086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_023C8086 ; AC_no_160
%NIC_101_1x1_AX_no_160%  = Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_02448086 ; AX_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_02648086 ; AC_no_160
%NIC_203_2x2_AX_no_160%  = Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_02748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_QSR_JfP2_1550s_AC_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_QSR_JfP2_1550i_AC_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_15521A56 ; AC
%NIC_1650s_2x2_AX%       = Install_RIV_QSR_HrP2_1650s_AX_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%       = Install_RIV_QSR_HrP2_1650i_AX_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_16521A56 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_20348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_20748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_40348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_40708086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_42348086 ; AC_no_160
%NIC_101_1x1_AX_no_160%  = Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_42448086 ; AX_no_160
%NIC_203_2x2_AX_no_160%  = Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_42748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_42A48086 ; AC_no_160
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_02F0&SUBSYS_60748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_00648086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_007C8086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_023C8086 ; AC_no_160
%NIC_101_1x1_AX_no_160%  = Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_02448086 ; AX_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_02648086 ; AC_no_160
%NIC_203_2x2_AX_no_160%  = Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_02748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_QSR_JfP2_1550s_AC_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_QSR_JfP2_1550i_AC_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_15521A56 ; AC
%NIC_1650s_2x2_AX%       = Install_RIV_QSR_HrP2_1650s_AX_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%       = Install_RIV_QSR_HrP2_1650i_AX_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_16521A56 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_20348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_20748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_40348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_40708086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_42348086 ; AC_no_160
%NIC_101_1x1_AX_no_160%  = Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_42448086 ; AX_no_160
%NIC_203_2x2_AX_no_160%  = Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_42748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_42A48086 ; AC_no_160
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_06F0&SUBSYS_60748086 ; AX
%NIC_200_2x2_AX%         = Install_GEN_QSR_CcP_200_AX_2x2_WinT , PCI\VEN_8086&DEV_2723&SUBSYS_00808086 ; AX
%NIC_200_2x2_AX%         = Install_GEN_QSR_CcP_200_AX_2x2_WinT , PCI\VEN_8086&DEV_2723&SUBSYS_00848086 ; AX
%NIC_200_2x2_AX%         = Install_GEN_QSR_CcP_200_AX_2x2_WinT , PCI\VEN_8086&DEV_2723&SUBSYS_00888086 ; AX
%NIC_200_2x2_AX%         = Install_GEN_QSR_CcP_200_AX_2x2_WinT , PCI\VEN_8086&DEV_2723&SUBSYS_008C8086 ; AX
%NIC_1650w_2x2_AX%       = Install_RIV_QSR_CcP_1650w_AX_2x2_WinT , PCI\VEN_8086&DEV_2723&SUBSYS_16531A56 ; AX
%NIC_1650x_2x2_AX%       = Install_RIV_QSR_CcP_1650x_AX_2x2_WinT , PCI\VEN_8086&DEV_2723&SUBSYS_16541A56 ; AX
%NIC_200_2x2_AX%         = Install_GEN_QSR_CcP_200_AX_2x2_WinT , PCI\VEN_8086&DEV_2723&SUBSYS_20808086 ; AX
%NIC_200_2x2_AX%         = Install_GEN_QSR_CcP_200_AX_2x2_WinT , PCI\VEN_8086&DEV_2723&SUBSYS_40808086 ; AX
%NIC_200_2x2_AX%         = Install_GEN_QSR_CcP_200_AX_2x2_WinT , PCI\VEN_8086&DEV_2723&SUBSYS_40888086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_00648086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_007C8086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_023C8086 ; AC_no_160
%NIC_101_1x1_AX_no_160%  = Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_02448086 ; AX_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_02648086 ; AC_no_160
%NIC_203_2x2_AX_no_160%  = Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_02748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_QSR_JfP2_1550s_AC_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_QSR_JfP2_1550i_AC_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_15521A56 ; AC
%NIC_1650s_2x2_AX%       = Install_RIV_QSR_HrP2_1650s_AX_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%       = Install_RIV_QSR_HrP2_1650i_AX_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_16521A56 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_20348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_20748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_40348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_40708086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_42348086 ; AC_no_160
%NIC_101_1x1_AX_no_160%  = Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_42448086 ; AX_no_160
%NIC_203_2x2_AX_no_160%  = Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_42748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_42A48086 ; AC_no_160
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_34F0&SUBSYS_60748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_00648086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_007C8086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_023C8086 ; AC_no_160
%NIC_101_1x1_AX_no_160%  = Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_02448086 ; AX_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_02648086 ; AC_no_160
%NIC_203_2x2_AX_no_160%  = Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_02748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_QSR_JfP2_1550s_AC_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_QSR_JfP2_1550i_AC_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_15521A56 ; AC
%NIC_1650s_2x2_AX%       = Install_RIV_QSR_HrP2_1650s_AX_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%       = Install_RIV_QSR_HrP2_1650i_AX_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_16521A56 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_20348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_20748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_40348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_40708086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_42348086 ; AC_no_160
%NIC_101_1x1_AX_no_160%  = Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_42448086 ; AX_no_160
%NIC_203_2x2_AX_no_160%  = Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_42748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_42A48086 ; AC_no_160
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_3DF0&SUBSYS_60748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_00648086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_007C8086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_023C8086 ; AC_no_160
%NIC_101_1x1_AX_no_160%  = Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_02448086 ; AX_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_02648086 ; AC_no_160
%NIC_203_2x2_AX_no_160%  = Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_02748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_QSR_JfP2_1550s_AC_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_QSR_JfP2_1550i_AC_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_15521A56 ; AC
%NIC_1650s_2x2_AX%       = Install_RIV_QSR_HrP2_1650s_AX_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%       = Install_RIV_QSR_HrP2_1650i_AX_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_16521A56 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_20348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_20748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_40348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_40708086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_42348086 ; AC_no_160
%NIC_101_1x1_AX_no_160%  = Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_42448086 ; AX_no_160
%NIC_203_2x2_AX_no_160%  = Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_42748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_42A48086 ; AC_no_160
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_43F0&SUBSYS_60748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_00648086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_007C8086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_023C8086 ; AC_no_160
%NIC_101_1x1_AX_no_160%  = Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_02448086 ; AX_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_02648086 ; AC_no_160
%NIC_203_2x2_AX_no_160%  = Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_02748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_QSR_JfP2_1550s_AC_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_QSR_JfP2_1550i_AC_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_15521A56 ; AC
%NIC_1650s_2x2_AX%       = Install_RIV_QSR_HrP2_1650s_AX_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%       = Install_RIV_QSR_HrP2_1650i_AX_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_16521A56 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_20348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_20748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_40348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_40708086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_42348086 ; AC_no_160
%NIC_101_1x1_AX_no_160%  = Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_42448086 ; AX_no_160
%NIC_203_2x2_AX_no_160%  = Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_42748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_42A48086 ; AC_no_160
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_4DF0&SUBSYS_60748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_SLR_JfP1_9461_AC_1x1_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_00648086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_02648086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_SLR_JfP2_1550s_AC_2x2_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_SLR_JfP2_1550i_AC_2x2_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_15521A56 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_20348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_40348086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_51F0&SUBSYS_42A48086 ; AC_no_160
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_SLR_JfP1_9461_AC_1x1_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_00648086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_02648086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_SLR_JfP2_1550s_AC_2x2_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_SLR_JfP2_1550i_AC_2x2_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_15521A56 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_20348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_40348086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_51F1&SUBSYS_42A48086 ; AC_no_160
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_SLR_JfP1_9461_AC_1x1_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_00648086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_02648086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_SLR_JfP2_1550s_AC_2x2_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_SLR_JfP2_1550i_AC_2x2_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_15521A56 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_20348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_40348086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_54F0&SUBSYS_42A48086 ; AC_no_160
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_SLR_JfP1_9461_AC_1x1_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_00648086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_02648086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_SLR_JfP2_1550s_AC_2x2_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_SLR_JfP2_1550i_AC_2x2_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_15521A56 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_20348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_40348086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_7A70&SUBSYS_42A48086 ; AC_no_160
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_SLR_JfP1_9461_AC_1x1_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_00648086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_02648086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_SLR_JfP2_1550s_AC_2x2_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_SLR_JfP2_1550i_AC_2x2_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_15521A56 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_20348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_40348086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_7AF0&SUBSYS_42A48086 ; AC_no_160
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_SLR_JfP1_9461_AC_1x1_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_00648086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_02648086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_SLR_JfP2_1550s_AC_2x2_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_SLR_JfP2_1550i_AC_2x2_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_15521A56 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_20348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_SLR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_40348086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_SLR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_7F70&SUBSYS_42A48086 ; AC_no_160
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_QSR_JfP1_9461_AC_1x1_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_00648086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_00708086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_00748086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_00788086 ; AX
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_007C8086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_023C8086 ; AC_no_160
%NIC_101_1x1_AX_no_160%  = Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_02448086 ; AX_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_02648086 ; AC_no_160
%NIC_203_2x2_AX_no_160%  = Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_02748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_QSR_JfP2_1550s_AC_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_QSR_JfP2_1550i_AC_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_15521A56 ; AC
%NIC_1650s_2x2_AX%       = Install_RIV_QSR_HrP2_1650s_AX_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_16511A56 ; AX
%NIC_1650i_2x2_AX%       = Install_RIV_QSR_HrP2_1650i_AX_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_16521A56 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_20348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_20748086 ; AX
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_QSR_JfP2_9560_AC_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_40348086 ; AC
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_40708086 ; AX
%NIC_9462_1x1_AC%        = Install_GEN_QSR_JfP1_9462_AC_1x1_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_42348086 ; AC_no_160
%NIC_101_1x1_AX_no_160%  = Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_42448086 ; AX_no_160
%NIC_203_2x2_AX_no_160%  = Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_42748086 ; AX_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_42A48086 ; AC_no_160
%NIC_201_2x2_AX%         = Install_GEN_QSR_HrP2_201_AX_2x2_WinT , PCI\VEN_8086&DEV_A0F0&SUBSYS_60748086 ; AX
%NIC_9260_2x2_AC%        = Install_BU_PSR_ThP_9260_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_00008086 ; AC
%NIC_9260_2x2_AC%        = Install_GEN_PSR_ThP_9260_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_00108086 ; AC
%NIC_9260_2x2_AC%        = Install_GEN_PSR_ThP_9260_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_00148086 ; AC
%NIC_9260_2x2_AC%        = Install_GEN_PSR_ThP_9260_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_00188086 ; AC
%NIC_9260_2x2_AC%        = Install_GEN_PSR_ThP_9260_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_001C8086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_PSR_JfP1_9461_AC_1x1 , PCI\VEN_8086&DEV_2526&SUBSYS_00608086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_PSR_JfP1_9461_AC_1x1 , PCI\VEN_8086&DEV_2526&SUBSYS_00648086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_PSR_JfP1_9462_AC_1x1 , PCI\VEN_8086&DEV_2526&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_PSR_JfP1_9462_AC_1x1 , PCI\VEN_8086&DEV_2526&SUBSYS_00A48086 ; AC
%NIC_9260_2x2_AC_no_160% = Install_GEN_PSR_ThP_9260_AC_no_160_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_02108086 ; AC_no_160
%NIC_9260_2x2_AC_no_160% = Install_GEN_PSR_ThP_9260_AC_no_160_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_02148086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9461_AC_no_160_1x1 , PCI\VEN_8086&DEV_2526&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9461_AC_no_160_1x1 , PCI\VEN_8086&DEV_2526&SUBSYS_02648086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9462_AC_no_160_1x1 , PCI\VEN_8086&DEV_2526&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9462_AC_no_160_1x1 , PCI\VEN_8086&DEV_2526&SUBSYS_02A48086 ; AC_no_160
%NIC_1550_2x2_AC%        = Install_RIV_PSR_ThP_1550_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_15501A56 ; AC
%NIC_1550s_2x2_AC%       = Install_RIV_PSR_JfP_1550s_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_PSR_JfP_1550i_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_15521A56 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_20348086 ; AC
%NIC_9260_2x2_AC%        = Install_GEN_PSR_ThP_9260_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_40108086 ; AC
%NIC_9260_2x2_AC%        = Install_GEN_PSR_ThP_9260_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_40188086 ; AC
%NIC_9260_2x2_AC%        = Install_GEN_PSR_ThP_9260_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_401C8086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_40348086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_PSR_JfP1_9462_AC_1x1 , PCI\VEN_8086&DEV_2526&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9462_AC_no_160_1x1 , PCI\VEN_8086&DEV_2526&SUBSYS_42A48086 ; AC_no_160
%NIC_9260_2x2_AC%        = Install_GEN_PSR_ThP_9260_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_60108086 ; AC
%NIC_9260_2x2_AC%        = Install_GEN_PSR_ThP_9260_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_60148086 ; AC
%NIC_9260_2x2_AC%        = Install_GEN_PSR_ThP_9260_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_80108086 ; AC
%NIC_9260_2x2_AC%        = Install_GEN_PSR_ThP_9260_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_80148086 ; AC
%NIC_9260_2x2_AC%        = Install_GEN_PSR_ThP_9260_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_A0148086 ; AC
%NIC_9260_2x2_AC%        = Install_GEN_PSR_ThP_9260_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_E0108086 ; AC
%NIC_9260_2x2_AC%        = Install_GEN_PSR_ThP_9260_AC_2x2 , PCI\VEN_8086&DEV_2526&SUBSYS_E0148086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_30DC&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_30DC&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_30DC&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_30DC&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_PSR_JfP1_9461_AC_1x1 , PCI\VEN_8086&DEV_30DC&SUBSYS_00608086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_PSR_JfP1_9461_AC_1x1 , PCI\VEN_8086&DEV_30DC&SUBSYS_00648086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_PSR_JfP1_9462_AC_1x1 , PCI\VEN_8086&DEV_30DC&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_PSR_JfP1_9462_AC_1x1 , PCI\VEN_8086&DEV_30DC&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_30DC&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_30DC&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_30DC&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_30DC&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9461_AC_no_160_1x1 , PCI\VEN_8086&DEV_30DC&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9461_AC_no_160_1x1 , PCI\VEN_8086&DEV_30DC&SUBSYS_02648086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9462_AC_no_160_1x1 , PCI\VEN_8086&DEV_30DC&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9462_AC_no_160_1x1 , PCI\VEN_8086&DEV_30DC&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_PSR_JfP_1550s_AC_2x2 , PCI\VEN_8086&DEV_30DC&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_PSR_JfP_1550i_AC_2x2 , PCI\VEN_8086&DEV_30DC&SUBSYS_15521A56 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_30DC&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_30DC&SUBSYS_20348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_30DC&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_30DC&SUBSYS_40348086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_PSR_JfP1_9462_AC_1x1 , PCI\VEN_8086&DEV_30DC&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_30DC&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9462_AC_no_160_1x1 , PCI\VEN_8086&DEV_30DC&SUBSYS_42A48086 ; AC_no_160
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_31DC&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_31DC&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_31DC&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_31DC&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_PSR_JfP1_9461_AC_1x1 , PCI\VEN_8086&DEV_31DC&SUBSYS_00608086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_PSR_JfP1_9461_AC_1x1 , PCI\VEN_8086&DEV_31DC&SUBSYS_00648086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_PSR_JfP1_9462_AC_1x1 , PCI\VEN_8086&DEV_31DC&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_PSR_JfP1_9462_AC_1x1 , PCI\VEN_8086&DEV_31DC&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_31DC&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_31DC&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_31DC&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_31DC&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9461_AC_no_160_1x1 , PCI\VEN_8086&DEV_31DC&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9461_AC_no_160_1x1 , PCI\VEN_8086&DEV_31DC&SUBSYS_02648086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9462_AC_no_160_1x1 , PCI\VEN_8086&DEV_31DC&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9462_AC_no_160_1x1 , PCI\VEN_8086&DEV_31DC&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_PSR_JfP_1550s_AC_2x2 , PCI\VEN_8086&DEV_31DC&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_PSR_JfP_1550i_AC_2x2 , PCI\VEN_8086&DEV_31DC&SUBSYS_15521A56 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_31DC&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_31DC&SUBSYS_20348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_31DC&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_31DC&SUBSYS_40348086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_PSR_JfP1_9462_AC_1x1 , PCI\VEN_8086&DEV_31DC&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_31DC&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9462_AC_no_160_1x1 , PCI\VEN_8086&DEV_31DC&SUBSYS_42A48086 ; AC_no_160
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_9DF0&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_9DF0&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_9DF0&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_9DF0&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_PSR_JfP1_9461_AC_1x1 , PCI\VEN_8086&DEV_9DF0&SUBSYS_00608086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_PSR_JfP1_9461_AC_1x1 , PCI\VEN_8086&DEV_9DF0&SUBSYS_00648086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_PSR_JfP1_9462_AC_1x1 , PCI\VEN_8086&DEV_9DF0&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_PSR_JfP1_9462_AC_1x1 , PCI\VEN_8086&DEV_9DF0&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_9DF0&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_9DF0&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_9DF0&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_9DF0&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9461_AC_no_160_1x1 , PCI\VEN_8086&DEV_9DF0&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9461_AC_no_160_1x1 , PCI\VEN_8086&DEV_9DF0&SUBSYS_02648086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9462_AC_no_160_1x1 , PCI\VEN_8086&DEV_9DF0&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9462_AC_no_160_1x1 , PCI\VEN_8086&DEV_9DF0&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_PSR_JfP_1550s_AC_2x2 , PCI\VEN_8086&DEV_9DF0&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_PSR_JfP_1550i_AC_2x2 , PCI\VEN_8086&DEV_9DF0&SUBSYS_15521A56 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_9DF0&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_9DF0&SUBSYS_20348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_9DF0&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_9DF0&SUBSYS_40348086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_PSR_JfP1_9462_AC_1x1 , PCI\VEN_8086&DEV_9DF0&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_9DF0&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9462_AC_no_160_1x1 , PCI\VEN_8086&DEV_9DF0&SUBSYS_42A48086 ; AC_no_160
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_A370&SUBSYS_00308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_A370&SUBSYS_00348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_A370&SUBSYS_00388086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_A370&SUBSYS_003C8086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_PSR_JfP1_9461_AC_1x1 , PCI\VEN_8086&DEV_A370&SUBSYS_00608086 ; AC
%NIC_9461_1x1_AC%        = Install_GEN_PSR_JfP1_9461_AC_1x1 , PCI\VEN_8086&DEV_A370&SUBSYS_00648086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_PSR_JfP1_9462_AC_1x1 , PCI\VEN_8086&DEV_A370&SUBSYS_00A08086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_PSR_JfP1_9462_AC_1x1 , PCI\VEN_8086&DEV_A370&SUBSYS_00A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_A370&SUBSYS_02308086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_A370&SUBSYS_02348086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_A370&SUBSYS_02388086 ; AC_no_160
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_A370&SUBSYS_023C8086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9461_AC_no_160_1x1 , PCI\VEN_8086&DEV_A370&SUBSYS_02608086 ; AC_no_160
%NIC_9461_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9461_AC_no_160_1x1 , PCI\VEN_8086&DEV_A370&SUBSYS_02648086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9462_AC_no_160_1x1 , PCI\VEN_8086&DEV_A370&SUBSYS_02A08086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9462_AC_no_160_1x1 , PCI\VEN_8086&DEV_A370&SUBSYS_02A48086 ; AC_no_160
%NIC_1550s_2x2_AC%       = Install_RIV_PSR_JfP_1550s_AC_2x2 , PCI\VEN_8086&DEV_A370&SUBSYS_15511A56 ; AC
%NIC_1550i_2x2_AC%       = Install_RIV_PSR_JfP_1550i_AC_2x2 , PCI\VEN_8086&DEV_A370&SUBSYS_15521A56 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_A370&SUBSYS_20308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_A370&SUBSYS_20348086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_A370&SUBSYS_40308086 ; AC
%NIC_9560_2x2_AC%        = Install_GEN_PSR_JfP_9560_AC_2x2 , PCI\VEN_8086&DEV_A370&SUBSYS_40348086 ; AC
%NIC_9462_1x1_AC%        = Install_GEN_PSR_JfP1_9462_AC_1x1 , PCI\VEN_8086&DEV_A370&SUBSYS_40A48086 ; AC
%NIC_9560_2x2_AC_no_160% = Install_GEN_PSR_JfP_9560_AC_no_160_2x2 , PCI\VEN_8086&DEV_A370&SUBSYS_42348086 ; AC_no_160
%NIC_9462_1x1_AC_no_160% = Install_GEN_PSR_JfP1_9462_AC_no_160_1x1 , PCI\VEN_8086&DEV_A370&SUBSYS_42A48086 ; AC_no_160
[Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_14
AddReg               = Reg_Common_14,Reg_Common_WPP_14,Reg_NDI_14,Reg_NDI_INT_WDI_14,Reg_IHV_Router_14,Reg_2x2_14,Reg_NDI_2x2_14,Reg_NDI_AX_14,Reg_AX_14,Reg_NDI_HRP2_14,Reg_NIC_201_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_14_WinT_non_6e,CopyFiles_IHV_Router_14_WinT_non_6e
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11


[Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_solar.reg_14


[Install_GEN_SLR_HrP2_201_AX_2x2_WinT_non_6e.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw14, 2,NIC_Service_14_WinT_non_6e,Common_EventLog_14_WinT_non_6e


[Install_GEN_SLR_HrP1_101_AX_no_160_1x1_WinT_non_6e]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_14
AddReg               = Reg_Common_14,Reg_Common_WPP_14,Reg_NDI_14,Reg_NDI_INT_WDI_14,Reg_IHV_Router_14,Reg_1x1_14,Reg_1x1_AX_14,Reg_NDI_AX_14,Reg_AX_14,Reg_NDI_HRP1_14,Reg_NIC_101_1x1_AX_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_14_WinT_non_6e,CopyFiles_IHV_Router_14_WinT_non_6e
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11


[Install_GEN_SLR_HrP1_101_AX_no_160_1x1_WinT_non_6e.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_solar.reg_14


[Install_GEN_SLR_HrP1_101_AX_no_160_1x1_WinT_non_6e.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw14, 2,NIC_Service_14_WinT_non_6e,Common_EventLog_14_WinT_non_6e


[Install_GEN_SLR_JnP_203_AX_no_160_2x2_WinT_non_6e]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_14
AddReg               = Reg_Common_14,Reg_Common_WPP_14,Reg_NDI_14,Reg_NDI_INT_WDI_14,Reg_IHV_Router_14,Reg_2x2_14,Reg_NDI_2x2_14,Reg_NDI_AX_14,Reg_AX_14,Reg_NIC_203_2x2_AX_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_14_WinT_non_6e,CopyFiles_IHV_Router_14_WinT_non_6e
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11


[Install_GEN_SLR_JnP_203_AX_no_160_2x2_WinT_non_6e.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_solar.reg_14


[Install_GEN_SLR_JnP_203_AX_no_160_2x2_WinT_non_6e.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw14, 2,NIC_Service_14_WinT_non_6e,Common_EventLog_14_WinT_non_6e


[Install_RIV_SLR_HrP2_1650s_AX_2x2_WinT_non_6e]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_14
AddReg               = Reg_Common_14,Reg_Common_WPP_14,Reg_NDI_14,Reg_NDI_INT_WDI_14,Reg_IHV_Router_14,Reg_2x2_14,Reg_NDI_2x2_14,Reg_NDI_AX_14,Reg_AX_14,RegSec_Riv_14,Reg_NDI_HRP2_14,Reg_NIC_1650s_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_14_WinT_non_6e,CopyFiles_IHV_Router_14_WinT_non_6e
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11


[Install_RIV_SLR_HrP2_1650s_AX_2x2_WinT_non_6e.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_solar.reg_14


[Install_RIV_SLR_HrP2_1650s_AX_2x2_WinT_non_6e.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw14, 2,NIC_Service_14_WinT_non_6e,Common_EventLog_14_WinT_non_6e


[Install_RIV_SLR_HrP2_1650i_AX_2x2_WinT_non_6e]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_14
AddReg               = Reg_Common_14,Reg_Common_WPP_14,Reg_NDI_14,Reg_NDI_INT_WDI_14,Reg_IHV_Router_14,Reg_2x2_14,Reg_NDI_2x2_14,Reg_NDI_AX_14,Reg_AX_14,RegSec_Riv_14,Reg_NDI_HRP2_14,Reg_NIC_1650i_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_14_WinT_non_6e,CopyFiles_IHV_Router_14_WinT_non_6e
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11


[Install_RIV_SLR_HrP2_1650i_AX_2x2_WinT_non_6e.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_solar.reg_14


[Install_RIV_SLR_HrP2_1650i_AX_2x2_WinT_non_6e.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw14, 2,NIC_Service_14_WinT_non_6e,Common_EventLog_14_WinT_non_6e


[Install_GEN_MAG_HrP2_201_AX_2x2_WinT_non_6e]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_14
AddReg               = Reg_Common_14,Reg_Common_WPP_14,Reg_NDI_14,Reg_NDI_INT_WDI_14,Reg_IHV_Router_14,Reg_2x2_14,Reg_NDI_2x2_14,Reg_NDI_AX_14,Reg_AX_14,Reg_NDI_HRP2_14,Reg_NIC_201_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_14_WinT_non_6e,CopyFiles_IHV_Router_14_WinT_non_6e
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11


[Install_GEN_MAG_HrP2_201_AX_2x2_WinT_non_6e.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_magnetar.reg_14


[Install_GEN_MAG_HrP2_201_AX_2x2_WinT_non_6e.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw14, 2,NIC_Service_14_WinT_non_6e,Common_EventLog_14_WinT_non_6e


[Install_GEN_MAG_HrP1_101_AX_no_160_1x1_WinT_non_6e]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_14
AddReg               = Reg_Common_14,Reg_Common_WPP_14,Reg_NDI_14,Reg_NDI_INT_WDI_14,Reg_IHV_Router_14,Reg_1x1_14,Reg_1x1_AX_14,Reg_NDI_AX_14,Reg_AX_14,Reg_NDI_HRP1_14,Reg_NIC_101_1x1_AX_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_14_WinT_non_6e,CopyFiles_IHV_Router_14_WinT_non_6e
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11


[Install_GEN_MAG_HrP1_101_AX_no_160_1x1_WinT_non_6e.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_magnetar.reg_14


[Install_GEN_MAG_HrP1_101_AX_no_160_1x1_WinT_non_6e.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw14, 2,NIC_Service_14_WinT_non_6e,Common_EventLog_14_WinT_non_6e


[Install_GEN_MAG_JnP_203_AX_no_160_2x2_WinT_non_6e]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_14
AddReg               = Reg_Common_14,Reg_Common_WPP_14,Reg_NDI_14,Reg_NDI_INT_WDI_14,Reg_IHV_Router_14,Reg_2x2_14,Reg_NDI_2x2_14,Reg_NDI_AX_14,Reg_AX_14,Reg_NIC_203_2x2_AX_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_14_WinT_non_6e,CopyFiles_IHV_Router_14_WinT_non_6e
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11


[Install_GEN_MAG_JnP_203_AX_no_160_2x2_WinT_non_6e.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_magnetar.reg_14


[Install_GEN_MAG_JnP_203_AX_no_160_2x2_WinT_non_6e.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw14, 2,NIC_Service_14_WinT_non_6e,Common_EventLog_14_WinT_non_6e


[Install_RIV_MAG_HrP2_1650s_AX_2x2_WinT_non_6e]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_14
AddReg               = Reg_Common_14,Reg_Common_WPP_14,Reg_NDI_14,Reg_NDI_INT_WDI_14,Reg_IHV_Router_14,Reg_2x2_14,Reg_NDI_2x2_14,Reg_NDI_AX_14,Reg_AX_14,RegSec_Riv_14,Reg_NDI_HRP2_14,Reg_NIC_1650s_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_14_WinT_non_6e,CopyFiles_IHV_Router_14_WinT_non_6e
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11


[Install_RIV_MAG_HrP2_1650s_AX_2x2_WinT_non_6e.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_magnetar.reg_14


[Install_RIV_MAG_HrP2_1650s_AX_2x2_WinT_non_6e.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw14, 2,NIC_Service_14_WinT_non_6e,Common_EventLog_14_WinT_non_6e


[Install_RIV_MAG_HrP2_1650i_AX_2x2_WinT_non_6e]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_14
AddReg               = Reg_Common_14,Reg_Common_WPP_14,Reg_NDI_14,Reg_NDI_INT_WDI_14,Reg_IHV_Router_14,Reg_2x2_14,Reg_NDI_2x2_14,Reg_NDI_AX_14,Reg_AX_14,RegSec_Riv_14,Reg_NDI_HRP2_14,Reg_NIC_1650i_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_14_WinT_non_6e,CopyFiles_IHV_Router_14_WinT_non_6e
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11


[Install_RIV_MAG_HrP2_1650i_AX_2x2_WinT_non_6e.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_magnetar.reg_14


[Install_RIV_MAG_HrP2_1650i_AX_2x2_WinT_non_6e.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw14, 2,NIC_Service_14_WinT_non_6e,Common_EventLog_14_WinT_non_6e


[NIC_Service_14_WinT_non_6e]
DisplayName          = "___" %NIC_Service_DispName_WINT_64%
ServiceType          = 1 ;%SERVICE_KERNEL_DRIVER%
StartType            = 3 ;%SERVICE_DEMAND_START%
ErrorControl         = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary        = %12%\Netwtw14.sys
LoadOrderGroup       = NDIS


[SourceDisksNames]
1                    = %SOURCEDISK1%,,

[SourceDisksFiles]
IntelIHVRouter14.dll = 1,,
Netwtw14.sys         = 1,,
netwfw14.dat         = 1,,

IntelIHVRouter10.dll = 1,,
Netwfw10.dat         = 1,,
Netwtw10.sys         = 1,,
Netwtw08.sys   = 1,,
Netwfw08.dat       = 1,,
IntelIHVRouter08.dll   = 1,,
[DestinationDirs]
DefaultDestDir                      = 11 ; Windows\System32
CopyFiles_Driver_14                 = 12 ; Windows\System32\Drivers
CopyFiles_xVT_14                    = 11 ; Windows\System32
CopyFiles_xVT_OC_14                 = 11 ; Windows\System32
CopyFiles_IHV_Router_14             = 11 ; Windows\System32
CopyFiles_Driver_14_WinT_non_6e     = 12 ; Windows\System32\Drivers
CopyFiles_IHV_Router_14_WinT_non_6e = 11 ; Windows\System32

CopyFiles_Driver_10          = 12 ; Windows\System32\Drivers
CopyFiles_xVT_10             = 11 ; Windows\System32
CopyFiles_xVT_OC_10          = 11 ; Windows\System32
CopyFiles_IHV_Router_10      = 11 ; Windows\System32
CopyFiles_Driver_10_WinT     = 12 ; Windows\System32\Drivers
CopyFiles_IHV_Router_10_WinT = 11 ; Windows\System32
CopyFiles_Driver     = 12 ; Windows\System32\Drivers
CopyFiles_xVT        = 11 ; Windows\System32
CopyFiles_xVT_OC     = 11 ; Windows\System32
CopyFiles_IHV_Router = 11 ; Windows\System32
[CopyFiles_Driver_14_WinT_non_6e]
Netwtw14.sys,,,2
netwfw14.dat,,,2


[CopyFiles_IHV_Router_14_WinT_non_6e]
IntelIHVRouter14.dll,,,2


[Common_EventLog_14_WinT_non_6e]
AddReg               = Reg_CommonAddEventLog_14_WinT_non_6e


[Reg_CommonAddEventLog_14_WinT_non_6e]
HKR,, EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\Drivers\Netwtw14.sys"
HKR,, TypesSupported,   0x00010001, 7


[DelReg_Common_14]
HKR, Ndi\


[Reg_Common_14]
HKR,,ExternalImage,0x10001,0x0
HKR,,FixedSupportedRates,0x10001,0xFFF
HKR,,ModulationType,2,"2"
HKR,,RadioEnable,0x10003,0x1
HKR,,RecommendedBeaconInterval,0x10001,0x64
HKR,,AtomMaxDpcTime,0x10001,0x14
HKR,,MaxDpcTime,0x10001,0x1E
HKR,,DuplicateRateSupported,0x10001,0x0
HKR,,ChannelWidth24,0,"1"
HKR,,ChannelWidth52,0,"1"
HKR,,CtsToItself,0,"0"
HKR,,*MiracastSupported,0x10001,0x1
HKR,,uAPSDSupport,0x10001,0
HKR,,SkipOverDtimEnable,0x10001,0x1
HKR,,LprxEnable,0x10001,0x1
HKR,,GreenFieldCapable,0x10001,0x0
HKR,,PanEnabled,0x10001,0x1
HKR,,BaEnable,0x10001,0x1
HKR,,TGeEnableBits,0x10001,0x00000037
HKR,,CtdpSupported,0x10001,1


[Reg_NDI_HRP2_14]
HKR,,CLSGUID,0,"{6506FE8C-5B1A-4A97-9AF4-4A9E325A69CC}"


[Reg_NDI_HRP1_14]
HKR,,CLSGUID,0,"{889E3741-FCC9-4FC0-973C-6FBDA8DF8573}"


[Reg_1x1_14]
HKR,,FixedSupportedHtRates,0x10001,0x000000FF
HKR,,SystemAllowedAntennas,0x10001,0x101
HKR,,VhtSupportedRxMcs,0x10001,0xFFFE
HKR,,VhtsupportedTxMcs,0x10001,0x2000FFFE
HKR,,GoVhtSupportedRxMcs,0x10001,0xFFFE
HKR,,GoVhtSupportedTxMcs,0x10001,0xFFFE
HKR,,rlcChainSettings,0x10001,0x2
HKR,,tlcValidAntenna,0x10001,0x1


[Reg_2x2_14]
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF
HKR,,SystemAllowedAntennas,0x10001,0x303


[Reg_1x1_AX_14]
HKR,,HeTxRxMcsNssSupportDword0,0x10001,0xFFFEFFFE
HKR,,HeTxRxMcsNssSupportDword1,0x10001,0xFFFEFFFE
HKR,,HeGoTxRxMcsNssSupportDword0,0x10001,0xFFFEFFFE
HKR,,HeGoTxRxMcsNssSupportDword1,0x10001,0xFFFEFFFE


[Reg_AX_14]
HKR,,SKU_CAP,0x10001,0x1f


[MSI_NDIS_solar.reg_14]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x10001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x10001, 3
HKR, "Interrupt Management\Affinity Policy", DevicePolicy, 0x00010001, 0
HKR, "Interrupt Management\Affinity Policy", AssignmentSetOverride, 0x00000003, 0


[MSI_NDIS_magnetar.reg_14]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x10001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x10001, 3
HKR, "Interrupt Management\Affinity Policy", DevicePolicy, 0x00010001, 0
HKR, "Interrupt Management\Affinity Policy", AssignmentSetOverride, 0x00000003, 0


[RegSec_Riv_14]
HKR,,QosClassMap,0x00000000,"00000000211111112222222233333333544444445555556566666666777777773012"


[Reg_IHV_Router_14]
HKR,Ndi\IHVExtensions, ExtensibilityDLL, 0, "%%SystemRoot%%\system32\IntelIHVRouter14.dll"


[Reg_NDI_AX_14]
HKR, Ndi\Params\IEEE11nMode,                   ParamDesc,   0, %11N_AX_MODE%
HKR, Ndi\Params\IEEE11nMode,                   Type,        0, "enum"
HKR, Ndi\Params\IEEE11nMode,                   Default,     0, "3"
HKR, Ndi\Params\IEEE11nMode,                   Optional,    0, "0"
HKR, Ndi\Params\IEEE11nMode\enum,              "0",         0, "1. "%DISABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "1",         0, "2. "%HT_ENABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "2",         0, "3. "%VHT_ENABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "3",         0, "4. "%11AX_ENABLED_STR%


[Reg_NDI_14]
HKR, Ndi\Params\ThroughputBoosterEnabled,      ParamDesc,   0, %THROUGHPUTBOOSTER_STR%
HKR, Ndi\Params\ThroughputBoosterEnabled,      Type,        2, "enum"
HKR, Ndi\Params\ThroughputBoosterEnabled,      Default,     2, "0"
HKR, Ndi\Params\ThroughputBoosterEnabled,      Optional,    2, "0"
HKR, Ndi\Params\ThroughputBoosterEnabled\enum, "0",         0, %DISABLED_STR%
HKR, Ndi\Params\ThroughputBoosterEnabled\enum, "1",         0, %ENABLED_STR%
HKR, Ndi\Params\WirelessMode,                  ParamDesc,   0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode,                  Type,        0, "enum",
HKR, Ndi\Params\WirelessMode,                  Default,     0, "34" ;abg
HKR, Ndi\Params\WirelessMode,                  Optional,    0, "0"
HKR, Ndi\Params\WirelessMode\enum,             "17",        0, "1. "%WIRELESS_MODE_A%
HKR, Ndi\Params\WirelessMode\enum,             "0",         0, "2. "%WIRELESS_MODE_B%
HKR, Ndi\Params\WirelessMode\enum,             "16",        0, "3. "%WIRELESS_MODE_G%
HKR, Ndi\Params\WirelessMode\enum,             "32",        0, "4. "%WIRELESS_MODE_BG%
HKR, Ndi\Params\WirelessMode\enum,             "18",        0, "5. "%WIRELESS_MODE_AG%
HKR, Ndi\Params\WirelessMode\enum,             "34",        0, "6. "%WIRELESS_MODE_ABG%
HKR, Ndi\Params\RoamingPreferredBandType,      ParamDesc,   0, %PREFERRED_BAND_STR%
HKR, Ndi\Params\RoamingPreferredBandType,      Type,        2, "enum"
HKR, Ndi\Params\RoamingPreferredBandType,      Default,     2, "0"
HKR, Ndi\Params\RoamingPreferredBandType,      Optional,    2, "0"
HKR, Ndi\Params\RoamingPreferredBandType\enum, "0",         0, "1. "%NO_PREFERECE_STR%
HKR, Ndi\Params\RoamingPreferredBandType\enum, "1",         0, "2. "%PREFER_24_BAND_STR%
HKR, Ndi\Params\RoamingPreferredBandType\enum, "2",         0, "3. "%PREFER_52_BAND_STR%
HKR, Ndi\Params\ChannelWidth24,                ParamDesc,   0,     %CHANNELWIDTH24%
HKR, Ndi\Params\ChannelWidth24,                Type,        0,     "enum"
HKR, Ndi\Params\ChannelWidth24,                Default,     0,     "1"
HKR, Ndi\Params\ChannelWidth24,                Optional,    0,     "0"
HKR, Ndi\Params\ChannelWidth24\enum,           "0",         0,     %CHANNELWIDTH20ONLY%
HKR, Ndi\Params\ChannelWidth24\enum,           "1",         0,     %CHANNELWIDTHAUTO%
HKR, Ndi\Params\ChannelWidth52,                ParamDesc,   0,  %CHANNELWIDTH52%
HKR, Ndi\Params\ChannelWidth52,                Type,        0,  "enum"
HKR, Ndi\Params\ChannelWidth52,                Default,     0,  "1"
HKR, Ndi\Params\ChannelWidth52,                Optional,    0,  "0"
HKR, Ndi\Params\ChannelWidth52\enum,           "0",         0,  %CHANNELWIDTH20ONLY%
HKR, Ndi\Params\ChannelWidth52\enum,           "1",         0,  %CHANNELWIDTHAUTO%
HKR, Ndi\Params\IbssTxPower,                   ParamDesc,   0, %IBSS_TX_POWER_STR%
HKR, Ndi\Params\IbssTxPower,                   Type,        2, "enum"
HKR, Ndi\Params\IbssTxPower,                   Default,     2, "100"
HKR, Ndi\Params\IbssTxPower,                   Optional,    2, "0"
HKR, Ndi\Params\IbssTxPower\enum,              "0",         0, "1. "%LOWEST_STR%
HKR, Ndi\Params\IbssTxPower\enum,              "25",        0, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\Params\IbssTxPower\enum,              "50",        0, "3. "%MEDIUM_STR%
HKR, Ndi\Params\IbssTxPower\enum,              "75",        0, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\Params\IbssTxPower\enum,              "100",       0, "5. "%HIGHEST_STR%
HKR, Ndi\Params\RoamAggressiveness,             ParamDesc,  0, %ROAMING_AGGRESSIVENESS_STR%
HKR, Ndi\Params\RoamAggressiveness,             Type,       2, "enum"
HKR, Ndi\Params\RoamAggressiveness,             Default,    2, "2"
HKR, Ndi\Params\RoamAggressiveness,             Optional,   2, "0"
HKR, Ndi\Params\RoamAggressiveness\enum,        "0",        0, "1. "%LOWEST_STR%
HKR, Ndi\Params\RoamAggressiveness\enum,        "1",        0, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\Params\RoamAggressiveness\enum,        "2",        0, "3. "%MEDIUM_STR%
HKR, Ndi\Params\RoamAggressiveness\enum,        "3",        0, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\Params\RoamAggressiveness\enum,        "4",        0, "5. "%HIGHEST_STR%
HKR, Ndi\Params\CtsToItself,                    ParamDesc,  0, %MIXED_MODE_PROTECTION_STR%
HKR, Ndi\Params\CtsToItself,                    Type,       2, "enum"
HKR, Ndi\Params\CtsToItself,                    Default,    2, "0"
HKR, Ndi\Params\CtsToItself,                    Optional,   2, "0"
HKR, Ndi\Params\CtsToItself\enum,               "0",        0, %RTS_CTS_ENABLED_STR%
HKR, Ndi\Params\CtsToItself\enum,               "1",        0, %CTS_TO_SELF_ENABLED_STR%
HKR, Ndi\Params\FatChannelIntolerant,           ParamDesc,  0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\Params\FatChannelIntolerant,           Type,       0, "enum"
HKR, Ndi\Params\FatChannelIntolerant,           Default,    0, "0"
HKR, Ndi\Params\FatChannelIntolerant,           Optional,   0, "0"
HKR, Ndi\Params\FatChannelIntolerant\enum,      "0",        0, %DISABLED_STR%
HKR, Ndi\Params\FatChannelIntolerant\enum,      "1",        0, %ENABLED_STR%
HKR, Ndi\Params\uAPSDSupport,                   ParamDesc,  0, %U_APSD_SUPPORT%
HKR, Ndi\Params\uAPSDSupport,                   Type,       0, "enum"
HKR, Ndi\Params\uAPSDSupport,                   Optional,   0, "0"
HKR, Ndi\Params\uAPSDSupport,                   Default,    0, "0"
HKR, Ndi\Params\uAPSDSupport\enum,              "0",        0, %DISABLED_STR%
HKR, Ndi\Params\uAPSDSupport\enum,              "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnPattern,                 ParamDesc,  0, %WAKE_ON_PATTERN_MATCH%
HKR, Ndi\Params\*WakeOnPattern\Enum,            "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnPattern\Enum,            "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnPattern,                 type,       0, "enum"
HKR, Ndi\Params\*WakeOnPattern,                 default,    0, "1"
HKR, Ndi\Params\*WakeOnMagicPacket,             ParamDesc,  0, %WAKE_ON_MAGIC_PACKET%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,        "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,        "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket,             type,       0, "enum"
HKR, Ndi\Params\*WakeOnMagicPacket,             default,    0, "1"
HKR, Ndi\Params\*PMWiFiRekeyOffload,            ParamDesc,  0, %PM_WIFI_REKEY_OFFLOAD%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload,            type,       0, "enum"
HKR, Ndi\Params\*PMWiFiRekeyOffload,            default,    0, "1"
HKR, Ndi\Params\*PMARPOffload,                  ParamDesc,  0, %PM_ARP_OFFLOAD%
HKR, Ndi\Params\*PMARPOffload\Enum,             "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMARPOffload\Enum,             "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMARPOffload,                  type,       0, "enum"
HKR, Ndi\Params\*PMARPOffload,                  default,    0, "1"
HKR, Ndi\Params\*PMNSOffload,                   ParamDesc,  0, %PM_NS_OFFLOAD%
HKR, Ndi\Params\*PMNSOffload\Enum,              "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMNSOffload\Enum,              "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMNSOffload,                   type,       0, "enum"
HKR, Ndi\Params\*PMNSOffload,                   default,    0, "1"
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       ParamDesc,  0, %DEVICE_SLEEP_ON_DISCONNECT%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       type,       0, "enum"
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       default,    0, "0"
HKR, Ndi\Params\MIMOPowerSaveMode,              ParamDesc,  0, %MIMO_POWER_SAVE_MODE_STR%
HKR, Ndi\Params\MIMOPowerSaveMode,              Type,       2, "enum"
HKR, Ndi\Params\MIMOPowerSaveMode,              Default,    2, "0"
HKR, Ndi\Params\MIMOPowerSaveMode,              Optional,   2, "0"
HKR, Ndi\Params\MIMOPowerSaveMode\enum,         "0",        0, %MIMO_AUTO_STR%
HKR, Ndi\Params\MIMOPowerSaveMode\enum,         "1",        0, %NO_MIMO_STR%
HKR, Ndi\Params\MIMOPowerSaveMode\enum,         "2",        0, %RTS_BEFORE_MIMO_STR%
HKR, Ndi\Params\MIMOPowerSaveMode\enum,         "3",        0, %NO_RTS_BEFORE_MIMO_STR%


[Reg_NDI_2x2_14]
HKR, Ndi\Params\*PacketCoalescing,              ParamDesc,  0, %PACKET_COALESCING%
HKR, Ndi\Params\*PacketCoalescing,              type,       0, "enum"
HKR, Ndi\Params\*PacketCoalescing,              default,    0, "1"
HKR, Ndi\Params\*PacketCoalescing\Enum,         "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PacketCoalescing\Enum,         "1",        0, %ENABLED_STR%


[Reg_NDI_INT_WDI_14]
HKR, Ndi\Interfaces,                            UpperRange, 0, "ndis5,wifipro,intel_psm"
HKR, Ndi\Interfaces,                            LowerRange, 0, "ethernet,wlan,vwifi"
HKR, Ndi,                                       Service,    0, "Netwtw14."


[Reg_Common_WPP_14]
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession, Start, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6B71976C-97EF-4946-861A-B00994DE0939}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6B71976C-97EF-4946-861A-B00994DE0939}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6B71976C-97EF-4946-861A-B00994DE0939}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6B71976C-97EF-4946-861A-B00994DE0939}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{ECC34691-A263-43AF-8863-CBD383025D11}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{ECC34691-A263-43AF-8863-CBD383025D11}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{ECC34691-A263-43AF-8863-CBD383025D11}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{ECC34691-A263-43AF-8863-CBD383025D11}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, EnableFlags, 0x00010001, 0x1fff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{411C4950-F958-4068-BABD-A197472DD6F0}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{411C4950-F958-4068-BABD-A197472DD6F0}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{411C4950-F958-4068-BABD-A197472DD6F0}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{411C4950-F958-4068-BABD-A197472DD6F0}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{91270A90-13CC-45C3-8D64-108876E7302C}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{91270A90-13CC-45C3-8D64-108876E7302C}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{91270A90-13CC-45C3-8D64-108876E7302C}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{91270A90-13CC-45C3-8D64-108876E7302C}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, Status, 0x00010001, 0x0


[Reg_NIC_201_2x2_AX]
HKR,,AdapterModel,0,%NIC_201_2x2_AX%
HKR,,DriverDesc,0,%NIC_201_2x2_AX%

[Reg_NIC_101_1x1_AX_no_160]
HKR,,AdapterModel,0,%NIC_101_1x1_AX_no_160%
HKR,,DriverDesc,0,%NIC_101_1x1_AX_no_160%

[Reg_NIC_203_2x2_AX_no_160]
HKR,,AdapterModel,0,%NIC_203_2x2_AX_no_160%
HKR,,DriverDesc,0,%NIC_203_2x2_AX_no_160%

[Reg_NIC_1650s_2x2_AX]
HKR,,AdapterModel,0,%NIC_1650s_2x2_AX%
HKR,,DriverDesc,0,%NIC_1650s_2x2_AX%

[Reg_NIC_1650i_2x2_AX]
HKR,,AdapterModel,0,%NIC_1650i_2x2_AX%
HKR,,DriverDesc,0,%NIC_1650i_2x2_AX%

; English (default)
[Install_GEN_QSR_JfP2_9560_AC_2x2_WinT]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP2_10,Reg_NIC_9560_2x2_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_QSR_JfP2_9560_AC_2x2_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10



[Install_GEN_QSR_JfP2_9560_AC_2x2_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_GEN_QSR_JfP1_9461_AC_1x1_WinT]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_1x1_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP1_10,Reg_NIC_9461_1x1_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_QSR_JfP1_9461_AC_1x1_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10



[Install_GEN_QSR_JfP1_9461_AC_1x1_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_GEN_QSR_HrP2_201_AX_2x2_WinT]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_10,Reg_AX_10,Reg_NDI_HRP2_10,Reg_NIC_201_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_QSR_HrP2_201_AX_2x2_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10



[Install_GEN_QSR_HrP2_201_AX_2x2_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_GEN_QSR_JfP1_9462_AC_1x1_WinT]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_1x1_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP1_10,Reg_NIC_9462_1x1_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_QSR_JfP1_9462_AC_1x1_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10



[Install_GEN_QSR_JfP1_9462_AC_1x1_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP2_10,Reg_NIC_9560_2x2_AC_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10



[Install_GEN_QSR_JfP2_9560_AC_no_160_2x2_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_1x1_10,Reg_1x1_AX_10,Reg_NDI_AX_10,Reg_AX_10,Reg_NDI_HRP1_10,Reg_NIC_101_1x1_AX_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10



[Install_GEN_QSR_HrP1_101_AX_no_160_1x1_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_1x1_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP1_10,Reg_NIC_9461_1x1_AC_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10



[Install_GEN_QSR_JfP1_9461_AC_no_160_1x1_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_10,Reg_AX_10,Reg_NIC_203_2x2_AX_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10



[Install_GEN_QSR_JnP_203_AX_no_160_2x2_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_1x1_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP1_10,Reg_NIC_9462_1x1_AC_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10



[Install_GEN_QSR_JfP1_9462_AC_no_160_1x1_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_RIV_QSR_JfP2_1550s_AC_2x2_WinT]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AC_10,Reg_AC_10,RegSec_Riv_10,Reg_NDI_JFP2_10,Reg_NIC_1550s_2x2_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_RIV_QSR_JfP2_1550s_AC_2x2_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10



[Install_RIV_QSR_JfP2_1550s_AC_2x2_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_RIV_QSR_JfP2_1550i_AC_2x2_WinT]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AC_10,Reg_AC_10,RegSec_Riv_10,Reg_NDI_JFP2_10,Reg_NIC_1550i_2x2_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_RIV_QSR_JfP2_1550i_AC_2x2_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10



[Install_RIV_QSR_JfP2_1550i_AC_2x2_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_RIV_QSR_HrP2_1650s_AX_2x2_WinT]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_10,Reg_AX_10,RegSec_Riv_10,Reg_NDI_HRP2_10,Reg_NIC_1650s_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_RIV_QSR_HrP2_1650s_AX_2x2_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10



[Install_RIV_QSR_HrP2_1650s_AX_2x2_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_RIV_QSR_HrP2_1650i_AX_2x2_WinT]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_10,Reg_AX_10,RegSec_Riv_10,Reg_NDI_HRP2_10,Reg_NIC_1650i_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_RIV_QSR_HrP2_1650i_AX_2x2_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10



[Install_RIV_QSR_HrP2_1650i_AX_2x2_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_GEN_QSR_CcP_200_AX_2x2_WinT]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_10,Reg_AX_10,Reg_NDI_CCP_10,Reg_NIC_200_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_QSR_CcP_200_AX_2x2_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10



[Install_GEN_QSR_CcP_200_AX_2x2_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_RIV_QSR_CcP_1650w_AX_2x2_WinT]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_10,Reg_AX_10,RegSec_Riv_10,Reg_NDI_CCP_10,Reg_NIC_1650w_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_RIV_QSR_CcP_1650w_AX_2x2_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10



[Install_RIV_QSR_CcP_1650w_AX_2x2_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_RIV_QSR_CcP_1650x_AX_2x2_WinT]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AX_10,Reg_AX_10,RegSec_Riv_10,Reg_NDI_CCP_10,Reg_NIC_1650x_2x2_AX
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_RIV_QSR_CcP_1650x_AX_2x2_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_quasar.reg_10



[Install_RIV_QSR_CcP_1650x_AX_2x2_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_GEN_SLR_JfP2_9560_AC_2x2_WinT]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP2_10,Reg_NIC_9560_2x2_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_SLR_JfP2_9560_AC_2x2_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_solar.reg_10



[Install_GEN_SLR_JfP2_9560_AC_2x2_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_GEN_SLR_JfP1_9461_AC_1x1_WinT]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_1x1_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP1_10,Reg_NIC_9461_1x1_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_SLR_JfP1_9461_AC_1x1_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_solar.reg_10



[Install_GEN_SLR_JfP1_9461_AC_1x1_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_GEN_SLR_JfP1_9462_AC_1x1_WinT]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_1x1_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP1_10,Reg_NIC_9462_1x1_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_SLR_JfP1_9462_AC_1x1_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_solar.reg_10



[Install_GEN_SLR_JfP1_9462_AC_1x1_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP2_10,Reg_NIC_9560_2x2_AC_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_solar.reg_10



[Install_GEN_SLR_JfP2_9560_AC_no_160_2x2_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_GEN_SLR_JfP1_9461_AC_no_160_1x1_WinT]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_1x1_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP1_10,Reg_NIC_9461_1x1_AC_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_SLR_JfP1_9461_AC_no_160_1x1_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_solar.reg_10



[Install_GEN_SLR_JfP1_9461_AC_no_160_1x1_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_1x1_10,Reg_NDI_AC_10,Reg_AC_10,Reg_NDI_JFP1_10,Reg_NIC_9462_1x1_AC_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_solar.reg_10



[Install_GEN_SLR_JfP1_9462_AC_no_160_1x1_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_RIV_SLR_JfP2_1550s_AC_2x2_WinT]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AC_10,Reg_AC_10,RegSec_Riv_10,Reg_NDI_JFP2_10,Reg_NIC_1550s_2x2_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_RIV_SLR_JfP2_1550s_AC_2x2_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_solar.reg_10



[Install_RIV_SLR_JfP2_1550s_AC_2x2_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[Install_RIV_SLR_JfP2_1550i_AC_2x2_WinT]
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common_10
AddReg               = Reg_Common_10,Reg_Common_WPP_10,Reg_NDI_10,Reg_NDI_INT_WDI_10,Reg_IHV_Router_10,Reg_2x2_10,Reg_NDI_2x2_10,Reg_NDI_AC_10,Reg_AC_10,RegSec_Riv_10,Reg_NDI_JFP2_10,Reg_NIC_1550i_2x2_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver_10_WinT,CopyFiles_IHV_Router_10_WinT
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_RIV_SLR_JfP2_1550i_AC_2x2_WinT.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_solar.reg_10



[Install_RIV_SLR_JfP2_1550i_AC_2x2_WinT.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw10, 2,NIC_Service_10_WinT,Common_EventLog_10_WinT



[NIC_Service_10_WinT]
DisplayName          = "___" %NIC_Service_DispName_WINT_64%
ServiceType          = 1 ;%SERVICE_KERNEL_DRIVER%
StartType            = 3 ;%SERVICE_DEMAND_START%
ErrorControl         = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary        = %12%\Netwtw10.sys
LoadOrderGroup       = NDIS



[CopyFiles_Driver_10_WinT]
Netwtw10.sys,,,2
Netwfw10.dat,,,2



[CopyFiles_IHV_Router_10_WinT]
IntelIHVRouter10.dll,,,2



[Common_EventLog_10_WinT]
AddReg               = Reg_CommonAddEventLog_10_WinT



[Reg_CommonAddEventLog_10_WinT]
HKR,, EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\Drivers\Netwtw10.sys"
HKR,, TypesSupported,   0x00010001, 7



[DelReg_Common_10]
HKR, Ndi\



[Reg_Common_10]
HKR,,ExternalImage,0x10001,0x0
HKR,,FixedSupportedRates,0x10001,0xFFF
HKR,,ModulationType,2,"2"
HKR,,RadioEnable,0x10003,0x1
HKR,,RecommendedBeaconInterval,0x10001,0x64
HKR,,AtomMaxDpcTime,0x10001,0x14
HKR,,MaxDpcTime,0x10001,0x1E
HKR,,DuplicateRateSupported,0x10001,0x0
HKR,,ChannelWidth24,0,"1"
HKR,,ChannelWidth52,0,"1"
HKR,,CtsToItself,0,"0"
HKR,,*MiracastSupported,0x10001,0x1
HKR,,uAPSDSupport,0x10001,0
HKR,,SkipOverDtimEnable,0x10001,0x1
HKR,,LprxEnable,0x10001,0x1
HKR,,GreenFieldCapable,0x10001,0x0
HKR,,PanEnabled,0x10001,0x1
HKR,,BaEnable,0x10001,0x1
HKR,,TGeEnableBits,0x10001,0x00000037
HKR,,CtdpSupported,0x10001,1



[Reg_NDI_JFP2_10]
HKR,,CLSGUID,0,"{0AC246D9-E2E5-4CD8-892B-7A3710024CA5}"



[Reg_NDI_JFP1_10]
HKR,,CLSGUID,0,"{5D8EFC94-E593-408E-B857-1D7339774A15}"



[Reg_NDI_HRP2_10]
HKR,,CLSGUID,0,"{6506FE8C-5B1A-4A97-9AF4-4A9E325A69CC}"



[Reg_NDI_HRP1_10]
HKR,,CLSGUID,0,"{889E3741-FCC9-4FC0-973C-6FBDA8DF8573}"



[Reg_NDI_CCP_10]
HKR,,CLSGUID,0,"{01E2765C-EEDC-4DB9-85A0-503A400892A0}"



[Reg_1x1_10]
HKR,,FixedSupportedHtRates,0x10001,0x000000FF
HKR,,SystemAllowedAntennas,0x10001,0x101
HKR,,VhtSupportedRxMcs,0x10001,0xFFFE
HKR,,VhtsupportedTxMcs,0x10001,0x2000FFFE
HKR,,GoVhtSupportedRxMcs,0x10001,0xFFFE
HKR,,GoVhtSupportedTxMcs,0x10001,0xFFFE
HKR,,rlcChainSettings,0x10001,0x2
HKR,,tlcValidAntenna,0x10001,0x1



[Reg_2x2_10]
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF
HKR,,SystemAllowedAntennas,0x10001,0x303



[Reg_1x1_AX_10]
HKR,,HeTxRxMcsNssSupportDword0,0x10001,0xFFFEFFFE
HKR,,HeTxRxMcsNssSupportDword1,0x10001,0xFFFEFFFE
HKR,,HeGoTxRxMcsNssSupportDword0,0x10001,0xFFFEFFFE
HKR,,HeGoTxRxMcsNssSupportDword1,0x10001,0xFFFEFFFE



[Reg_AC_10]
HKR,,SKU_CAP,0x10001,0xf



[Reg_AX_10]
HKR,,SKU_CAP,0x10001,0x1f



[MSI_NDIS_quasar.reg_10]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x10001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x10001, 2
HKR, "Interrupt Management\Affinity Policy", DevicePolicy, 0x00010001, 4
HKR, "Interrupt Management\Affinity Policy", AssignmentSetOverride, 0x00000003, 1



[MSI_NDIS_solar.reg_10]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x10001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x10001, 3
HKR, "Interrupt Management\Affinity Policy", DevicePolicy, 0x00010001, 0
HKR, "Interrupt Management\Affinity Policy", AssignmentSetOverride, 0x00000003, 0



[RegSec_Riv_10]
HKR,,QosClassMap,0x00000000,"00000000211111112222222233333333544444445555556566666666777777773012"



[Reg_IHV_Router_10]
HKR,Ndi\IHVExtensions, ExtensibilityDLL, 0, "%%SystemRoot%%\system32\IntelIHVRouter10.dll"



[Reg_NDI_AC_10]
HKR, Ndi\Params\IEEE11nMode,                   ParamDesc,   0, %11N_AC_MODE%
HKR, Ndi\Params\IEEE11nMode,                   Type,        0, "enum"
HKR, Ndi\Params\IEEE11nMode,                   Default,     0, "2"
HKR, Ndi\Params\IEEE11nMode,                   Optional,    0, "0"
HKR, Ndi\Params\IEEE11nMode\enum,              "0",         0, "1. "%DISABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "1",         0, "2. "%HT_ENABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "2",         0, "3. "%VHT_ENABLED_STR%



[Reg_NDI_AX_10]
HKR, Ndi\Params\IEEE11nMode,                   ParamDesc,   0, %11N_AX_MODE%
HKR, Ndi\Params\IEEE11nMode,                   Type,        0, "enum"
HKR, Ndi\Params\IEEE11nMode,                   Default,     0, "3"
HKR, Ndi\Params\IEEE11nMode,                   Optional,    0, "0"
HKR, Ndi\Params\IEEE11nMode\enum,              "0",         0, "1. "%DISABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "1",         0, "2. "%HT_ENABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "2",         0, "3. "%VHT_ENABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "3",         0, "4. "%11AX_ENABLED_STR%



[Reg_NDI_10]
HKR, Ndi\Params\ThroughputBoosterEnabled,      ParamDesc,   0, %THROUGHPUTBOOSTER_STR%
HKR, Ndi\Params\ThroughputBoosterEnabled,      Type,        2, "enum"
HKR, Ndi\Params\ThroughputBoosterEnabled,      Default,     2, "0"
HKR, Ndi\Params\ThroughputBoosterEnabled,      Optional,    2, "0"
HKR, Ndi\Params\ThroughputBoosterEnabled\enum, "0",         0, %DISABLED_STR%
HKR, Ndi\Params\ThroughputBoosterEnabled\enum, "1",         0, %ENABLED_STR%
HKR, Ndi\Params\WirelessMode,                  ParamDesc,   0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode,                  Type,        0, "enum",
HKR, Ndi\Params\WirelessMode,                  Default,     0, "34" ;abg
HKR, Ndi\Params\WirelessMode,                  Optional,    0, "0"
HKR, Ndi\Params\WirelessMode\enum,             "17",        0, "1. "%WIRELESS_MODE_A%
HKR, Ndi\Params\WirelessMode\enum,             "0",         0, "2. "%WIRELESS_MODE_B%
HKR, Ndi\Params\WirelessMode\enum,             "16",        0, "3. "%WIRELESS_MODE_G%
HKR, Ndi\Params\WirelessMode\enum,             "32",        0, "4. "%WIRELESS_MODE_BG%
HKR, Ndi\Params\WirelessMode\enum,             "18",        0, "5. "%WIRELESS_MODE_AG%
HKR, Ndi\Params\WirelessMode\enum,             "34",        0, "6. "%WIRELESS_MODE_ABG%
HKR, Ndi\Params\RoamingPreferredBandType,      ParamDesc,   0, %PREFERRED_BAND_STR%
HKR, Ndi\Params\RoamingPreferredBandType,      Type,        2, "enum"
HKR, Ndi\Params\RoamingPreferredBandType,      Default,     2, "0"
HKR, Ndi\Params\RoamingPreferredBandType,      Optional,    2, "0"
HKR, Ndi\Params\RoamingPreferredBandType\enum, "0",         0, "1. "%NO_PREFERECE_STR%
HKR, Ndi\Params\RoamingPreferredBandType\enum, "1",         0, "2. "%PREFER_24_BAND_STR%
HKR, Ndi\Params\RoamingPreferredBandType\enum, "2",         0, "3. "%PREFER_52_BAND_STR%
HKR, Ndi\Params\ChannelWidth24,                ParamDesc,   0,     %CHANNELWIDTH24%
HKR, Ndi\Params\ChannelWidth24,                Type,        0,     "enum"
HKR, Ndi\Params\ChannelWidth24,                Default,     0,     "1"
HKR, Ndi\Params\ChannelWidth24,                Optional,    0,     "0"
HKR, Ndi\Params\ChannelWidth24\enum,           "0",         0,     %CHANNELWIDTH20ONLY%
HKR, Ndi\Params\ChannelWidth24\enum,           "1",         0,     %CHANNELWIDTHAUTO%
HKR, Ndi\Params\ChannelWidth52,                ParamDesc,   0,  %CHANNELWIDTH52%
HKR, Ndi\Params\ChannelWidth52,                Type,        0,  "enum"
HKR, Ndi\Params\ChannelWidth52,                Default,     0,  "1"
HKR, Ndi\Params\ChannelWidth52,                Optional,    0,  "0"
HKR, Ndi\Params\ChannelWidth52\enum,           "0",         0,  %CHANNELWIDTH20ONLY%
HKR, Ndi\Params\ChannelWidth52\enum,           "1",         0,  %CHANNELWIDTHAUTO%
HKR, Ndi\Params\IbssTxPower,                   ParamDesc,   0, %IBSS_TX_POWER_STR%
HKR, Ndi\Params\IbssTxPower,                   Type,        2, "enum"
HKR, Ndi\Params\IbssTxPower,                   Default,     2, "100"
HKR, Ndi\Params\IbssTxPower,                   Optional,    2, "0"
HKR, Ndi\Params\IbssTxPower\enum,              "0",         0, "1. "%LOWEST_STR%
HKR, Ndi\Params\IbssTxPower\enum,              "25",        0, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\Params\IbssTxPower\enum,              "50",        0, "3. "%MEDIUM_STR%
HKR, Ndi\Params\IbssTxPower\enum,              "75",        0, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\Params\IbssTxPower\enum,              "100",       0, "5. "%HIGHEST_STR%
HKR, Ndi\Params\RoamAggressiveness,             ParamDesc,  0, %ROAMING_AGGRESSIVENESS_STR%
HKR, Ndi\Params\RoamAggressiveness,             Type,       2, "enum"
HKR, Ndi\Params\RoamAggressiveness,             Default,    2, "2"
HKR, Ndi\Params\RoamAggressiveness,             Optional,   2, "0"
HKR, Ndi\Params\RoamAggressiveness\enum,        "0",        0, "1. "%LOWEST_STR%
HKR, Ndi\Params\RoamAggressiveness\enum,        "1",        0, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\Params\RoamAggressiveness\enum,        "2",        0, "3. "%MEDIUM_STR%
HKR, Ndi\Params\RoamAggressiveness\enum,        "3",        0, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\Params\RoamAggressiveness\enum,        "4",        0, "5. "%HIGHEST_STR%
HKR, Ndi\Params\CtsToItself,                    ParamDesc,  0, %MIXED_MODE_PROTECTION_STR%
HKR, Ndi\Params\CtsToItself,                    Type,       2, "enum"
HKR, Ndi\Params\CtsToItself,                    Default,    2, "0"
HKR, Ndi\Params\CtsToItself,                    Optional,   2, "0"
HKR, Ndi\Params\CtsToItself\enum,               "0",        0, %RTS_CTS_ENABLED_STR%
HKR, Ndi\Params\CtsToItself\enum,               "1",        0, %CTS_TO_SELF_ENABLED_STR%
HKR, Ndi\Params\FatChannelIntolerant,           ParamDesc,  0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\Params\FatChannelIntolerant,           Type,       0, "enum"
HKR, Ndi\Params\FatChannelIntolerant,           Default,    0, "0"
HKR, Ndi\Params\FatChannelIntolerant,           Optional,   0, "0"
HKR, Ndi\Params\FatChannelIntolerant\enum,      "0",        0, %DISABLED_STR%
HKR, Ndi\Params\FatChannelIntolerant\enum,      "1",        0, %ENABLED_STR%
HKR, Ndi\Params\uAPSDSupport,                   ParamDesc,  0, %U_APSD_SUPPORT%
HKR, Ndi\Params\uAPSDSupport,                   Type,       0, "enum"
HKR, Ndi\Params\uAPSDSupport,                   Optional,   0, "0"
HKR, Ndi\Params\uAPSDSupport,                   Default,    0, "0"
HKR, Ndi\Params\uAPSDSupport\enum,              "0",        0, %DISABLED_STR%
HKR, Ndi\Params\uAPSDSupport\enum,              "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnPattern,                 ParamDesc,  0, %WAKE_ON_PATTERN_MATCH%
HKR, Ndi\Params\*WakeOnPattern\Enum,            "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnPattern\Enum,            "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnPattern,                 type,       0, "enum"
HKR, Ndi\Params\*WakeOnPattern,                 default,    0, "1"
HKR, Ndi\Params\*WakeOnMagicPacket,             ParamDesc,  0, %WAKE_ON_MAGIC_PACKET%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,        "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,        "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket,             type,       0, "enum"
HKR, Ndi\Params\*WakeOnMagicPacket,             default,    0, "1"
HKR, Ndi\Params\*PMWiFiRekeyOffload,            ParamDesc,  0, %PM_WIFI_REKEY_OFFLOAD%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload,            type,       0, "enum"
HKR, Ndi\Params\*PMWiFiRekeyOffload,            default,    0, "1"
HKR, Ndi\Params\*PMARPOffload,                  ParamDesc,  0, %PM_ARP_OFFLOAD%
HKR, Ndi\Params\*PMARPOffload\Enum,             "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMARPOffload\Enum,             "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMARPOffload,                  type,       0, "enum"
HKR, Ndi\Params\*PMARPOffload,                  default,    0, "1"
HKR, Ndi\Params\*PMNSOffload,                   ParamDesc,  0, %PM_NS_OFFLOAD%
HKR, Ndi\Params\*PMNSOffload\Enum,              "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMNSOffload\Enum,              "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMNSOffload,                   type,       0, "enum"
HKR, Ndi\Params\*PMNSOffload,                   default,    0, "1"
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       ParamDesc,  0, %DEVICE_SLEEP_ON_DISCONNECT%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       type,       0, "enum"
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       default,    0, "0"
HKR, Ndi\Params\MIMOPowerSaveMode,              ParamDesc,  0, %MIMO_POWER_SAVE_MODE_STR%
HKR, Ndi\Params\MIMOPowerSaveMode,              Type,       2, "enum"
HKR, Ndi\Params\MIMOPowerSaveMode,              Default,    2, "0"
HKR, Ndi\Params\MIMOPowerSaveMode,              Optional,   2, "0"
HKR, Ndi\Params\MIMOPowerSaveMode\enum,         "0",        0, %MIMO_AUTO_STR%
HKR, Ndi\Params\MIMOPowerSaveMode\enum,         "1",        0, %NO_MIMO_STR%
HKR, Ndi\Params\MIMOPowerSaveMode\enum,         "2",        0, %RTS_BEFORE_MIMO_STR%
HKR, Ndi\Params\MIMOPowerSaveMode\enum,         "3",        0, %NO_RTS_BEFORE_MIMO_STR%



[Reg_NDI_2x2_10]
HKR, Ndi\Params\*PacketCoalescing,              ParamDesc,  0, %PACKET_COALESCING%
HKR, Ndi\Params\*PacketCoalescing,              type,       0, "enum"
HKR, Ndi\Params\*PacketCoalescing,              default,    0, "1"
HKR, Ndi\Params\*PacketCoalescing\Enum,         "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PacketCoalescing\Enum,         "1",        0, %ENABLED_STR%



[Reg_NDI_INT_WDI_10]
HKR, Ndi\Interfaces,                            UpperRange, 0, "ndis5,wifipro,intel_psm"
HKR, Ndi\Interfaces,                            LowerRange, 0, "ethernet,wlan,vwifi"
HKR, Ndi,                                       Service,    0, "Netwtw10."



[Reg_Common_WPP_10]
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession, Start, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6B71976C-97EF-4946-861A-B00994DE0939}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6B71976C-97EF-4946-861A-B00994DE0939}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6B71976C-97EF-4946-861A-B00994DE0939}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6B71976C-97EF-4946-861A-B00994DE0939}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{ECC34691-A263-43AF-8863-CBD383025D11}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{ECC34691-A263-43AF-8863-CBD383025D11}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{ECC34691-A263-43AF-8863-CBD383025D11}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{ECC34691-A263-43AF-8863-CBD383025D11}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, EnableFlags, 0x00010001, 0x1fff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{411C4950-F958-4068-BABD-A197472DD6F0}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{411C4950-F958-4068-BABD-A197472DD6F0}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{411C4950-F958-4068-BABD-A197472DD6F0}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{411C4950-F958-4068-BABD-A197472DD6F0}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{91270A90-13CC-45C3-8D64-108876E7302C}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{91270A90-13CC-45C3-8D64-108876E7302C}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{91270A90-13CC-45C3-8D64-108876E7302C}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{91270A90-13CC-45C3-8D64-108876E7302C}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, Status, 0x00010001, 0x0



[Reg_NIC_9560_2x2_AC]
HKR,,AdapterModel,0,%NIC_9560_2x2_AC%
HKR,,DriverDesc,0,%NIC_9560_2x2_AC%


[Reg_NIC_9461_1x1_AC]
HKR,,AdapterModel,0,%NIC_9461_1x1_AC%
HKR,,DriverDesc,0,%NIC_9461_1x1_AC%


[Reg_NIC_9462_1x1_AC]
HKR,,AdapterModel,0,%NIC_9462_1x1_AC%
HKR,,DriverDesc,0,%NIC_9462_1x1_AC%


[Reg_NIC_9560_2x2_AC_no_160]
HKR,,AdapterModel,0,%NIC_9560_2x2_AC_no_160%
HKR,,DriverDesc,0,%NIC_9560_2x2_AC_no_160%


[Reg_NIC_9461_1x1_AC_no_160]
HKR,,AdapterModel,0,%NIC_9461_1x1_AC_no_160%
HKR,,DriverDesc,0,%NIC_9461_1x1_AC_no_160%


[Reg_NIC_9462_1x1_AC_no_160]
HKR,,AdapterModel,0,%NIC_9462_1x1_AC_no_160%
HKR,,DriverDesc,0,%NIC_9462_1x1_AC_no_160%


[Reg_NIC_1550s_2x2_AC]
HKR,,AdapterModel,0,%NIC_1550s_2x2_AC%
HKR,,DriverDesc,0,%NIC_1550s_2x2_AC%


[Reg_NIC_1550i_2x2_AC]
HKR,,AdapterModel,0,%NIC_1550i_2x2_AC%
HKR,,DriverDesc,0,%NIC_1550i_2x2_AC%

; English (default)

[Reg_NIC_200_2x2_AX]
HKR,,AdapterModel,0,%NIC_200_2x2_AX%
HKR,,DriverDesc,0,%NIC_200_2x2_AX%



[Reg_NIC_1650w_2x2_AX]
HKR,,AdapterModel,0,%NIC_1650w_2x2_AX%
HKR,,DriverDesc,0,%NIC_1650w_2x2_AX%



[Reg_NIC_1650x_2x2_AX]
HKR,,AdapterModel,0,%NIC_1650x_2x2_AX%
HKR,,DriverDesc,0,%NIC_1650x_2x2_AX%

; English (default)


[Install_BU_PSR_ThP_9260_AC_2x2]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common
AddReg               = Reg_Common,Reg_Common_WPP,Reg_NDI,Reg_NDI_INT_WDI,Reg_IHV_Router,Reg_2x2,Reg_NDI_2x2,Reg_NDI_AC,Reg_AC,RegSec_BU,Reg_NDI_THP,Reg_NIC_9260_2x2_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver,CopyFiles_IHV_Router
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_BU_PSR_ThP_9260_AC_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_pulsar.reg



[Install_BU_PSR_ThP_9260_AC_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw08, 2,NIC_Service,Common_EventLog



[Install_GEN_PSR_ThP_9260_AC_2x2]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common
AddReg               = Reg_Common,Reg_Common_WPP,Reg_NDI,Reg_NDI_INT_WDI,Reg_IHV_Router,Reg_2x2,Reg_NDI_2x2,Reg_NDI_AC,Reg_AC,Reg_NDI_THP,Reg_NIC_9260_2x2_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver,CopyFiles_IHV_Router
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_PSR_ThP_9260_AC_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_pulsar.reg



[Install_GEN_PSR_ThP_9260_AC_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw08, 2,NIC_Service,Common_EventLog



[Install_GEN_PSR_JfP_9560_AC_2x2]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common
AddReg               = Reg_Common,Reg_Common_WPP,Reg_NDI,Reg_NDI_INT_WDI,Reg_IHV_Router,Reg_2x2,Reg_NDI_2x2,Reg_NDI_AC,Reg_AC,Reg_NDI_JFP,Reg_NIC_9560_2x2_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver,CopyFiles_IHV_Router
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_PSR_JfP_9560_AC_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_pulsar.reg



[Install_GEN_PSR_JfP_9560_AC_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw08, 2,NIC_Service,Common_EventLog



[Install_GEN_PSR_JfP1_9461_AC_1x1]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common
AddReg               = Reg_Common,Reg_Common_WPP,Reg_NDI,Reg_NDI_INT_WDI,Reg_IHV_Router,Reg_1x1,Reg_NDI_AC,Reg_AC,Reg_NDI_JFP1,Reg_NIC_9461_1x1_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver,CopyFiles_IHV_Router
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_PSR_JfP1_9461_AC_1x1.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_pulsar.reg



[Install_GEN_PSR_JfP1_9461_AC_1x1.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw08, 2,NIC_Service,Common_EventLog



[Install_GEN_PSR_JfP1_9462_AC_1x1]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common
AddReg               = Reg_Common,Reg_Common_WPP,Reg_NDI,Reg_NDI_INT_WDI,Reg_IHV_Router,Reg_1x1,Reg_NDI_AC,Reg_AC,Reg_NDI_JFP1,Reg_NIC_9462_1x1_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver,CopyFiles_IHV_Router
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_PSR_JfP1_9462_AC_1x1.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_pulsar.reg



[Install_GEN_PSR_JfP1_9462_AC_1x1.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw08, 2,NIC_Service,Common_EventLog



[Install_GEN_PSR_ThP_9260_AC_no_160_2x2]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common
AddReg               = Reg_Common,Reg_Common_WPP,Reg_NDI,Reg_NDI_INT_WDI,Reg_IHV_Router,Reg_2x2,Reg_NDI_2x2,Reg_NDI_AC,Reg_AC,Reg_NDI_THP,Reg_NIC_9260_2x2_AC_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver,CopyFiles_IHV_Router
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_PSR_ThP_9260_AC_no_160_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_pulsar.reg



[Install_GEN_PSR_ThP_9260_AC_no_160_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw08, 2,NIC_Service,Common_EventLog



[Install_GEN_PSR_JfP_9560_AC_no_160_2x2]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common
AddReg               = Reg_Common,Reg_Common_WPP,Reg_NDI,Reg_NDI_INT_WDI,Reg_IHV_Router,Reg_2x2,Reg_NDI_2x2,Reg_NDI_AC,Reg_AC,Reg_NDI_JFP,Reg_NIC_9560_2x2_AC_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver,CopyFiles_IHV_Router
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_PSR_JfP_9560_AC_no_160_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_pulsar.reg



[Install_GEN_PSR_JfP_9560_AC_no_160_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw08, 2,NIC_Service,Common_EventLog



[Install_GEN_PSR_JfP1_9461_AC_no_160_1x1]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common
AddReg               = Reg_Common,Reg_Common_WPP,Reg_NDI,Reg_NDI_INT_WDI,Reg_IHV_Router,Reg_1x1,Reg_NDI_AC,Reg_AC,Reg_NDI_JFP1,Reg_NIC_9461_1x1_AC_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver,CopyFiles_IHV_Router
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_PSR_JfP1_9461_AC_no_160_1x1.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_pulsar.reg



[Install_GEN_PSR_JfP1_9461_AC_no_160_1x1.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw08, 2,NIC_Service,Common_EventLog



[Install_GEN_PSR_JfP1_9462_AC_no_160_1x1]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common
AddReg               = Reg_Common,Reg_Common_WPP,Reg_NDI,Reg_NDI_INT_WDI,Reg_IHV_Router,Reg_1x1,Reg_NDI_AC,Reg_AC,Reg_NDI_JFP1,Reg_NIC_9462_1x1_AC_no_160
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver,CopyFiles_IHV_Router
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_GEN_PSR_JfP1_9462_AC_no_160_1x1.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_pulsar.reg



[Install_GEN_PSR_JfP1_9462_AC_no_160_1x1.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw08, 2,NIC_Service,Common_EventLog



[Install_RIV_PSR_ThP_1550_AC_2x2]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common
AddReg               = Reg_Common,Reg_Common_WPP,Reg_NDI,Reg_NDI_INT_WDI,Reg_IHV_Router,Reg_2x2,Reg_NDI_2x2,Reg_NDI_AC,Reg_AC,RegSec_Riv,Reg_NDI_THP,Reg_NIC_1550_2x2_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver,CopyFiles_IHV_Router
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_RIV_PSR_ThP_1550_AC_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_pulsar.reg



[Install_RIV_PSR_ThP_1550_AC_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw08, 2,NIC_Service,Common_EventLog



[Install_RIV_PSR_JfP_1550s_AC_2x2]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common
AddReg               = Reg_Common,Reg_Common_WPP,Reg_NDI,Reg_NDI_INT_WDI,Reg_IHV_Router,Reg_2x2,Reg_NDI_2x2,Reg_NDI_AC,Reg_AC,RegSec_Riv,Reg_NDI_JFP,Reg_NIC_1550s_2x2_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver,CopyFiles_IHV_Router
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_RIV_PSR_JfP_1550s_AC_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_pulsar.reg



[Install_RIV_PSR_JfP_1550s_AC_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw08, 2,NIC_Service,Common_EventLog



[Install_RIV_PSR_JfP_1550i_AC_2x2]
FeatureScore         = 0xFC
Include              = netvwifibus.inf
Needs                = VWiFiBus.CopyFiles
DelReg               = DelReg_Common
AddReg               = Reg_Common,Reg_Common_WPP,Reg_NDI,Reg_NDI_INT_WDI,Reg_IHV_Router,Reg_2x2,Reg_NDI_2x2,Reg_NDI_AC,Reg_AC,RegSec_Riv,Reg_NDI_JFP,Reg_NIC_1550i_2x2_AC
Characteristics      = 0x84 ; NCF_HAS_UI, NCF_PHYSICAL
BusType              = 5    ; PCI bus
CopyFiles            = CopyFiles_Driver,CopyFiles_IHV_Router
*IfType              = 71   ; IF_TYPE_IEEE80211
*MediaType           = 16   ; NdisMediumNative802_11
*PhysicalMediaType   = 9    ; NdisPhysicalMediumNative802_11



[Install_RIV_PSR_JfP_1550i_AC_2x2.HW]
Include              = netvwifibus.inf
Needs                = VWiFiBus.PnPFilterRegistration.HW
AddReg               = MSI_NDIS_pulsar.reg



[Install_RIV_PSR_JfP_1550i_AC_2x2.Services]
Include              = netvwifibus.inf
Needs                = VWiFiBus.Services
AddService           = Netwtw08, 2,NIC_Service,Common_EventLog



[NIC_Service]
DisplayName          = "___" %NIC_Service_DispName_WINT_64%
ServiceType          = 1 ;%SERVICE_KERNEL_DRIVER%
StartType            = 3 ;%SERVICE_DEMAND_START%
ErrorControl         = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary        = %12%\Netwtw08.sys
LoadOrderGroup       = NDIS



[CopyFiles_Driver]
Netwtw08.sys,,,2
Netwfw08.dat,,,2



[CopyFiles_IHV_Router]
IntelIHVRouter08.dll,,,2



[Common_EventLog]
AddReg               = Reg_CommonAddEventLog



[Reg_CommonAddEventLog]
HKR,, EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\Drivers\Netwtw08.sys"
HKR,, TypesSupported,   0x00010001, 7



[DelReg_Common]
HKR, Ndi\



[Reg_Common]
HKR,,ApsdTriggerQueues,0x10001,0x0
HKR,,CardType,0x10001,2
HKR,,CCXv4FeatureSet,0x10001,0x0
HKR,,CcxSdkActive,0x10003,0x1
HKR,,CcxVersion,0x10003,0x4
HKR,,ConfigurationName,0,"PR0W1RELE55"
HKR,,ConnectionPriority,0,"2"
HKR,,DesiredAuthenticationMode,0x10003,0x0
HKR,,DesiredCipher,0x10003,0x1
HKR,,DesiredDefaultKeyId,0x10003,0x1
HKR,,DesiredPortType,0x10003,0x1
HKR,,DesiredPSKey1,0x2,""
HKR,,DesiredPSKey2,0x2,""
HKR,,DesiredPSKey3,0x2,""
HKR,,DesiredPSKey4,0x2,""
HKR,,ExternalImage,0x10001,0x0
HKR,,FixedLongPreamble,0x10001,0x0
HKR,,FixedSupportedRates,0x10001,0xFFF
HKR,,ModulationType,2,"2"
HKR,,NdisEnvironment,0x10001,0
HKR,,NetType,0,"WLAN"
HKR,,PibssShortSlot,0x10001,0x1
HKR,,Provider,0,%PROVIDER_NAME%
HKR,,RadioEnable,0x10003,0x1
HKR,,RecommendedBeaconInterval,0x10001,0x64
HKR,,BTOnThreshold,0x10001,0x4
HKR,,APMMode,0x10001,0x0
HKR,,AtomMaxDpcTime,0x10001,0x14
HKR,,MaxDpcTime,0x10001,0x1E
HKR,,DuplicateRateSupported,0x10001,0x0
HKR,,BaEnable,0x10001,0x0
HKR,,PanTimeoutForResetTxFailCnt,0x10001,0x64
HKR,,ChannelWidth24,0,"1"
HKR,,ChannelWidth52,0,"1"
HKR,,CtsToItself,0,"0"
HKR,,*MiracastSupported,0x10001,0x1
HKR,,uAPSDSupport,0x10001,0
HKR,,SkipOverDtimEnable,0x10001,0x1
HKR,,LprxEnable,0x10001,0x1
HKR,,GreenFieldCapable,0x10001,0x0
HKR,,PanEnabled,0x10001,0x1
HKR,,BaEnable,0x10001,0x1
HKR,,CalibrationActive,0x10001,0x0
HKR,,CalibrationActiveUcode,0x10001,0x0
HKR,,TGeEnableBits,0x10001,0x00000037
HKR,,BTDuration,0x10001,0xFFFFFFFF
HKR,,CtdpSupported,0x10001,1



[Reg_NDI_THP]
HKR,,CLSGUID,0,"{745DB533-B9E9-41D3-89F5-25AD6EE5BE17}"



[Reg_NDI_JFP]
HKR,,CLSGUID,0,"{0AC246D9-E2E5-4CD8-892B-7A3710024CA5}"



[Reg_NDI_JFP1]
HKR,,CLSGUID,0,"{5D8EFC94-E593-408E-B857-1D7339774A15}"



[RegSec_BU]
HKR,,BuFlags,0x10001,0x19



[Reg_1x1]
HKR,,FixedSupportedHtRates,0x10001,0x000000FF
HKR,,SystemAllowedAntennas,0x10001,0x101
HKR,,VhtSupportedRxMcs,0x10001,0xFFFE
HKR,,VhtsupportedTxMcs,0x10001,0x2000FFFE
HKR,,GoVhtSupportedRxMcs,0x10001,0xFFFE
HKR,,GoVhtSupportedTxMcs,0x10001,0xFFFE
HKR,,rlcChainSettings,0x10001,0x2
HKR,,tlcValidAntenna,0x10001,0x1



[Reg_2x2]
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,LowLinearitySupported,0x10001,0



[Reg_AC]
HKR,,SKU_CAP,0x10001,0xf



[MSI_NDIS_pulsar.reg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x10001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x10001, 2



[RegSec_Riv]
HKR,,QosClassMap,0x00000000,"00000000211111112222222233333333544444445555556566666666777777773012"



[Reg_IHV_Router]
HKR,Ndi\IHVExtensions, ExtensibilityDLL, 0, "%%SystemRoot%%\system32\IntelIHVRouter08.dll"



[Reg_NDI_AC]
HKR, Ndi\Params\IEEE11nMode,                   ParamDesc,   0, %11N_AC_MODE%
HKR, Ndi\Params\IEEE11nMode,                   Type,        0, "enum"
HKR, Ndi\Params\IEEE11nMode,                   Default,     0, "2"
HKR, Ndi\Params\IEEE11nMode,                   Optional,    0, "0"
HKR, Ndi\Params\IEEE11nMode\enum,              "0",         0, "1. "%DISABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "1",         0, "2. "%HT_ENABLED_STR%
HKR, Ndi\Params\IEEE11nMode\enum,              "2",         0, "3. "%VHT_ENABLED_STR%



[Reg_NDI]
HKR, Ndi\Params\ThroughputBoosterEnabled,      ParamDesc,   0, %THROUGHPUTBOOSTER_STR%
HKR, Ndi\Params\ThroughputBoosterEnabled,      Type,        2, "enum"
HKR, Ndi\Params\ThroughputBoosterEnabled,      Default,     2, "0"
HKR, Ndi\Params\ThroughputBoosterEnabled,      Optional,    2, "0"
HKR, Ndi\Params\ThroughputBoosterEnabled\enum, "0",         0, %DISABLED_STR%
HKR, Ndi\Params\ThroughputBoosterEnabled\enum, "1",         0, %ENABLED_STR%
HKR, Ndi\Params\WirelessMode,                  ParamDesc,   0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode,                  Type,        0, "enum",
HKR, Ndi\Params\WirelessMode,                  Default,     0, "34" ;abg
HKR, Ndi\Params\WirelessMode,                  Optional,    0, "0"
HKR, Ndi\Params\WirelessMode\enum,             "17",        0, "1. "%WIRELESS_MODE_A%
HKR, Ndi\Params\WirelessMode\enum,             "0",         0, "2. "%WIRELESS_MODE_B%
HKR, Ndi\Params\WirelessMode\enum,             "16",        0, "3. "%WIRELESS_MODE_G%
HKR, Ndi\Params\WirelessMode\enum,             "32",        0, "4. "%WIRELESS_MODE_BG%
HKR, Ndi\Params\WirelessMode\enum,             "18",        0, "5. "%WIRELESS_MODE_AG%
HKR, Ndi\Params\WirelessMode\enum,             "34",        0, "6. "%WIRELESS_MODE_ABG%
HKR, Ndi\Params\RoamingPreferredBandType,      ParamDesc,   0, %PREFERRED_BAND_STR%
HKR, Ndi\Params\RoamingPreferredBandType,      Type,        2, "enum"
HKR, Ndi\Params\RoamingPreferredBandType,      Default,     2, "0"
HKR, Ndi\Params\RoamingPreferredBandType,      Optional,    2, "0"
HKR, Ndi\Params\RoamingPreferredBandType\enum, "0",         0, "1. "%NO_PREFERECE_STR%
HKR, Ndi\Params\RoamingPreferredBandType\enum, "1",         0, "2. "%PREFER_24_BAND_STR%
HKR, Ndi\Params\RoamingPreferredBandType\enum, "2",         0, "3. "%PREFER_52_BAND_STR%
HKR, Ndi\Params\ChannelWidth24,                ParamDesc,   0,     %CHANNELWIDTH24%
HKR, Ndi\Params\ChannelWidth24,                Type,        0,     "enum"
HKR, Ndi\Params\ChannelWidth24,                Default,     0,     "1"
HKR, Ndi\Params\ChannelWidth24,                Optional,    0,     "0"
HKR, Ndi\Params\ChannelWidth24\enum,           "0",         0,     %CHANNELWIDTH20ONLY%
HKR, Ndi\Params\ChannelWidth24\enum,           "1",         0,     %CHANNELWIDTHAUTO%
HKR, Ndi\Params\ChannelWidth52,                ParamDesc,   0,  %CHANNELWIDTH52%
HKR, Ndi\Params\ChannelWidth52,                Type,        0,  "enum"
HKR, Ndi\Params\ChannelWidth52,                Default,     0,  "1"
HKR, Ndi\Params\ChannelWidth52,                Optional,    0,  "0"
HKR, Ndi\Params\ChannelWidth52\enum,           "0",         0,  %CHANNELWIDTH20ONLY%
HKR, Ndi\Params\ChannelWidth52\enum,           "1",         0,  %CHANNELWIDTHAUTO%
HKR, Ndi\Params\IbssTxPower,                   ParamDesc,   0, %IBSS_TX_POWER_STR%
HKR, Ndi\Params\IbssTxPower,                   Type,        2, "enum"
HKR, Ndi\Params\IbssTxPower,                   Default,     2, "100"
HKR, Ndi\Params\IbssTxPower,                   Optional,    2, "0"
HKR, Ndi\Params\IbssTxPower\enum,              "0",         0, "1. "%LOWEST_STR%
HKR, Ndi\Params\IbssTxPower\enum,              "25",        0, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\Params\IbssTxPower\enum,              "50",        0, "3. "%MEDIUM_STR%
HKR, Ndi\Params\IbssTxPower\enum,              "75",        0, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\Params\IbssTxPower\enum,              "100",       0, "5. "%HIGHEST_STR%
HKR, Ndi\Params\RoamAggressiveness,             ParamDesc,  0, %ROAMING_AGGRESSIVENESS_STR%
HKR, Ndi\Params\RoamAggressiveness,             Type,       2, "enum"
HKR, Ndi\Params\RoamAggressiveness,             Default,    2, "2"
HKR, Ndi\Params\RoamAggressiveness,             Optional,   2, "0"
HKR, Ndi\Params\RoamAggressiveness\enum,        "0",        0, "1. "%LOWEST_STR%
HKR, Ndi\Params\RoamAggressiveness\enum,        "1",        0, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\Params\RoamAggressiveness\enum,        "2",        0, "3. "%MEDIUM_STR%
HKR, Ndi\Params\RoamAggressiveness\enum,        "3",        0, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\Params\RoamAggressiveness\enum,        "4",        0, "5. "%HIGHEST_STR%
HKR, Ndi\Params\CtsToItself,                    ParamDesc,  0, %MIXED_MODE_PROTECTION_STR%
HKR, Ndi\Params\CtsToItself,                    Type,       2, "enum"
HKR, Ndi\Params\CtsToItself,                    Default,    2, "0"
HKR, Ndi\Params\CtsToItself,                    Optional,   2, "0"
HKR, Ndi\Params\CtsToItself\enum,               "0",        0, %RTS_CTS_ENABLED_STR%
HKR, Ndi\Params\CtsToItself\enum,               "1",        0, %CTS_TO_SELF_ENABLED_STR%
HKR, Ndi\Params\FatChannelIntolerant,           ParamDesc,  0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\Params\FatChannelIntolerant,           Type,       0, "enum"
HKR, Ndi\Params\FatChannelIntolerant,           Default,    0, "0"
HKR, Ndi\Params\FatChannelIntolerant,           Optional,   0, "0"
HKR, Ndi\Params\FatChannelIntolerant\enum,      "0",        0, %DISABLED_STR%
HKR, Ndi\Params\FatChannelIntolerant\enum,      "1",        0, %ENABLED_STR%
HKR, Ndi\Params\uAPSDSupport,                   ParamDesc,  0, %U_APSD_SUPPORT%
HKR, Ndi\Params\uAPSDSupport,                   Type,       0, "enum"
HKR, Ndi\Params\uAPSDSupport,                   Optional,   0, "0"
HKR, Ndi\Params\uAPSDSupport,                   Default,    0, "0"
HKR, Ndi\Params\uAPSDSupport\enum,              "0",        0, %DISABLED_STR%
HKR, Ndi\Params\uAPSDSupport\enum,              "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnPattern,                 ParamDesc,  0, %WAKE_ON_PATTERN_MATCH%
HKR, Ndi\Params\*WakeOnPattern\Enum,            "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnPattern\Enum,            "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnPattern,                 type,       0, "enum"
HKR, Ndi\Params\*WakeOnPattern,                 default,    0, "1"
HKR, Ndi\Params\*WakeOnMagicPacket,             ParamDesc,  0, %WAKE_ON_MAGIC_PACKET%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,        "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,        "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket,             type,       0, "enum"
HKR, Ndi\Params\*WakeOnMagicPacket,             default,    0, "1"
HKR, Ndi\Params\*PMWiFiRekeyOffload,            ParamDesc,  0, %PM_WIFI_REKEY_OFFLOAD%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload,            type,       0, "enum"
HKR, Ndi\Params\*PMWiFiRekeyOffload,            default,    0, "1"
HKR, Ndi\Params\*PMARPOffload,                  ParamDesc,  0, %PM_ARP_OFFLOAD%
HKR, Ndi\Params\*PMARPOffload\Enum,             "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMARPOffload\Enum,             "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMARPOffload,                  type,       0, "enum"
HKR, Ndi\Params\*PMARPOffload,                  default,    0, "1"
HKR, Ndi\Params\*PMNSOffload,                   ParamDesc,  0, %PM_NS_OFFLOAD%
HKR, Ndi\Params\*PMNSOffload\Enum,              "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMNSOffload\Enum,              "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMNSOffload,                   type,       0, "enum"
HKR, Ndi\Params\*PMNSOffload,                   default,    0, "1"
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       ParamDesc,  0, %DEVICE_SLEEP_ON_DISCONNECT%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       type,       0, "enum"
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       default,    0, "0"
HKR, Ndi\Params\MIMOPowerSaveMode,              ParamDesc,  0, %MIMO_POWER_SAVE_MODE_STR%
HKR, Ndi\Params\MIMOPowerSaveMode,              Type,       2, "enum"
HKR, Ndi\Params\MIMOPowerSaveMode,              Default,    2, "0"
HKR, Ndi\Params\MIMOPowerSaveMode,              Optional,   2, "0"
HKR, Ndi\Params\MIMOPowerSaveMode\enum,         "0",        0, %MIMO_AUTO_STR%
HKR, Ndi\Params\MIMOPowerSaveMode\enum,         "1",        0, %NO_MIMO_STR%
HKR, Ndi\Params\MIMOPowerSaveMode\enum,         "2",        0, %RTS_BEFORE_MIMO_STR%
HKR, Ndi\Params\MIMOPowerSaveMode\enum,         "3",        0, %NO_RTS_BEFORE_MIMO_STR%



[Reg_NDI_2x2]
HKR, Ndi\Params\*PacketCoalescing,              ParamDesc,  0, %PACKET_COALESCING%
HKR, Ndi\Params\*PacketCoalescing,              type,       0, "enum"
HKR, Ndi\Params\*PacketCoalescing,              default,    0, "1"
HKR, Ndi\Params\*PacketCoalescing\Enum,         "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PacketCoalescing\Enum,         "1",        0, %ENABLED_STR%



[Reg_NDI_INT_WDI]
HKR, Ndi\Interfaces,                            UpperRange, 0, "ndis5,wifipro,intel_psm"
HKR, Ndi\Interfaces,                            LowerRange, 0, "ethernet,wlan,vwifi"
HKR, Ndi,                                       Service,    0, "Netwtw08."



[Reg_Common_WPP]
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession, Start, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7D55FE6F-EAC4-49DA-8F47-CC7B4EF3F172}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{04835337-59F0-4ED5-B552-8DBD0E528FD9}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6AE0AA38-F827-46C0-8C4C-A32ABF4C175D}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{71BC4141-CF9B-4B85-815B-7891424F9DE8}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{13F911C5-F20B-44B7-91D1-3B4A926EC3EE}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DE877B6F-712B-42A6-A06D-F10BF9B8BB8C}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{0FACA5CB-6060-457E-B228-D12F0E4D280A}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6B71976C-97EF-4946-861A-B00994DE0939}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6B71976C-97EF-4946-861A-B00994DE0939}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6B71976C-97EF-4946-861A-B00994DE0939}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{6B71976C-97EF-4946-861A-B00994DE0939}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{7A6E6362-F70A-456A-B765-ECB98E5C63C7}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3845FDE5-2F2B-43AA-B78B-742B6364A2EC}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FB2CF4C2-1FC9-4D49-901A-60B426C4A7A6}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FF730A61-F14F-4F4A-9FEF-D5222F169737}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{ECC34691-A263-43AF-8863-CBD383025D11}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{ECC34691-A263-43AF-8863-CBD383025D11}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{ECC34691-A263-43AF-8863-CBD383025D11}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{ECC34691-A263-43AF-8863-CBD383025D11}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4E6E67D4-B87A-4654-818F-DE5C7CA11A04}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DCAC780D-2DB2-43FD-95EF-F2F01B250530}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{460722B7-0C89-48D1-997D-DC352D990BCB}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{45A06657-5750-47CE-A2AB-D9EFC89C7932}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{030049D6-0C86-47AA-91A7-4E1DD52CF571}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{67DD83E2-051D-4D07-A6A0-0AF726C02163}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{FA2456C4-85C1-487B-92E8-461567A70D57}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{939365A8-3771-4791-A0CE-D542EAC1B2EA}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, EnableFlags, 0x00010001, 0x1fff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B24C5278-100A-49E0-9133-D0987DA71DE3}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{EC3F4BF1-E2E6-4EBB-937F-ABB22A7568CB}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{B1C6A36E-49F8-480F-9C41-ABA3E6CF7635}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C94F476-91B0-4F22-8687-925C2DA5FB49}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{431BACD7-33F3-410E-B6DD-54FE6C6AB4C9}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, EnableFlags, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{19A34C92-CB6D-46BC-AE0E-9983C966BE86}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E7AD1A85-B112-418C-8BC5-D75B3D6C4330}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{61AEF8A0-878B-46CA-87F6-64E7D58A2A95}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E14EA266-FA36-415A-83ED-7482BC8D8EC7}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{4D9C3E2F-5ED3-4DE7-83D1-FC2061AC7D01}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{794E231D-349E-4CD0-AAD5-D067B01C7F07}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{411C4950-F958-4068-BABD-A197472DD6F0}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{411C4950-F958-4068-BABD-A197472DD6F0}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{411C4950-F958-4068-BABD-A197472DD6F0}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{411C4950-F958-4068-BABD-A197472DD6F0}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3C83EFD6-AF5E-4D99-A04B-9F526A6D6412}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E6FEA6FF-E9D6-4A73-8F35-35B426C5584B}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{3540DA01-6900-4A5B-A384-6A004DE4C5B4}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{E05B9662-F9E7-4338-89A5-C54815C82791}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{64B45C89-E5A7-4AC5-ACD4-0C638584BFD6}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{D18B1F60-D9C4-4E0B-813F-781FDCFF04E6}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{DFC96C3D-045C-4C09-8670-00782F09CDD9}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{A9ED464B-4A32-4585-A27C-CB5ED464EC29}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{91270A90-13CC-45C3-8D64-108876E7302C}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{91270A90-13CC-45C3-8D64-108876E7302C}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{91270A90-13CC-45C3-8D64-108876E7302C}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{91270A90-13CC-45C3-8D64-108876E7302C}, Status, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, EnableFlags, 0x00010001, 0xffff
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\WifiDriverIHVSession\{2B5E730B-9A6C-492A-B8DB-0E3B1B0EC064}, Status, 0x00010001, 0x0



[Reg_NIC_9260_2x2_AC]
HKR,,AdapterModel,0,%NIC_9260_2x2_AC%
HKR,,DriverDesc,0,%NIC_9260_2x2_AC%



[Reg_NIC_9260_2x2_AC_no_160]
HKR,,AdapterModel,0,%NIC_9260_2x2_AC_no_160%
HKR,,DriverDesc,0,%NIC_9260_2x2_AC_no_160%



[Reg_NIC_1550_2x2_AC]
HKR,,AdapterModel,0,%NIC_1550_2x2_AC%
HKR,,DriverDesc,0,%NIC_1550_2x2_AC%



[Strings]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Intel(R) Wireless Adapter Driver for Windows 10 - 64 Bit"
RECOMMENDED_CHANNEL24_STR    = "Ad Hoc Channel 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Ad Hoc Channel 802.11a"
RECOMMENDED_BAND             = "Ad Hoc Default Wireless Mode"
IBSS_TX_POWER_STR            = "Transmit Power"
ROAMING_AGGRESSIVENESS_STR   = "Roaming Aggressiveness"
ADHOC_POWER_MANAGEMENT_STR   = "Ad Hoc Power Management"
ADHOC_QOS_MODE_STR           = "Ad Hoc QoS Mode"
MIXED_MODE_PROTECTION_STR    = "Mixed Mode Protection"
THROUGHPUT_ENHANCEMENT_STR   = "Throughput Enhancement"
WIRELESS_MODE_STR            = "802.11a/b/g Wireless Mode"
WIRELESS_MODE_A              = "5GHz  802.11a"
WIRELESS_MODE_B              = "2.4GHz 802.11b"
WIRELESS_MODE_G              = "2.4GHz 802.11g"
WIRELESS_MODE_BG             = "2.4GHz 802.11b/g"
WIRELESS_MODE_AG             = "Dual Band 802.11a/g"
WIRELESS_MODE_ABG            = "Dual Band 802.11a/b/g"
PREFERRED_BAND_STR           = "Preferred Band"
CHANNELWIDTH6                = "Channel Width for 6GHz"
CHANNELWIDTH52               = "Channel Width for 5GHz"
CHANNELWIDTH24               = "Channel Width for 2.4GHz"
TGnMode                      = "802.11n Wireless Mode"
11N_AC_MODE                  = "802.11n/ac Wireless Mode"
11N_AX_MODE                  = "802.11n/ac/ax Wireless Mode"
11N_BE_MODE                  = "802.11n/ac/ax/be Wireless Mode"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Fat Channel Intolerant"
LOWEST_STR                   = "Lowest"
MEDIUM_LOW_STR               = "Medium-low"
MEDIUM_STR                   = "Medium"
MEDIUM_HIGH_STR              = "Medium-High"
HIGHEST_STR                  = "Highest"
DISABLED_STR                 = "Disabled"
ENABLED_STR                  = "Enabled"
MAXIMUM_POWER_SAVING_STR     = "Maximum Power Savings"
NOISY_ENVIRONMENT_STR        = "Noisy Environment"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "CTS-to-self Enabled"
RTS_CTS_ENABLED_STR          = "RTS/CTS Enabled"
AUTO_STR                     = "Auto"
CHANNELWIDTH20ONLY           = "20 MHz Only"
CHANNELWIDTHAUTO             = "Auto"
WMM_DISABLED_STR             = "WMM Disabled"
WMM_ENABLED_STR              = "WMM Enabled"
NO_PREFERECE_STR             = "No Preference"
PREFER_24_BAND_STR           = "Prefer 2.4GHz band"
PREFER_52_BAND_STR           = "Prefer 5GHz band"
PREFER_6_BAND_STR            = "Prefer 6GHz band"
PREFER_52_6_BAND_STR         = "Prefer 5GHz + 6GHz band"
WAKE_ON_MAGIC_PACKET         = "Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH        = "Wake on Pattern Match"
PM_WIFI_REKEY_OFFLOAD        = "GTK rekeying for WoWLAN"
PM_ARP_OFFLOAD               = "ARP offload for WoWLAN"
PM_NS_OFFLOAD                = "NS offload for WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Sleep on WoWLAN Disconnect"
PACKET_COALESCING            = "Packet Coalescing"
U_APSD_SUPPORT               = "U-APSD support"
THROUGHPUTBOOSTER_STR        = "Throughput Booster"
MIMO_POWER_SAVE_MODE_STR     = "MIMO Power Save Mode"
MIMO_AUTO_STR                = "Auto SMPS"
NO_MIMO_STR                  = "Static SMPS"
RTS_BEFORE_MIMO_STR          = "Dynamic SMPS"
NO_RTS_BEFORE_MIMO_STR       = "No SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "Double Connect Technology"
SOURCEDISK1                  = "Intel(R) Wireless Install Disk"
UHB_BAND_SUPPORTED_STR       = "Ultra High Band (6GHz)"
HUMAN_PRESENCE_DETECTION_STR = "Human Presence Detection"

; Arabic (Saudi Arabia)
NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"
[Strings.0401]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "برنامج تشغيل محول Intel(R) Wireless لنظام Windows 10 64 Bit"
RECOMMENDED_CHANNEL24_STR    = "قناة الأقران 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "قناة الأقران 802.11a"
RECOMMENDED_BAND             = "وضع اللاسلكي الافتراضي للأقران"
IBSS_TX_POWER_STR            = "طاقة الإرسال"
ROAMING_AGGRESSIVENESS_STR   = "نشاط التجوال"
ADHOC_POWER_MANAGEMENT_STR   = "إدارة طاقة الأقران"
ADHOC_QOS_MODE_STR           = "الوضع QoS للأقران"
MIXED_MODE_PROTECTION_STR    = "حماية الوضع المختلط"
THROUGHPUT_ENHANCEMENT_STR   = "تحسين الخرج"
WIRELESS_MODE_STR            = "الوضع اللاسلكي 802.11a/b/g"
WIRELESS_MODE_A              = "5 جيجاهرتز 802.11a"
WIRELESS_MODE_B              = "2.4  جيجاهرتز 802.11b"
WIRELESS_MODE_G              = "2.4  جيجاهرتز 802.11g"
WIRELESS_MODE_BG             = "2.4 جيجاهرتز 802.11b/g"
WIRELESS_MODE_AG             = "نطاق مزدوج 802.11a/g"
WIRELESS_MODE_ABG            = "نطاق مزدوج 802.11a/b/g"
PREFERRED_BAND_STR           = "مدى الموجات المفضل"
CHANNELWIDTH52               = "عرض القناة للّتردد 5 غيغاهرتز"
CHANNELWIDTH6                = "عرض القناة للّتردد 6 غيغاهرتز"
CHANNELWIDTH24               = "عرض القناة للّتردد 2.4 غيغاهرتز"
TGnMode                      = "الوضع اللاسلكي 802.11n"
11N_AC_MODE                  = "الوضع اللاسلكي 802.11n/ac"
11N_AX_MODE                  = "الوضع اللاسلكي 802.11n/ac/ax"
11N_BE_MODE                  = "الوضع اللاسلكي 802.11n/ac/ax/be"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "غير متوافق مع قناة 40 ميجاهيرتز"
LOWEST_STR                   = "الأدنى"
MEDIUM_LOW_STR               = "متوسط-منخفض"
MEDIUM_STR                   = "متوسط"
MEDIUM_HIGH_STR              = "متوسط-مرتفع"
HIGHEST_STR                  = "الأعلى"
DISABLED_STR                 = "معطل"
ENABLED_STR                  = "ممكَّن"
MAXIMUM_POWER_SAVING_STR     = "أقصى توفير للطاقة"
NOISY_ENVIRONMENT_STR        = "بيئة الضوضاء"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "تمكين CTS الذاتي"
RTS_CTS_ENABLED_STR          = "تمكين RTS/CTS"
AUTO_STR                     = "تلقائي"
CHANNELWIDTH20ONLY           = "20 ميجاهيرتز"
CHANNELWIDTHAUTO             = "تلقائي"
WMM_DISABLED_STR             = "WMM معطل"
WMM_ENABLED_STR              = "WMM ممكَّن"
NO_PREFERECE_STR             = "بلا تفضيل"
PREFER_24_BAND_STR           = "يفضل مدى موجات 2.4 جيجاهيرتز"
PREFER_52_BAND_STR           = "أفضّل مدى موجات 5 جيجاهرتز"
PREFER_6_BAND_STR            = "أفضّل مدى موجات 6 جيجاهرتز"
PREFER_52_6_BAND_STR         = "أفضّل نطاق 5 غيغاهرتز + 6 غيغاهرتز"
WAKE_ON_MAGIC_PACKET         = "التنبيه عند الحزمة السحرية"
WAKE_ON_PATTERN_MATCH        = "التنبيه عند مطابقة النقش"
PM_WIFI_REKEY_OFFLOAD        = "إعادة إنشاء مفتاح GTK لتنبيه WLAN"
PM_ARP_OFFLOAD               = "توزيع نقل البيانات باستخدام ARP لتنبيه WLAN"
PM_NS_OFFLOAD                = "توزيع نقل البيانات باستخدام NS لتنبيه WLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "السكون عند فصل تنبيه WLAN"
PACKET_COALESCING            = "إدماج الحزمة"
U_APSD_SUPPORT               = "دعم U-APSD"
THROUGHPUTBOOSTER_STR        = "معزز معدل النقل"
MIMO_POWER_SAVE_MODE_STR     = "وضع توفير الطاقة لـ MIMO"
MIMO_AUTO_STR                = "SMPS التلقائي"
NO_MIMO_STR                  = "SMPS الثابت"
RTS_BEFORE_MIMO_STR          = "SMPS الديناميكي"
NO_RTS_BEFORE_MIMO_STR       = "ما من SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "تقنية الاتصال الثنائي"
SOURCEDISK1                  = "قرص تثبيت مجموعة Intel(R) Wireless"
UHB_BAND_SUPPORTED_STR       = "نطاق مرتفع للغاية (6 غيغاهرتز)"
HUMAN_PRESENCE_DETECTION_STR = "اكتشاف وجود بشري"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Chinese (Simplified)
[Strings.0804]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Intel(R) Wireless 适配器驱动程序（适用于 Windows 10 64 位）"
RECOMMENDED_CHANNEL24_STR    = "Ad Hoc 信道 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Ad Hoc 信道 802.11a"
RECOMMENDED_BAND             = "Ad Hoc 默认无线模式"
IBSS_TX_POWER_STR            = "传输电源"
ROAMING_AGGRESSIVENESS_STR   = "漫游主动性"
ADHOC_POWER_MANAGEMENT_STR   = "Ad Hoc 电源管理"
ADHOC_QOS_MODE_STR           = "Ad Hoc QoS 模式"
MIXED_MODE_PROTECTION_STR    = "混合模式保护"
THROUGHPUT_ENHANCEMENT_STR   = "吞吐量增强"
WIRELESS_MODE_STR            = "802.11a/b/g 无线模式"
WIRELESS_MODE_A              = "5GHz 802.11a"
WIRELESS_MODE_B              = "2.4GHz 802.11b"
WIRELESS_MODE_G              = "2.4GHz 802.11g"
WIRELESS_MODE_BG             = "2.4GHz 802.11b/g"
WIRELESS_MODE_AG             = "双频带 802.11a/g"
WIRELESS_MODE_ABG            = "双频带 802.11a/b/g"
PREFERRED_BAND_STR           = "首选频带"
CHANNELWIDTH52               = "5GHz 信道宽度"
CHANNELWIDTH6                = "6GHz 信道宽度"
CHANNELWIDTH24               = "2.4GHz 信道宽度"
TGnMode                      = "802.11n 无线模式"
11N_AC_MODE                  = "802.11n/ac 无线模式"
11N_AX_MODE                  = "802.11n/ac/ax 无线模式"
11N_BE_MODE                  = "802.11n/ac/ax/be 无线模式"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "与 40Mhz 信道不兼容"
LOWEST_STR                   = "最低值"
MEDIUM_LOW_STR               = "中低"
MEDIUM_STR                   = "中间"
MEDIUM_HIGH_STR              = "中高"
HIGHEST_STR                  = "最高值"
DISABLED_STR                 = "已禁用"
ENABLED_STR                  = "已启用"
MAXIMUM_POWER_SAVING_STR     = "最大节能"
NOISY_ENVIRONMENT_STR        = "嘈杂环境"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "CTS-to-self 已启用"
RTS_CTS_ENABLED_STR          = "RTS/CTS 已启用"
AUTO_STR                     = "自动"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "自动"
WMM_DISABLED_STR             = "WMM 已禁用"
WMM_ENABLED_STR              = "WMM 已启用"
NO_PREFERECE_STR             = "无首选项"
PREFER_24_BAND_STR           = "首选 2.4 GHz 频带"
PREFER_52_BAND_STR           = "首选 5GHz 频带"
PREFER_6_BAND_STR            = "首选 6GHz 频带"
PREFER_52_6_BAND_STR         = "首选 5 GHz + 6 GHz 频带"
WAKE_ON_MAGIC_PACKET         = "唤醒幻数据包"
WAKE_ON_PATTERN_MATCH        = "唤醒模式匹配"
PM_WIFI_REKEY_OFFLOAD        = "WoWLAN 的 GTK 重新生成密钥"
PM_ARP_OFFLOAD               = "WoWLAN 的 ARP 卸载"
PM_NS_OFFLOAD                = "WoWLAN 的 NS 卸载"
DEVICE_SLEEP_ON_DISCONNECT   = "WoWLAN 断开连接时睡眠"
PACKET_COALESCING            = "数据包合并"
U_APSD_SUPPORT               = "支持 U-APSD "
THROUGHPUTBOOSTER_STR        = "吞吐量助推器"
MIMO_POWER_SAVE_MODE_STR     = "MIMO 节能模式"
MIMO_AUTO_STR                = "自动 SMPS"
NO_MIMO_STR                  = "静态 SMPS"
RTS_BEFORE_MIMO_STR          = "动态 SMPS"
NO_RTS_BEFORE_MIMO_STR       = "无 SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "双连接技术"
SOURCEDISK1                  = "Intel(R) Wireless 系列安装盘"
UHB_BAND_SUPPORTED_STR       = "超高频段 (6GHz)"
HUMAN_PRESENCE_DETECTION_STR = "用户存在检测"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Chinese (Traditional)
[Strings.0404]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "用於 Windows 10 64 Bit 的 Intel(R) Wireless 介面卡驅動程式"
RECOMMENDED_CHANNEL24_STR    = "點對點 (ad hoc) 通道 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "點對點 (ad hoc) 通道 802.11a"
RECOMMENDED_BAND             = "點對點 (ad hoc) 預設無線模式"
IBSS_TX_POWER_STR            = "傳輸電源"
ROAMING_AGGRESSIVENESS_STR   = "漫遊積極度"
ADHOC_POWER_MANAGEMENT_STR   = "點對點 (ad hoc) 電源管理"
ADHOC_QOS_MODE_STR           = "點對點 (ad hoc) QoS 模式"
MIXED_MODE_PROTECTION_STR    = "混合模式保護"
THROUGHPUT_ENHANCEMENT_STR   = "輸送量增強功能"
WIRELESS_MODE_STR            = "802.11a/b/g 無線模式"
WIRELESS_MODE_A              = "5GHz 802.11a"
WIRELESS_MODE_B              = "2.4GHz 802.11b"
WIRELESS_MODE_G              = "2.4GHz 802.11g"
WIRELESS_MODE_BG             = "2.4GHz 802.11b/g"
WIRELESS_MODE_AG             = "雙頻 802.11a/g"
WIRELESS_MODE_ABG            = "雙頻 802.11a/b/g"
PREFERRED_BAND_STR           = "偏好的頻帶"
CHANNELWIDTH52               = "5GHz 的通道寬度"
CHANNELWIDTH6                = "6GHz 的通道寬度"
CHANNELWIDTH24               = "2.4GHz 的通道寬度"
TGnMode                      = "802.11n 無線模式"
11N_AC_MODE                  = "802.11n/ac 無線模式"
11N_AX_MODE                  = "802.11n/ac/ax 無線模式"
11N_BE_MODE                  = "802.11n/ac/ax/be 無線模式"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "不容大量通道"
LOWEST_STR                   = "最低"
MEDIUM_LOW_STR               = "中低"
MEDIUM_STR                   = "中"
MEDIUM_HIGH_STR              = "中高"
HIGHEST_STR                  = "最高"
DISABLED_STR                 = "停用"
ENABLED_STR                  = "啟用"
MAXIMUM_POWER_SAVING_STR     = "最省電"
NOISY_ENVIRONMENT_STR        = "噪音環境"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "啟用 CTS-to-self"
RTS_CTS_ENABLED_STR          = "啟用 RTS/CTS"
AUTO_STR                     = "自動"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "自動"
WMM_DISABLED_STR             = "WMM 停用"
WMM_ENABLED_STR              = "WMM 啟用"
NO_PREFERECE_STR             = "無偏好設定"
PREFER_24_BAND_STR           = "喜好 2.4 GHz 頻帶"
PREFER_52_BAND_STR           = "偏好 5GHz 頻帶"
PREFER_6_BAND_STR            = "偏好 6GHz 頻帶"
PREFER_52_6_BAND_STR         = "偏好 5 GHz + 6 GHz 頻段"
WAKE_ON_MAGIC_PACKET         = "收到 Magic 封包時喚醒"
WAKE_ON_PATTERN_MATCH        = "收到模式對應時喚醒"
PM_WIFI_REKEY_OFFLOAD        = "WoWLAN GTK 金鑰重建"
PM_ARP_OFFLOAD               = "WoWLAN ARP 卸載"
PM_NS_OFFLOAD                = "WoWLAN NS 卸載"
DEVICE_SLEEP_ON_DISCONNECT   = "WoWLAN 中斷連線時睡眠"
PACKET_COALESCING            = "封包聯合"
U_APSD_SUPPORT               = "U-APSD 支援"
THROUGHPUTBOOSTER_STR        = "傳輸加速"
MIMO_POWER_SAVE_MODE_STR     = "MIMO 省電模式"
MIMO_AUTO_STR                = "自動 SMPS"
NO_MIMO_STR                  = "靜態 SMPS"
RTS_BEFORE_MIMO_STR          = "動態 SMPS"
NO_RTS_BEFORE_MIMO_STR       = "無 SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "雙連線技術"
SOURCEDISK1                  = "Intel(R) Wireless 系列安裝磁碟"
UHB_BAND_SUPPORTED_STR       = "超高頻 (6GHz)"
HUMAN_PRESENCE_DETECTION_STR = "使用者在場偵測"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"
 ; Chinese (Traditional)

; Chinese (Hong Kong)
[Strings.0C04]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "用於 Windows 10 64 Bit 的 Intel(R) Wireless 介面卡驅動程式"
RECOMMENDED_CHANNEL24_STR    = "點對點 (ad hoc) 通道 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "點對點 (ad hoc) 通道 802.11a"
RECOMMENDED_BAND             = "點對點 (ad hoc) 預設無線模式"
IBSS_TX_POWER_STR            = "傳輸電源"
ROAMING_AGGRESSIVENESS_STR   = "漫遊積極度"
ADHOC_POWER_MANAGEMENT_STR   = "點對點 (ad hoc) 電源管理"
ADHOC_QOS_MODE_STR           = "點對點 (ad hoc) QoS 模式"
MIXED_MODE_PROTECTION_STR    = "混合模式保護"
THROUGHPUT_ENHANCEMENT_STR   = "輸送量增強功能"
WIRELESS_MODE_STR            = "802.11a/b/g 無線模式"
WIRELESS_MODE_A              = "5GHz 802.11a"
WIRELESS_MODE_B              = "2.4GHz 802.11b"
WIRELESS_MODE_G              = "2.4GHz 802.11g"
WIRELESS_MODE_BG             = "2.4GHz 802.11b/g"
WIRELESS_MODE_AG             = "雙頻 802.11a/g"
WIRELESS_MODE_ABG            = "雙頻 802.11a/b/g"
PREFERRED_BAND_STR           = "偏好的頻帶"
CHANNELWIDTH52               = "5GHz 的通道寬度"
CHANNELWIDTH6                = "6GHz 的通道寬度"
CHANNELWIDTH24               = "2.4GHz 的通道寬度"
TGnMode                      = "802.11n 無線模式"
11N_AC_MODE                  = "802.11n/ac 無線模式"
11N_AX_MODE                  = "802.11n/ac/ax 無線模式"
11N_BE_MODE                  = "802.11n/ac/ax/be 無線模式"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "不容大量通道"
LOWEST_STR                   = "最低"
MEDIUM_LOW_STR               = "中低"
MEDIUM_STR                   = "中"
MEDIUM_HIGH_STR              = "中高"
HIGHEST_STR                  = "最高"
DISABLED_STR                 = "停用"
ENABLED_STR                  = "啟用"
MAXIMUM_POWER_SAVING_STR     = "最省電"
NOISY_ENVIRONMENT_STR        = "噪音環境"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "啟用 CTS-to-self"
RTS_CTS_ENABLED_STR          = "啟用 RTS/CTS"
AUTO_STR                     = "自動"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "自動"
WMM_DISABLED_STR             = "WMM 停用"
WMM_ENABLED_STR              = "WMM 啟用"
NO_PREFERECE_STR             = "無偏好設定"
PREFER_24_BAND_STR           = "喜好 2.4 GHz 頻帶"
PREFER_52_BAND_STR           = "偏好 5GHz 頻帶"
PREFER_6_BAND_STR            = "偏好 6GHz 頻帶"
PREFER_52_6_BAND_STR         = "偏好 5 GHz + 6 GHz 頻段"
WAKE_ON_MAGIC_PACKET         = "收到 Magic 封包時喚醒"
WAKE_ON_PATTERN_MATCH        = "收到模式對應時喚醒"
PM_WIFI_REKEY_OFFLOAD        = "WoWLAN GTK 金鑰重建"
PM_ARP_OFFLOAD               = "WoWLAN ARP 卸載"
PM_NS_OFFLOAD                = "WoWLAN NS 卸載"
DEVICE_SLEEP_ON_DISCONNECT   = "WoWLAN 中斷連線時睡眠"
PACKET_COALESCING            = "封包聯合"
U_APSD_SUPPORT               = "U-APSD 支援"
THROUGHPUTBOOSTER_STR        = "傳輸加速"
MIMO_POWER_SAVE_MODE_STR     = "MIMO 省電模式"
MIMO_AUTO_STR                = "自動 SMPS"
NO_MIMO_STR                  = "靜態 SMPS"
RTS_BEFORE_MIMO_STR          = "動態 SMPS"
NO_RTS_BEFORE_MIMO_STR       = "無 SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "雙連線技術"
SOURCEDISK1                  = "Intel(R) Wireless 系列安裝磁碟"
UHB_BAND_SUPPORTED_STR       = "超高頻 (6GHz)"
HUMAN_PRESENCE_DETECTION_STR = "使用者在場偵測"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Czech (Czechia)
[Strings.0405]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Ovladač adaptéru Intel(R) Wireless pro systém Windows 10 64 Bit"
RECOMMENDED_CHANNEL24_STR    = "Kanál ad hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Kanál ad hoc 802.11a"
RECOMMENDED_BAND             = "Výchozí bezdrátový režim ad hoc"
IBSS_TX_POWER_STR            = "Vysílací energie"
ROAMING_AGGRESSIVENESS_STR   = "Agresivita roamingu"
ADHOC_POWER_MANAGEMENT_STR   = "Správa napájení ad hoc"
ADHOC_QOS_MODE_STR           = "Režim Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR    = "Ochrana smíšeného režimu"
THROUGHPUT_ENHANCEMENT_STR   = "Zlepšení propustnosti"
WIRELESS_MODE_STR            = "Bezdrátový režim 802.11a/b/g"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2,4 GHz 802.11b"
WIRELESS_MODE_G              = "2,4 GHz 802.11g"
WIRELESS_MODE_BG             = "2,4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Dual Band 802.11a/g"
WIRELESS_MODE_ABG            = "Dual Band 802.11a/b/g"
PREFERRED_BAND_STR           = "Upřednostňované pásmo"
CHANNELWIDTH52               = "Šířka kanálu pro 5 GHz"
CHANNELWIDTH6                = "Šířka kanálu pro 6 GHz"
CHANNELWIDTH24               = "Šířka kanálu pro 2,4 GHz"
TGnMode                      = "Bezdrátový režim 802.11n"
11N_AC_MODE                  = "Bezdrátový režim 802.11n/ac"
11N_AX_MODE                  = "Bezdrátový režim 802.11n/ac/ax"
11N_BE_MODE                  = "Bezdrátový režim 802.11n/ac/ax/be"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Nekompatibilní s šířkou kanálu 40 MHz"
LOWEST_STR                   = "Nejnižší"
MEDIUM_LOW_STR               = "Středně nízký"
MEDIUM_STR                   = "Střední"
MEDIUM_HIGH_STR              = "Středně vysoký"
HIGHEST_STR                  = "Nejvyšší"
DISABLED_STR                 = "Zakázáno"
ENABLED_STR                  = "Povoleno"
MAXIMUM_POWER_SAVING_STR     = "Maximální úspora energie"
NOISY_ENVIRONMENT_STR        = "Prostředí s velkým šumem"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "CTS-to-self povoleno"
RTS_CTS_ENABLED_STR          = "RTS/CTS povoleno"
AUTO_STR                     = "Automaticky"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "Automaticky"
WMM_DISABLED_STR             = "WMM zakázáno"
WMM_ENABLED_STR              = "WMM povoleno"
NO_PREFERECE_STR             = "Žádná předvolba"
PREFER_24_BAND_STR           = "Upřednostňovat pásmo 2,4 GHz"
PREFER_52_BAND_STR           = "Dát přednost pásmu 5 GHz"
PREFER_6_BAND_STR            = "Dát přednost pásmu 6 GHz"
PREFER_52_6_BAND_STR         = "Dát přednost pásmům 5 GHz a 6 GHz"
WAKE_ON_MAGIC_PACKET         = "Probuzení paketem Magic"
WAKE_ON_PATTERN_MATCH        = "Probuzení porovnávacím vzorkem"
PM_WIFI_REKEY_OFFLOAD        = "Vystavování nových klíčů GTK pro technologii WoWLAN"
PM_ARP_OFFLOAD               = "Snižování zatížení ARP pro technologii WoWLAN"
PM_NS_OFFLOAD                = "Snižování zatížení NS pro technologii WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Režim spánku při odpojení technologie WoWLAN"
PACKET_COALESCING            = "Slučování paketů"
U_APSD_SUPPORT               = "Podpora U-APSD"
THROUGHPUTBOOSTER_STR        = "Podpora průchodnosti"
MIMO_POWER_SAVE_MODE_STR     = "Režim úspory energie MIMO"
MIMO_AUTO_STR                = "Automatický režim SMPS"
NO_MIMO_STR                  = "Statický režim SMPS"
RTS_BEFORE_MIMO_STR          = "Dynamický režim SMPS"
NO_RTS_BEFORE_MIMO_STR       = "Žádný režim SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "Technologie Double Connect"
SOURCEDISK1                  = "Instalační disk adaptéru řady Intel(R) Wireless"
UHB_BAND_SUPPORTED_STR       = "Ultravysoké pásmo (6 GHz)"
HUMAN_PRESENCE_DETECTION_STR = "Detekce přítomnosti člověka"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Danish (Denmark)
[Strings.0406]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Intel(R) Wireless adapter driver til Windows 10 64 Bit"
RECOMMENDED_CHANNEL24_STR    = "Ad hoc-kanal 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Ad hoc-kanal 802.11a"
RECOMMENDED_BAND             = "Ad hoc standard trådløs tilstand"
IBSS_TX_POWER_STR            = "Sendeeffekt"
ROAMING_AGGRESSIVENESS_STR   = "Roaming-aggressivitet"
ADHOC_POWER_MANAGEMENT_STR   = "Ad Hoc-strømstyring"
ADHOC_QOS_MODE_STR           = "Ad Hoc QoS-tilstand"
MIXED_MODE_PROTECTION_STR    = "Beskyttelse til blandet miljø"
THROUGHPUT_ENHANCEMENT_STR   = "Forbedring af ydelse"
WIRELESS_MODE_STR            = "802.11a/b/g trådløs tilstand"
WIRELESS_MODE_A              = "5GHz 802.11a"
WIRELESS_MODE_B              = "2,4GHz 802.11b"
WIRELESS_MODE_G              = "2,4GHz 802.11g"
WIRELESS_MODE_BG             = "2,4GHz 802.11b/g"
WIRELESS_MODE_AG             = "Dual Band 802.11a/g"
WIRELESS_MODE_ABG            = "Dual Band 802.11a/b/g"
PREFERRED_BAND_STR           = "Foretrukket bånd"
CHANNELWIDTH52               = "Kanalbredde for 5 GHz"
CHANNELWIDTH6                = "Kanalbredde for 6 GHz"
CHANNELWIDTH24               = "Kanalbredde for 2,4 GHz"
TGnMode                      = "802.11n trådløs tilstand"
11N_AC_MODE                  = "802.11n/ac trådløs tilstand"
11N_AX_MODE                  = "802.11n/ac/ax trådløs tilstand"
11N_BE_MODE                  = "802.11n/ac/ax/be trådløs tilstand"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "40Mhz kanal intolerant"
LOWEST_STR                   = "Laveste"
MEDIUM_LOW_STR               = "Mellem-lav"
MEDIUM_STR                   = "Mellem"
MEDIUM_HIGH_STR              = "Mellem-høj"
HIGHEST_STR                  = "Højeste"
DISABLED_STR                 = "Deaktiveret"
ENABLED_STR                  = "Aktiveret"
MAXIMUM_POWER_SAVING_STR     = "Maks. strømbesparelse"
NOISY_ENVIRONMENT_STR        = "Støjfyldt miljø"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "CTS-to-self aktiveret "
RTS_CTS_ENABLED_STR          = "RTS/CTS aktiveret "
AUTO_STR                     = "Auto"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "Auto"
WMM_DISABLED_STR             = "WMM deaktiveret"
WMM_ENABLED_STR              = "WMM aktiveret"
NO_PREFERECE_STR             = "Ingen indstilling"
PREFER_24_BAND_STR           = "Foretræk 2,4 GHz bånd"
PREFER_52_BAND_STR           = "Foretræk 5GHz-båndet"
PREFER_6_BAND_STR            = "Foretræk 6GHz-båndet"
PREFER_52_6_BAND_STR         = "Foretræk 5 GHz- og 6 GHz-båndet"
WAKE_ON_MAGIC_PACKET         = "Vækning ved magisk pakke"
WAKE_ON_PATTERN_MATCH        = "Vækning ved mønstermatch"
PM_WIFI_REKEY_OFFLOAD        = "GTK-nøglefornyelse til WoWLAN"
PM_ARP_OFFLOAD               = "ARP-aflastning til WoWLAN"
PM_NS_OFFLOAD                = "NS-aflastning til WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Slumring ved afbrydelse af WoWLAN"
PACKET_COALESCING            = "Pakke-samling"
U_APSD_SUPPORT               = "U-APSD Support"
THROUGHPUTBOOSTER_STR        = "Gennemløbsforstærker"
MIMO_POWER_SAVE_MODE_STR     = "MIMO-strømsparetilstand"
MIMO_AUTO_STR                = "Auto-SMPS"
NO_MIMO_STR                  = "Statisk SMPS"
RTS_BEFORE_MIMO_STR          = "Dynamisk SMPS"
NO_RTS_BEFORE_MIMO_STR       = "Ingen SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "Dobbelt forbindelse teknologi"
SOURCEDISK1                  = "Intel(R) Wireless installationsdisk"
UHB_BAND_SUPPORTED_STR       = "Ultrahøjt bånd (6 GHz)"
HUMAN_PRESENCE_DETECTION_STR = "Registrering af menneskelig tilstedeværelse"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; German (Germany)
[Strings.0407]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Intel(R) Wireless Adaptertreiber für Windows 10 64-Bit"
RECOMMENDED_CHANNEL24_STR    = "Ad-Hoc-Kanal 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Ad-Hoc-Kanal 802.11a"
RECOMMENDED_BAND             = "Ad-hoc Standard-WLAN-Modus"
IBSS_TX_POWER_STR            = "Übertragungsleistung"
ROAMING_AGGRESSIVENESS_STR   = "Roaming-Dynamik"
ADHOC_POWER_MANAGEMENT_STR   = "Ad-Hoc-Energieverwaltung"
ADHOC_QOS_MODE_STR           = "Ad-Hoc QoS-Modus"
MIXED_MODE_PROTECTION_STR    = "Schutz f. gemischte Umgebungen"
THROUGHPUT_ENHANCEMENT_STR   = "Durchsatzverbesserung"
WIRELESS_MODE_STR            = "Wireless-Modus 802.11a/b/g"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2,4 GHz 802.11b"
WIRELESS_MODE_G              = "2,4 GHz 802.11g"
WIRELESS_MODE_BG             = "2,4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Dual Band 802.11a/g"
WIRELESS_MODE_ABG            = "Dual Band 802.11a/b/g"
PREFERRED_BAND_STR           = "Bevorzugtes Band"
CHANNELWIDTH52               = "Kanalbreite für 5 GHz"
CHANNELWIDTH6                = "Kanalbreite für 6 GHz"
CHANNELWIDTH24               = "Kanalbreite für 2,4 GHz"
TGnMode                      = "Wireless-Modus 802.11n"
11N_AC_MODE                  = "Wireless-Modus 802.11n/ac"
11N_AX_MODE                  = "Wireless-Modus 802.11n/ac/ax"
11N_BE_MODE                  = "Wireless-Modus 802.11n/ac/ax/be"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Fat Kanal Intolerant"
LOWEST_STR                   = "Am niedrigsten"
MEDIUM_LOW_STR               = "Mittel-niedrig"
MEDIUM_STR                   = "Mittel"
MEDIUM_HIGH_STR              = "Mittel-hoch"
HIGHEST_STR                  = "Am höchsten"
DISABLED_STR                 = "Deaktiviert"
ENABLED_STR                  = "Aktiviert"
MAXIMUM_POWER_SAVING_STR     = "Maximale Energieersparnis"
NOISY_ENVIRONMENT_STR        = "Laute Umgebung"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "'CTS-to-self' aktiviert"
RTS_CTS_ENABLED_STR          = "RTS/CTS aktiviert"
AUTO_STR                     = "Auto"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "Auto"
WMM_DISABLED_STR             = "WMM deaktiviert"
WMM_ENABLED_STR              = "WMM aktiviert"
NO_PREFERECE_STR             = "Keine Einstellung"
PREFER_24_BAND_STR           = "2,4-GHz-Band bevorzugen"
PREFER_52_BAND_STR           = "5 GHz-Band bevorzugt"
PREFER_6_BAND_STR            = "6 GHz-Band bevorzugt"
PREFER_52_6_BAND_STR         = "5-GHz- + 6-GHz-Band bevorzugen"
WAKE_ON_MAGIC_PACKET         = "Aktivierung durch Magic Packet"
WAKE_ON_PATTERN_MATCH        = "Aktivierung durch Musterübereinstimmung"
PM_WIFI_REKEY_OFFLOAD        = "GTK führt Neuverschlüsselung für WoWLAN durch"
PM_ARP_OFFLOAD               = "ARP-Offload für WoWLAN"
PM_NS_OFFLOAD                = "NS-Offload für WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Medientrennung beim Aufrechterhalten des Energiesparmodus von WoWLAN"
PACKET_COALESCING            = "Paketzusammenfügung"
U_APSD_SUPPORT               = "U-APSD-Unterstützung"
THROUGHPUTBOOSTER_STR        = "Durchsatzbooster"
MIMO_POWER_SAVE_MODE_STR     = "MIMO-Energiesparmodus"
MIMO_AUTO_STR                = "Auto-SMPS"
NO_MIMO_STR                  = "Statische SMPS"
RTS_BEFORE_MIMO_STR          = "Dynamische SMPS"
NO_RTS_BEFORE_MIMO_STR       = "Keine SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "Doppelanschlusstechnik"
SOURCEDISK1                  = "Intel(R) Wireless - Installationsdiskette"
UHB_BAND_SUPPORTED_STR       = "Ultra High-Band (6 GHz)"
HUMAN_PRESENCE_DETECTION_STR = "Präsenzerkennung (Human Presence Detection, HPD)"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Greek (Greece)
[Strings.0408]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Πρόγραμμα οδήγησης προσαρμογέα Intel(R) Wireless για Windows 10 64 Bit"
RECOMMENDED_CHANNEL24_STR    = "Κανάλι ad hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Κανάλι ad hoc 802.11a"
RECOMMENDED_BAND             = "Προεπιλεγμένη ασύρματη λειτουργία ad hoc"
IBSS_TX_POWER_STR            = "Ισχύς μετάδοσης"
ROAMING_AGGRESSIVENESS_STR   = "Δυναμικότητα περιαγωγής"
ADHOC_POWER_MANAGEMENT_STR   = "Διαχείριση ισχύος ad hoc"
ADHOC_QOS_MODE_STR           = "Τρόπος λειτουργίας Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR    = "Προστασία μεικτής λειτουργίας"
THROUGHPUT_ENHANCEMENT_STR   = "Βελτίωση ικανότητας μετάδοσης"
WIRELESS_MODE_STR            = "Ασύρματη λειτουργία 802.11a/b/g"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2,4 GHz 802.11b"
WIRELESS_MODE_G              = "2,4 GHz 802.11g"
WIRELESS_MODE_BG             = "2,4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Διπλή ζώνη 802.11a/g"
WIRELESS_MODE_ABG            = "Διπλή ζώνη 802.11a/b/g"
PREFERRED_BAND_STR           = "Προτιμώμενη ζώνη"
CHANNELWIDTH52               = "Εύρος καναλιού για 5GHz"
CHANNELWIDTH6                = "Εύρος καναλιού για 6GHz"
CHANNELWIDTH24               = "Εύρος καναλιού για 2,4GHz"
TGnMode                      = "Ασύρματη λειτουργία 802.11n"
11N_AC_MODE                  = "Ασύρματη λειτουργία 802.11n/ac"
11N_AX_MODE                  = "Ασύρματη λειτουργία 802.11n/ac/ax"
11N_BE_MODE                  = "Ασύρματη λειτουργία 802.11n/ac/ax/be"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Μη συμβατό με ισχυρά κανάλια"
LOWEST_STR                   = "Χαμηλότερη"
MEDIUM_LOW_STR               = "Μεσαία-Χαμηλή"
MEDIUM_STR                   = "Μεσαία"
MEDIUM_HIGH_STR              = "Μεσαία-Υψηλή"
HIGHEST_STR                  = "Υψηλότερη"
DISABLED_STR                 = "Απενεργοποιημένη"
ENABLED_STR                  = "Ενεργοποιημένη"
MAXIMUM_POWER_SAVING_STR     = "Μέγιστη εξοικονόμηση ισχύος"
NOISY_ENVIRONMENT_STR        = "Θορυβώδες περιβάλλον"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "Ενεργοποιημένο CTS-to-self"
RTS_CTS_ENABLED_STR          = "Ενεργοποιημένο RTS/CTS"
AUTO_STR                     = "Αυτόματα"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "Αυτόματα"
WMM_DISABLED_STR             = "Απενεργοποιημένη WMM"
WMM_ENABLED_STR              = "Ενεργοποιημένη WMM"
NO_PREFERECE_STR             = "Καμία προτίμηση"
PREFER_24_BAND_STR           = "Προτίμηση ζώνη 2,4 GHz"
PREFER_52_BAND_STR           = "Προτίμηση ζώνης 5 GHz"
PREFER_6_BAND_STR            = "Προτίμηση ζώνης 6 GHz"
PREFER_52_6_BAND_STR         = "Προτίμηση ζώνης 5 GHz + 6 GHz"
WAKE_ON_MAGIC_PACKET         = "Ενεργοποίηση με Μαγικό πακέτο"
WAKE_ON_PATTERN_MATCH        = "Ενεργοποίηση με αντιστοίχιση μοτίβου"
PM_WIFI_REKEY_OFFLOAD        = "Το GTK ζητά τη δημιουργία νέου κλειδιού για WoWLAN"
PM_ARP_OFFLOAD               = "Μείωση φόρτου ARP για WoWLAN"
PM_NS_OFFLOAD                = "Μείωση φόρτου NS για WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Αναστολή λειτουργίας κατά την αποσύνδεση του WoWLAN"
PACKET_COALESCING            = "Ενοποίηση πακέτων"
U_APSD_SUPPORT               = "Υποστήριξη U-APSD"
THROUGHPUTBOOSTER_STR        = "Ενισχυτής μετάδοσης"
MIMO_POWER_SAVE_MODE_STR     = "Λειτουργία εξοικονόμησης ενέργειας MIMO"
MIMO_AUTO_STR                = "Αυτόματο SMPS"
NO_MIMO_STR                  = "Στατικό SMPS"
RTS_BEFORE_MIMO_STR          = "Δυναμικό SMPS"
NO_RTS_BEFORE_MIMO_STR       = "Χωρίς SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "Τεχνολογία διπλής σύνδεσης"
SOURCEDISK1                  = "Δισκέτα εγκατάστασης Intel(R) Wireless"
UHB_BAND_SUPPORTED_STR       = "Ζώνη εξαιρετικά υψηλών συχνοτήτων (6 GHz)"
HUMAN_PRESENCE_DETECTION_STR = "Ανίχνευση ανθρώπινης παρουσίας"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Spanish (Spain)
[Strings.0C0A]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Controlador del adaptador Intel(R) Wireless para Windows 10 de 64 bits"
RECOMMENDED_CHANNEL24_STR    = "Canal Ad Hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Canal Ad Hoc 802.11a"
RECOMMENDED_BAND             = "Modo inalámbrico predeterminado Ad Hoc"
IBSS_TX_POWER_STR            = "Potencia de transmisión"
ROAMING_AGGRESSIVENESS_STR   = "Agresividad de itinerancia"
ADHOC_POWER_MANAGEMENT_STR   = "Administración de energía Ad Hoc"
ADHOC_QOS_MODE_STR           = "Modo QoS Ad Hoc"
MIXED_MODE_PROTECTION_STR    = "Protección de modo mixto"
THROUGHPUT_ENHANCEMENT_STR   = "Optimización de la capacidad de proceso"
WIRELESS_MODE_STR            = "Modo inalámbrico 802.11a/b/g"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2,4 GHz 802.11b"
WIRELESS_MODE_G              = "2,4 GHz 802.11g"
WIRELESS_MODE_BG             = "2,4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Doble banda 802.11a/g"
WIRELESS_MODE_ABG            = "Doble banda 802.11a/b/g"
PREFERRED_BAND_STR           = "Banda preferida"
CHANNELWIDTH52               = "Ancho de canal para 5 GHz"
CHANNELWIDTH6                = "Ancho de canal para 6 GHz"
CHANNELWIDTH24               = "Ancho de canal para 2,4GHz"
TGnMode                      = "Modo inalámbrico 802.11n"
11N_AC_MODE                  = "Modo inalámbrico 802.11n/ac"
11N_AX_MODE                  = "Modo inalámbrico 802.11n/ac/ax"
11N_BE_MODE                  = "Modo inalámbrico 802.11n/ac/ax/be"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "No compatible con canal de 40 MHz"
LOWEST_STR                   = "Mínimo"
MEDIUM_LOW_STR               = "Bajo"
MEDIUM_STR                   = "Mediano"
MEDIUM_HIGH_STR              = "Alto"
HIGHEST_STR                  = "Máximo"
DISABLED_STR                 = "Desactivado"
ENABLED_STR                  = "Activado"
MAXIMUM_POWER_SAVING_STR     = "Máximo ahorro de energía"
NOISY_ENVIRONMENT_STR        = "Entorno ruidoso"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "CTS-to-self activado"
RTS_CTS_ENABLED_STR          = "RTS/CTS activado"
AUTO_STR                     = "Automático"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "Automático"
WMM_DISABLED_STR             = "WMM desactivado"
WMM_ENABLED_STR              = "WMM activado"
NO_PREFERECE_STR             = "Sin preferencias"
PREFER_24_BAND_STR           = "Preferir la banda de 2,4 GHz"
PREFER_52_BAND_STR           = "Preferencia de banda 5 GHz"
PREFER_6_BAND_STR            = "Preferencia de banda 6 GHz"
PREFER_52_6_BAND_STR         = "Preferencia de bandas 5 GHz + 6 GHz"
WAKE_ON_MAGIC_PACKET         = "Magic Packet de reactivación"
WAKE_ON_PATTERN_MATCH        = "Coincidencia de patrones de reactivación"
PM_WIFI_REKEY_OFFLOAD        = "Regeneración de clave GTK para WoWLAN"
PM_ARP_OFFLOAD               = "Descarga ARP para WoWLAN"
PM_NS_OFFLOAD                = "Descarga NS para WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Suspensión al desconectar WoWLAN"
PACKET_COALESCING            = "Fusión de paquetes"
U_APSD_SUPPORT               = "Soporte de U-APSD"
THROUGHPUTBOOSTER_STR        = "Impulsar la capacidad de proceso"
MIMO_POWER_SAVE_MODE_STR     = "Modo de ahorro de energía MIMO"
MIMO_AUTO_STR                = "SMPS automático"
NO_MIMO_STR                  = "SMPS estático"
RTS_BEFORE_MIMO_STR          = "SMPS dinámico"
NO_RTS_BEFORE_MIMO_STR       = "Sin SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "Tecnología de conexión doble"
SOURCEDISK1                  = "Disco de instalación de Intel(R) Wireless"
UHB_BAND_SUPPORTED_STR       = "Banda ultraalta (6 GHz)"
HUMAN_PRESENCE_DETECTION_STR = "Detección de presencia humana"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Finnish (Finland)
[Strings.040B]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Intel(R) Wireless -sovitinohjain Windows 10 64-bit -käyttöjärjestelmään"
RECOMMENDED_CHANNEL24_STR    = "Ad Hoc -kanava 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Ad Hoc -kanava 802.11a "
RECOMMENDED_BAND             = "Langaton Ad Hoc -oletustila"
IBSS_TX_POWER_STR            = "Lähetysteho"
ROAMING_AGGRESSIVENESS_STR   = "Solukonpäivitysaktiivisuus"
ADHOC_POWER_MANAGEMENT_STR   = "Ad Hoc -virranhallinta"
ADHOC_QOS_MODE_STR           = "Ad Hoc QoS -tila"
MIXED_MODE_PROTECTION_STR    = "Sekatilan Suojaus"
THROUGHPUT_ENHANCEMENT_STR   = "Läpimenon parantaminen"
WIRELESS_MODE_STR            = "802.11a/b/g Langaton tila"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2,4 GHz 802.11b"
WIRELESS_MODE_G              = "2,4 GHz 802.11g"
WIRELESS_MODE_BG             = "2,4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Kaksikaistainen 802.11a/g"
WIRELESS_MODE_ABG            = "Kaksikaistainen 802.11a/b/g"
PREFERRED_BAND_STR           = "Ensisijainen kaista"
CHANNELWIDTH52               = "5 GHz:n kanavaleveys"
CHANNELWIDTH6                = "6 GHz:n kanavaleveys"
CHANNELWIDTH24               = "2,4 GHz:n kanavaleveys"
TGnMode                      = "802.11n Langaton tila"
11N_AC_MODE                  = "802.11n/ac Langaton tila"
11N_AX_MODE                  = "802.11n/ac/ax Langaton tila"
11N_BE_MODE                  = "802.11n/ac/ax/be Langaton tila"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Fat Channel -esto"
LOWEST_STR                   = "Pienin"
MEDIUM_LOW_STR               = "Kohtalainen-pieni"
MEDIUM_STR                   = "Kohtalainen"
MEDIUM_HIGH_STR              = "Kohtalainen-suuri"
HIGHEST_STR                  = "Suurin"
DISABLED_STR                 = "Poissa käytöstä"
ENABLED_STR                  = "Käytössä"
MAXIMUM_POWER_SAVING_STR     = "Suurin virransäästö"
NOISY_ENVIRONMENT_STR        = "Häiriöllinen ympäristö"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "CTS itselle käytössä"
RTS_CTS_ENABLED_STR          = "RTS/CTS käytössä"
AUTO_STR                     = "Automaattinen"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "Automaattinen"
WMM_DISABLED_STR             = "WMM poissa käytöstä"
WMM_ENABLED_STR              = "WMM käytössä"
NO_PREFERECE_STR             = "Ei ensisijaisuutta"
PREFER_24_BAND_STR           = "2,4 GHz:n kaista ensisijainen"
PREFER_52_BAND_STR           = "5 GHz:n kaista"
PREFER_6_BAND_STR            = "6 GHz:n kaista"
PREFER_52_6_BAND_STR         = "5 GHz:n + 6 GHz:n kaista ensisijainen"
WAKE_ON_MAGIC_PACKET         = "Aktivointi Magic-paketilla"
WAKE_ON_PATTERN_MATCH        = "Aktivointi mallivastaavuudella"
PM_WIFI_REKEY_OFFLOAD        = "WoWLAN-toiminnon GTK-uudelleenavainnus "
PM_ARP_OFFLOAD               = "WoWLAN-toiminnon ARP-purku"
PM_NS_OFFLOAD                = "WoWLAN-toiminnon NS-purku"
DEVICE_SLEEP_ON_DISCONNECT   = "Lepotilaan, kun WoWLAN-yhteys katkaistu"
PACKET_COALESCING            = "Pakettien yhdistäminen"
U_APSD_SUPPORT               = "U-APSD-tuki"
THROUGHPUTBOOSTER_STR        = "Siirtomäärän tehostus"
MIMO_POWER_SAVE_MODE_STR     = "MIMO-virransäästötila"
MIMO_AUTO_STR                = "AutomaattinenSMPS"
NO_MIMO_STR                  = "Staattinen SMPS"
RTS_BEFORE_MIMO_STR          = "Dynaaminen SMPS"
NO_RTS_BEFORE_MIMO_STR       = "Ei SMPS:ää"
DOUBLECONNECTTECHNOLOGY_STR  = "Dual Connect -teknologia"
SOURCEDISK1                  = "Intel(R) Wireless asennuslevy"
UHB_BAND_SUPPORTED_STR       = "Äärimmäisen suuri kaistanleveys (6 GHz)"
HUMAN_PRESENCE_DETECTION_STR = "Ihmisen läsnäolon havaitseminen"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; French (France)
[Strings.040C]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Pilote de carte Intel(R) Wireless pour Windows 10 64 bits "
RECOMMENDED_CHANNEL24_STR    = "Canal ad hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Canal ad hoc 802.11a"
RECOMMENDED_BAND             = "Mode ad hoc sans fil par défaut"
IBSS_TX_POWER_STR            = "Puissance de transmission"
ROAMING_AGGRESSIVENESS_STR   = "Agressivité de l’itinérance"
ADHOC_POWER_MANAGEMENT_STR   = "Gestion de l'alimentation ad hoc"
ADHOC_QOS_MODE_STR           = "Mode Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR    = "Protection en mode mixte"
THROUGHPUT_ENHANCEMENT_STR   = "Optimisation du débit"
WIRELESS_MODE_STR            = "Mode sans fil 802.11a/b/g"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2,4 GHz 802.11b"
WIRELESS_MODE_G              = "2,4 GHz 802.11g"
WIRELESS_MODE_BG             = "2,4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Dual Band 802.11a/g"
WIRELESS_MODE_ABG            = "Dual Band 802.11a/b/g"
PREFERRED_BAND_STR           = "Bande privilégiée"
CHANNELWIDTH52               = "Largeur de canal pour 5 GHz"
CHANNELWIDTH6                = "Largeur de canal pour 6 GHz"
CHANNELWIDTH24               = "Largeur de canal pour 2,4 GHz"
TGnMode                      = "Mode sans fil 802.11n"
11N_AC_MODE                  = "Mode sans fil 802.11n/ac"
11N_AX_MODE                  = "Mode sans fil 802.11n/ac/ax"
11N_BE_MODE                  = "Mode sans fil 802.11n/ac/ax/be"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Incompatible avec canaux de 40 MHz"
LOWEST_STR                   = "Min."
MEDIUM_LOW_STR               = "Faible"
MEDIUM_STR                   = "Moyenne"
MEDIUM_HIGH_STR              = "Élevée"
HIGHEST_STR                  = "Max."
DISABLED_STR                 = "Désactivé(e)"
ENABLED_STR                  = "Activé(e)"
MAXIMUM_POWER_SAVING_STR     = "Économie d'énergie max."
NOISY_ENVIRONMENT_STR        = "Environnement bruyant"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "Auto-CTS activée"
RTS_CTS_ENABLED_STR          = "RTS/CTS activée"
AUTO_STR                     = "Auto"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "Auto"
WMM_DISABLED_STR             = "WMM désactivée"
WMM_ENABLED_STR              = "WMM activée"
NO_PREFERECE_STR             = "Aucune préférence"
PREFER_24_BAND_STR           = "Préférer bande 2,4 GHz"
PREFER_52_BAND_STR           = "Préférer la bande 5 GHz"
PREFER_6_BAND_STR            = "Préférer la bande 6 GHz"
PREFER_52_6_BAND_STR         = "Préférer la bande 5 GHz + 6 GHz"
WAKE_ON_MAGIC_PACKET         = "Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH        = "Correspondance au modèle WOL"
PM_WIFI_REKEY_OFFLOAD        = "Régénération des clés GTK pour WoWLAN"
PM_ARP_OFFLOAD               = "Délestage ARP pour WoWLAN"
PM_NS_OFFLOAD                = "Délestage NS pour WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Veille à la déconnexion WoWLAN"
PACKET_COALESCING            = "Fusion des paquets"
U_APSD_SUPPORT               = "Assistance U-APSD"
THROUGHPUTBOOSTER_STR        = "Multiplicateur de débit"
MIMO_POWER_SAVE_MODE_STR     = "MIMO – Mode économie d'énergie"
MIMO_AUTO_STR                = "SMPS auto"
NO_MIMO_STR                  = "SMPS statique"
RTS_BEFORE_MIMO_STR          = "SMPS dynamique"
NO_RTS_BEFORE_MIMO_STR       = "SMPS désactivé"
DOUBLECONNECTTECHNOLOGY_STR  = "Technologie de connexion double"
SOURCEDISK1                  = "Disque d'installation de Intel(R) Wireless"
UHB_BAND_SUPPORTED_STR       = "Bande ultra élevée (6 GHz)"
HUMAN_PRESENCE_DETECTION_STR = "Détection de la présence humaine"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Hebrew (Israel)
[Strings.040D]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "מנהל התקן של מתאם Intel(R) Wireless עבור Windows 10 64 Bit"
RECOMMENDED_CHANNEL24_STR    = "ערוץ אד הוק 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "ערוץ אד הוק 802.11a"
RECOMMENDED_BAND             = "מצב אלחוטי ברירת מחדל של אד הוק"
IBSS_TX_POWER_STR            = "עוצמת שידור"
ROAMING_AGGRESSIVENESS_STR   = "תוקפנות נדידה"
ADHOC_POWER_MANAGEMENT_STR   = "ניהול צריכת חשמל אד הוק"
ADHOC_QOS_MODE_STR           = "מצב QoS אד-הוק"
MIXED_MODE_PROTECTION_STR    = "הגנת מצב מעורב"
THROUGHPUT_ENHANCEMENT_STR   = "שיפור קצב העברה"
WIRELESS_MODE_STR            = "מצב אלחוטי 802.11a/b/g"
WIRELESS_MODE_A              = "5GHz ‏802.11a"
WIRELESS_MODE_B              = "2.4GHz ‏802.11b"
WIRELESS_MODE_G              = "2.4GHz ‏802.11g"
WIRELESS_MODE_BG             = "2.4GHz ‏802.11b/g"
WIRELESS_MODE_AG             = "פס כפול 802.11a/g"
WIRELESS_MODE_ABG            = "פס כפול 802.11a/b/g"
PREFERRED_BAND_STR           = "פס מועדף"
CHANNELWIDTH52               = "רוחב פס עבור 5GHz"
CHANNELWIDTH6                = "רוחב פס עבור 6GHz"
CHANNELWIDTH24               = "רוחב פס עבור 2.4GHz"
TGnMode                      = "מצב אלחוטי 802.11n"
11N_AC_MODE                  = "מצב אלחוטי 802.11n/ac"
11N_AX_MODE                  = "מצב אלחוטי 802.11n/ac/ax"
11N_BE_MODE                  = "מצב אלחוטי 802.11n/ac/ax/be"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "לא תואם לערוץ 40Mhz"
LOWEST_STR                   = "נמוך ביותר"
MEDIUM_LOW_STR               = "בינוני-נמוך"
MEDIUM_STR                   = "בינוני"
MEDIUM_HIGH_STR              = "בינוני-גבוה"
HIGHEST_STR                  = "גבוה ביותר"
DISABLED_STR                 = "מנוטרל"
ENABLED_STR                  = "זמין"
MAXIMUM_POWER_SAVING_STR     = "חיסכון מרבי בחשמל"
NOISY_ENVIRONMENT_STR        = "סביבה רועשת"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "מאופשר CTS-אל-עצמו"
RTS_CTS_ENABLED_STR          = "מאופשר RTS/CTS"
AUTO_STR                     = "אוטומטי"
CHANNELWIDTH20ONLY           = "‎20 MHz"
CHANNELWIDTHAUTO             = "אוטומטי"
WMM_DISABLED_STR             = "WMM מנוטרל"
WMM_ENABLED_STR              = "WMM זמין"
NO_PREFERECE_STR             = "אין העדפה"
PREFER_24_BAND_STR           = "העדפת פס ‎2.4GHz"
PREFER_52_BAND_STR           = "העדפת פס ‎5GHz"
PREFER_6_BAND_STR            = "העדפת פס ‎6GHz"
PREFER_52_6_BAND_STR         = "העדפת פס 5GHz + 6GHz"
WAKE_ON_MAGIC_PACKET         = "התעורר בעת מנת Magic"
WAKE_ON_PATTERN_MATCH        = "התעורר בעת התאמת תבנית"
PM_WIFI_REKEY_OFFLOAD        = "החלפת מפתחות GTK עבור WoWLAN"
PM_ARP_OFFLOAD               = "העברת ARP עבור WoWLAN"
PM_NS_OFFLOAD                = "העברת NS עבור WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "כניסה למצב שינה עם ניתוק WoWLAN"
PACKET_COALESCING            = "מיזוג מנה"
U_APSD_SUPPORT               = "תמיכה ב- U-APSD"
THROUGHPUTBOOSTER_STR        = "הגברת תפוקה"
MIMO_POWER_SAVE_MODE_STR     = "מצב חיסכון בחשמל MIMO"
MIMO_AUTO_STR                = "SMPS אוטומטי"
NO_MIMO_STR                  = "SMPS סטטי"
RTS_BEFORE_MIMO_STR          = "SMPS דינמי"
NO_RTS_BEFORE_MIMO_STR       = "ללא SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "טכנולוגיית חיבור כפול"
SOURCEDISK1                  = "דיסק התקנה של Intel(R) Wireless"
UHB_BAND_SUPPORTED_STR       = "תדר גבוה במיוחד (6GHz)"
HUMAN_PRESENCE_DETECTION_STR = "זיהוי נוכחות אנשים"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Hungarian (Hungary)
[Strings.040E]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Intel(R) Wireless adapter illesztőprogram 64 bites Windows 10"
RECOMMENDED_CHANNEL24_STR    = "Alkalmi csatorna 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Alkalmi csatorna 802.11a"
RECOMMENDED_BAND             = "Alkalmi kapcsolat alap üzemmódja"
IBSS_TX_POWER_STR            = "Sugárzási teljesítmény"
ROAMING_AGGRESSIVENESS_STR   = "A barangolás intenzitása"
ADHOC_POWER_MANAGEMENT_STR   = "Alkalmi hálózat energiagazdálkodásai"
ADHOC_QOS_MODE_STR           = "Alkalmi QoS üzemmód"
MIXED_MODE_PROTECTION_STR    = "Vegyes üzemmódú védelem"
THROUGHPUT_ENHANCEMENT_STR   = "Az átviteli kapacitás növelése"
WIRELESS_MODE_STR            = "802.11a/b/g Vezeték nélküli üzemmód"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2,4 GHz 802.11b"
WIRELESS_MODE_G              = "2,4 GHz 802.11g"
WIRELESS_MODE_BG             = "2,4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Dual Band 802.11a/g"
WIRELESS_MODE_ABG            = "Dual Band 802.11a/b/g"
PREFERRED_BAND_STR           = "Preferált frekvenciasáv"
CHANNELWIDTH52               = "Csatorna sávszélessége 5 GHz értékre"
CHANNELWIDTH6                = "Csatorna sávszélessége 6 GHz értékre"
CHANNELWIDTH24               = "Csatorna sávszélessége 2,4 GHz értékre"
TGnMode                      = "802.11n Vezeték nélküli üzemmód"
11N_AC_MODE                  = "802.11n/ac Vezeték nélküli üzemmód"
11N_AX_MODE                  = "802.11n/ac/ax Vezeték nélküli üzemmód"
11N_BE_MODE                  = "802.11n/ac/ax/be Vezeték nélküli üzemmód"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Csökkentett sávszélességen működik"
LOWEST_STR                   = "Legalacsonyabb"
MEDIUM_LOW_STR               = "Közepes - alacsony"
MEDIUM_STR                   = "Közepes"
MEDIUM_HIGH_STR              = "Közepes - magas"
HIGHEST_STR                  = "Legmagasabb"
DISABLED_STR                 = "Letiltva"
ENABLED_STR                  = "Engedélyezve"
MAXIMUM_POWER_SAVING_STR     = "Max. energiatakarékosság"
NOISY_ENVIRONMENT_STR        = "Zajos környezet"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "CTS-to-self engedélyezve"
RTS_CTS_ENABLED_STR          = "RTS/CTS engedélyezve"
AUTO_STR                     = "Auto"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "Auto"
WMM_DISABLED_STR             = "WMM letiltva"
WMM_ENABLED_STR              = "WMM engedélyezve"
NO_PREFERECE_STR             = "Nincs preferencia"
PREFER_24_BAND_STR           = "2,4 GHz-es sáv preferálása"
PREFER_52_BAND_STR           = "A 5 GHz-es sáv előnyben részesítése"
PREFER_6_BAND_STR            = "A 6 GHz-es sáv előnyben részesítése"
PREFER_52_6_BAND_STR         = "5 GHz-es + 6 GHz-es sáv preferálása"
WAKE_ON_MAGIC_PACKET         = "Ébresztés magic-csomaggal"
WAKE_ON_PATTERN_MATCH        = "Ébresztés mintaegyezésre"
PM_WIFI_REKEY_OFFLOAD        = "GTK újrakulcsolás WoWLAN hálózathoz"
PM_ARP_OFFLOAD               = "ARP tehermentesítés WoWLAN hálózathoz"
PM_NS_OFFLOAD                = "NS tehermentesítés WoWLAN hálózathoz"
DEVICE_SLEEP_ON_DISCONNECT   = "Alvó állapot WoWLAN hálózati szétkapcsolás esetén"
PACKET_COALESCING            = "Csomagegyesítés"
U_APSD_SUPPORT               = "U-APSD támogatás"
THROUGHPUTBOOSTER_STR        = "Átviteli sebesség növelés "
MIMO_POWER_SAVE_MODE_STR     = "MIMO energiatakarékos üzemmód"
MIMO_AUTO_STR                = "Auto. SMPS"
NO_MIMO_STR                  = "Statikus SMPS"
RTS_BEFORE_MIMO_STR          = "Dinamikus SMPS"
NO_RTS_BEFORE_MIMO_STR       = "Nincs SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "Dupla csatlakozási technológia"
SOURCEDISK1                  = "Intel(R) Wireless telepítő lemez"
UHB_BAND_SUPPORTED_STR       = "Ultraszéles frekvenciasáv (6 GHz)"
HUMAN_PRESENCE_DETECTION_STR = "Emberi jelenlét észlelése"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Italian (Italy)
[Strings.0410]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Driver scheda Intel(R) Wireless per Windows 10 64 Bit"
RECOMMENDED_CHANNEL24_STR    = "Canale Ad Hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Canale Ad Hoc 802.11a"
RECOMMENDED_BAND             = "Modalità wireless predefinita Ad Hoc"
IBSS_TX_POWER_STR            = "Potenza di trasmissione"
ROAMING_AGGRESSIVENESS_STR   = "Efficacia roaming"
ADHOC_POWER_MANAGEMENT_STR   = "Risparmio energia ad hoc"
ADHOC_QOS_MODE_STR           = "Modalità Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR    = "Protezione a modalità mista"
THROUGHPUT_ENHANCEMENT_STR   = "Miglioramento velocità effettiva"
WIRELESS_MODE_STR            = "Modalità wireless 802.11a/b/g"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2,4 GHz 802311b"
WIRELESS_MODE_G              = "2,4 GHz 802.11g"
WIRELESS_MODE_BG             = "2,4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Dual Band 802.11a/g"
WIRELESS_MODE_ABG            = "Dual Band 802.11a/b/g"
PREFERRED_BAND_STR           = "Banda preferita"
CHANNELWIDTH52               = "Larghezza canale per 5 GHz"
CHANNELWIDTH6                = "Larghezza canale per 6 GHz"
CHANNELWIDTH24               = "Larghezza canale per 2,4 GHz"
TGnMode                      = "Modalità wireless 802.11n"
11N_AC_MODE                  = "Modalità wireless 802.11n/ac"
11N_AX_MODE                  = "Modalità wireless 802.11n/ac/ax"
11N_BE_MODE                  = "Modalità wireless 802.11n/ac/ax/be"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Fat Channel incompatibile"
LOWEST_STR                   = "Minimo"
MEDIUM_LOW_STR               = "Medio-basso"
MEDIUM_STR                   = "Medio"
MEDIUM_HIGH_STR              = "Medio-alto"
HIGHEST_STR                  = "Massimo"
DISABLED_STR                 = "Disattivata"
ENABLED_STR                  = "Attivata"
MAXIMUM_POWER_SAVING_STR     = "Max. risparmio energetico"
NOISY_ENVIRONMENT_STR        = "Ambienti rumorosi"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "CTS-to-self attivato"
RTS_CTS_ENABLED_STR          = "Attivato RTS/CTS"
AUTO_STR                     = "Auto"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "Auto"
WMM_DISABLED_STR             = "WMM disattivata"
WMM_ENABLED_STR              = "WMM attivata"
NO_PREFERECE_STR             = "Nessuna preferenza"
PREFER_24_BAND_STR           = "Preferenza a banda a 2,4 GHz"
PREFER_52_BAND_STR           = "Banda a 5 GHz"
PREFER_6_BAND_STR            = "Banda a 6 GHz"
PREFER_52_6_BAND_STR         = "Preferenza per la banda a 5 GHz e 6 GHz"
WAKE_ON_MAGIC_PACKET         = "Magic Packet per riattivazione"
WAKE_ON_PATTERN_MATCH        = "Corrispondenza motivo per riattivazione"
PM_WIFI_REKEY_OFFLOAD        = "Rigenerazione delle chiavi GTK per WoWLAN"
PM_ARP_OFFLOAD               = "Offload ARP per WoWLAN"
PM_NS_OFFLOAD                = "Offload NS per WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Sospensione attiva alla disconnessione da WoWLAN"
PACKET_COALESCING            = "Unione pacchetti"
U_APSD_SUPPORT               = "Supporto U-APSD"
THROUGHPUTBOOSTER_STR        = "Incremento del throughput"
MIMO_POWER_SAVE_MODE_STR     = "Modalità risparmio energia MIMO"
MIMO_AUTO_STR                = "SMPS automatico"
NO_MIMO_STR                  = "SMPS statico"
RTS_BEFORE_MIMO_STR          = "SMPS dinamico"
NO_RTS_BEFORE_MIMO_STR       = "Senza SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "Tecnologia a doppia connessione"
SOURCEDISK1                  = "Disco di installazione per Intel(R) Wireless"
UHB_BAND_SUPPORTED_STR       = "Banda ultralarga (6GHz)"
HUMAN_PRESENCE_DETECTION_STR = "Rilevamento della presenza umana"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Japanese (Japan)
[Strings.0411]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Windows 10 64 ビット用 Intel(R) Wireless アダプタードライバー"
RECOMMENDED_CHANNEL24_STR    = "アドホック チャネル 802.11b/g "
RECOMMENDED_CHANNEL52_STR    = "アドホック チャネル 802.11a"
RECOMMENDED_BAND             = "アドホック デフォルト ワイヤレス モード"
IBSS_TX_POWER_STR            = "送信パワー"
ROAMING_AGGRESSIVENESS_STR   = "ローミングの積極性"
ADHOC_POWER_MANAGEMENT_STR   = "アドホック電源管理"
ADHOC_QOS_MODE_STR           = "アドホック QoS モード"
MIXED_MODE_PROTECTION_STR    = "混在モード保護"
THROUGHPUT_ENHANCEMENT_STR   = "スループットの増加"
WIRELESS_MODE_STR            = "802.11a/b/g ワイヤレスモード"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2.4 GHz 802.11b"
WIRELESS_MODE_G              = "2.4 GHz 802.11g"
WIRELESS_MODE_BG             = "2.4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Dual Band 802.11a/g"
WIRELESS_MODE_ABG            = "デュアルバンド 802.11a/b/g"
PREFERRED_BAND_STR           = "優先バンド"
CHANNELWIDTH52               = "チャネル幅 (5GHz 用)"
CHANNELWIDTH6                = "チャネル幅 (6GHz 用)"
CHANNELWIDTH24               = "チャネル幅 (2.4GHz 用)"
TGnMode                      = "802.11n ワイヤレスモード"
11N_AC_MODE                  = "802.11n/ac ワイヤレスモード"
11N_AX_MODE                  = "802.11n/ac/ax ワイヤレスモード"
11N_BE_MODE                  = "802.11n/ac/ax/be ワイヤレスモード"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "40Mhz チャネル幅非互換"
LOWEST_STR                   = "最低"
MEDIUM_LOW_STR               = "中低"
MEDIUM_STR                   = "中"
MEDIUM_HIGH_STR              = "中高"
HIGHEST_STR                  = "最高"
DISABLED_STR                 = "無効"
ENABLED_STR                  = "有効"
MAXIMUM_POWER_SAVING_STR     = "最大節電"
NOISY_ENVIRONMENT_STR        = "雑音環境"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "個別 CTS 有効"
RTS_CTS_ENABLED_STR          = "RTS/CTS 有効"
AUTO_STR                     = "自動"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "自動"
WMM_DISABLED_STR             = "WMM 無効"
WMM_ENABLED_STR              = "WMM 有効"
NO_PREFERECE_STR             = "優先順位なし"
PREFER_24_BAND_STR           = "2.4 GHz バンドの優先"
PREFER_52_BAND_STR           = "5 GHz バンドを優先"
PREFER_6_BAND_STR            = "6 GHz バンドを優先"
PREFER_52_6_BAND_STR         = "5GHz と 6GHz バンドを優先"
WAKE_ON_MAGIC_PACKET         = "Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH        = "Wake on Pattern Match"
PM_WIFI_REKEY_OFFLOAD        = "WoWLAN の GTK Rekey"
PM_ARP_OFFLOAD               = "WoWLAN の ARP オフロード"
PM_NS_OFFLOAD                = "WoWLAN の NS オフロード"
DEVICE_SLEEP_ON_DISCONNECT   = "WoWLAN のスリープ状態の解除"
PACKET_COALESCING            = "パケット結合"
U_APSD_SUPPORT               = "U-APSD 対応"
THROUGHPUTBOOSTER_STR        = "スループット・ブースター"
MIMO_POWER_SAVE_MODE_STR     = "MIMO 省電力モード"
MIMO_AUTO_STR                = "自動 SMPS"
NO_MIMO_STR                  = "静的 SMPS"
RTS_BEFORE_MIMO_STR          = "動的 SMPS"
NO_RTS_BEFORE_MIMO_STR       = "SMPS なし"
DOUBLECONNECTTECHNOLOGY_STR  = "ダブル・コネクト・テクノロジー"
SOURCEDISK1                  = "Intel(R) Wireless インストール・ディスク"
UHB_BAND_SUPPORTED_STR       = "超高帯域幅 (6GHz)"
HUMAN_PRESENCE_DETECTION_STR = "ユーザーの存在を検出"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Korean (Korea)
[Strings.0412]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Windows 10 64비트용 Intel(R) Wireless 어댑터 드라이버"
RECOMMENDED_CHANNEL24_STR    = "Ad Hoc 채널 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Ad Hoc 채널 802.11a"
RECOMMENDED_BAND             = "Ad Hoc 기본 무선 모드"
IBSS_TX_POWER_STR            = "전송 전원"
ROAMING_AGGRESSIVENESS_STR   = "로밍의 주동성"
ADHOC_POWER_MANAGEMENT_STR   = "Ad Hoc 전원 관리"
ADHOC_QOS_MODE_STR           = "Ad Hoc QoS 모드"
MIXED_MODE_PROTECTION_STR    = "혼합 모드 보호"
THROUGHPUT_ENHANCEMENT_STR   = "처리량 개선"
WIRELESS_MODE_STR            = "802.11a/b/g 무선 모드"
WIRELESS_MODE_A              = "5GHz 802.11a"
WIRELESS_MODE_B              = "2.4GHz 802.11b"
WIRELESS_MODE_G              = "2.4GHz 802.11g"
WIRELESS_MODE_BG             = "2.4GHz 802.11b/g"
WIRELESS_MODE_AG             = "듀얼 밴드 802.11a/g"
WIRELESS_MODE_ABG            = "듀얼 밴드 802.11a/b/g"
PREFERRED_BAND_STR           = "기본 설정 밴드"
CHANNELWIDTH52               = "5GHz 채널 폭"
CHANNELWIDTH6                = "6GHz 채널 폭"
CHANNELWIDTH24               = "2.4GHz 채널 폭"
TGnMode                      = "802.11n 무선 모드"
11N_AC_MODE                  = "802.11n/ac 무선 모드"
11N_AX_MODE                  = "802.11n/ac/ax 무선 모드"
11N_BE_MODE                  = "802.11n/ac/ax/be 무선 모드"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "과부하 채널 비지원"
LOWEST_STR                   = "최하"
MEDIUM_LOW_STR               = "보통-낮음"
MEDIUM_STR                   = "보통"
MEDIUM_HIGH_STR              = "보통-높음"
HIGHEST_STR                  = "최고"
DISABLED_STR                 = "비활성화함"
ENABLED_STR                  = "활성화함"
MAXIMUM_POWER_SAVING_STR     = "최대 절전"
NOISY_ENVIRONMENT_STR        = "잡음 환경"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "자체 CTS 활성화함"
RTS_CTS_ENABLED_STR          = "RTS/CTS 활성화함"
AUTO_STR                     = "자동"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "자동"
WMM_DISABLED_STR             = "WMM 비활성화함"
WMM_ENABLED_STR              = "WMM 활성화함"
NO_PREFERECE_STR             = "기본 설정 없음"
PREFER_24_BAND_STR           = "2.4 GHz 밴드 선택"
PREFER_52_BAND_STR           = "5GHz 밴드 기본 설정"
PREFER_6_BAND_STR            = "6GHz 밴드 기본 설정"
PREFER_52_6_BAND_STR         = "5GHz + 6GHz 밴드 기본 설정"
WAKE_ON_MAGIC_PACKET         = "Wake on 매직 패킷"
WAKE_ON_PATTERN_MATCH        = "Wake on 패턴 일치"
PM_WIFI_REKEY_OFFLOAD        = "WoWLAN에 대한 GTK 키 재입력"
PM_ARP_OFFLOAD               = "WoWLAN에 대한 ARP 오프로드"
PM_NS_OFFLOAD                = "WoWLAN에 대한 NS 오프로드"
DEVICE_SLEEP_ON_DISCONNECT   = "WoWLAN 연결 해제 시 절전 상태"
PACKET_COALESCING            = "패킷 통합"
U_APSD_SUPPORT               = "U-APSD 지원"
THROUGHPUTBOOSTER_STR        = "처리량 부스터"
MIMO_POWER_SAVE_MODE_STR     = "MIMO 절전 모드"
MIMO_AUTO_STR                = "자동 SMPS"
NO_MIMO_STR                  = "정적 SMPS"
RTS_BEFORE_MIMO_STR          = "동적 SMPS"
NO_RTS_BEFORE_MIMO_STR       = "SMPS 안 함"
DOUBLECONNECTTECHNOLOGY_STR  = "이중 연결 기술"
SOURCEDISK1                  = "Intel(R) Wireless 시리즈 설치 디스크"
UHB_BAND_SUPPORTED_STR       = "초고대역 (6GHz)"
HUMAN_PRESENCE_DETECTION_STR = "인체 감지"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Dutch (Netherlands)
[Strings.0413]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Intel(R) Wireless adapter stuurprogramma onder Windows 10 64 Bit"
RECOMMENDED_CHANNEL24_STR    = "Ad-hockanaal 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Ad-hockanaal 802.11a"
RECOMMENDED_BAND             = "Ad-hoc standaard draadloze modus"
IBSS_TX_POWER_STR            = "Verzendenergie"
ROAMING_AGGRESSIVENESS_STR   = "Agressiviteit bij roamen"
ADHOC_POWER_MANAGEMENT_STR   = "Energiebeheer ad-hocverbindingen"
ADHOC_QOS_MODE_STR           = "Ad-hoc QoS-modus"
MIXED_MODE_PROTECTION_STR    = "Beveiliging van gemengde modus"
THROUGHPUT_ENHANCEMENT_STR   = "Verbetering van  doorvoer"
WIRELESS_MODE_STR            = "802.11a/b/g draadloze modus"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2,4 GHz 802.11b"
WIRELESS_MODE_G              = "2,4 GHz 802.11g"
WIRELESS_MODE_BG             = "2,4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Dual-band 802.11a/g"
WIRELESS_MODE_ABG            = "Dual-band 802.11a/b/g"
PREFERRED_BAND_STR           = "Voorkeursband"
CHANNELWIDTH52               = "Kanaalbreedte voor 5 GHz"
CHANNELWIDTH6                = "Kanaalbreedte voor 6 GHz"
CHANNELWIDTH24               = "Kanaalbreedte voor 2,4 GHz"
TGnMode                      = "802.11n draadloze modus"
11N_AC_MODE                  = "802.11n/ac draadloze modus"
11N_AX_MODE                  = "802.11n/ac/ax draadloze modus"
11N_BE_MODE                  = "802.11n/ac/ax/be draadloze modus"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Niet compatibel met 40-Mhz kanaal"
LOWEST_STR                   = "Laagste"
MEDIUM_LOW_STR               = "Laag"
MEDIUM_STR                   = "Normaal"
MEDIUM_HIGH_STR              = "Hoog"
HIGHEST_STR                  = "Hoogste"
DISABLED_STR                 = "Uitgeschakeld"
ENABLED_STR                  = "Ingeschakeld"
MAXIMUM_POWER_SAVING_STR     = "Maximale energiebesparing"
NOISY_ENVIRONMENT_STR        = "Omgeving met ruis"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "CTS-naar-zelf ingeschakeld"
RTS_CTS_ENABLED_STR          = "RTS/CTS ingeschakeld"
AUTO_STR                     = "Automatisch"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "Automatisch"
WMM_DISABLED_STR             = "WMM uitgeschakeld"
WMM_ENABLED_STR              = "WMM ingeschakeld"
NO_PREFERECE_STR             = "Geen voorkeur"
PREFER_24_BAND_STR           = "Voorkeur voor 2,4-GHz band"
PREFER_52_BAND_STR           = "5 GHz band"
PREFER_6_BAND_STR            = "6 GHz band"
PREFER_52_6_BAND_STR         = "Voorkeur voor 5-GHz + 6-GHz band"
WAKE_ON_MAGIC_PACKET         = "Activeren na Magic-pakket"
WAKE_ON_PATTERN_MATCH        = "patroonovereenkomst"
PM_WIFI_REKEY_OFFLOAD        = "GTK opnieuw versleutelen voor WoWLAN"
PM_ARP_OFFLOAD               = "ARP-offload voor WoWLAN"
PM_NS_OFFLOAD                = "NS-offload voor WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Slapen bij verbroken WoWLAN-verbinding"
PACKET_COALESCING            = "Pakketsamenvoeging"
U_APSD_SUPPORT               = "U-APSD ondersteuning"
THROUGHPUTBOOSTER_STR        = "Throughput booster"
MIMO_POWER_SAVE_MODE_STR     = "MIMO energiebesparende stand"
MIMO_AUTO_STR                = "Automatische SMPS"
NO_MIMO_STR                  = "Statische SMPS"
RTS_BEFORE_MIMO_STR          = "Dynamische SMPS"
NO_RTS_BEFORE_MIMO_STR       = "Geen SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "Double Connect technologie"
SOURCEDISK1                  = "Installatieschijf voor Intel(R) Wireless"
UHB_BAND_SUPPORTED_STR       = "Ultra High Band (6 GHz)"
HUMAN_PRESENCE_DETECTION_STR = "Detectie van personen"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Norwegian Bokmål (Norway)
[Strings.0414]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Intel(R) Wireless kortdriver for Windows 10 64-bit"
RECOMMENDED_CHANNEL24_STR    = "Ad Hoc-kanal 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Ad Hoc-kanal 802.11a"
RECOMMENDED_BAND             = "Ad hoc standard trådløsmodus"
IBSS_TX_POWER_STR            = "Overføringsstrøm"
ROAMING_AGGRESSIVENESS_STR   = "Streifingsaggresjon"
ADHOC_POWER_MANAGEMENT_STR   = "Ad Hoc strømstyring"
ADHOC_QOS_MODE_STR           = "Ad Hoc QoS modus"
MIXED_MODE_PROTECTION_STR    = "Blandet modus-beskyttelse"
THROUGHPUT_ENHANCEMENT_STR   = "Gjennomstrømningsutvidelse"
WIRELESS_MODE_STR            = "802.11a/b/g trådløsmodus"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2,4 GHz 802.11b"
WIRELESS_MODE_G              = "2,4 GHz 802.11g"
WIRELESS_MODE_BG             = "2,4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Tobånds 802.11a/g"
WIRELESS_MODE_ABG            = "Tobånds 802.11a/b/g"
PREFERRED_BAND_STR           = "Foretrukket bånd"
CHANNELWIDTH52               = "Kanalbredde for 5 GHz"
CHANNELWIDTH6                = "Kanalbredde for 6 GHz"
CHANNELWIDTH24               = "Kanalbredde for 2,4 GHz"
TGnMode                      = "802.11n trådløsmodus"
11N_AC_MODE                  = "802.11n/ac trådløsmodus"
11N_AX_MODE                  = "802.11n/ac/ax trådløsmodus"
11N_BE_MODE                  = "802.11n/ac/ax/be trådløsmodus"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Intolerant for kanal"
LOWEST_STR                   = "Laveste"
MEDIUM_LOW_STR               = "Middels-lav"
MEDIUM_STR                   = "Middels"
MEDIUM_HIGH_STR              = "Middels-høy"
HIGHEST_STR                  = "Høyeste"
DISABLED_STR                 = "Deaktivert"
ENABLED_STR                  = "Aktivert"
MAXIMUM_POWER_SAVING_STR     = "Maksimal strømsparing"
NOISY_ENVIRONMENT_STR        = "Støyende miljø"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "CTS-til-selv aktivert"
RTS_CTS_ENABLED_STR          = "RTS/CTS-aktivert"
AUTO_STR                     = "Automatisk"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "Automatisk"
WMM_DISABLED_STR             = "WMM deaktivert"
WMM_ENABLED_STR              = "WMM aktivert"
NO_PREFERECE_STR             = "Ingen preferanser"
PREFER_24_BAND_STR           = "Foretrekk 2,4 GHz-bånd"
PREFER_52_BAND_STR           = "Foretrekke 5 GHz-bånd"
PREFER_6_BAND_STR            = "Foretrekke 6 GHz-bånd"
PREFER_52_6_BAND_STR         = "Foretrekk 5 GHz- + 6 GHz-båndet"
WAKE_ON_MAGIC_PACKET         = "Reaktivert etter magisk pakke"
WAKE_ON_PATTERN_MATCH        = "Reaktivert etter samsvarende mønster"
PM_WIFI_REKEY_OFFLOAD        = "GTK-omnøkling for WoWLAN"
PM_ARP_OFFLOAD               = "ARP-avlastning for WoWLAN"
PM_NS_OFFLOAD                = "NS-avlastning for WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Hvilemodus ved WoWLAN-frakobling"
PACKET_COALESCING            = "Pakkeoppsamling"
U_APSD_SUPPORT               = "Støtte for U-APSD:"
THROUGHPUTBOOSTER_STR        = "Gjennomstrømmings-Booster"
MIMO_POWER_SAVE_MODE_STR     = "MIMO-strømsparingsmodus"
MIMO_AUTO_STR                = "Auto-SMPS"
NO_MIMO_STR                  = "Statisk SMPS"
RTS_BEFORE_MIMO_STR          = "Dynamisk SMPS"
NO_RTS_BEFORE_MIMO_STR       = "Ingen SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "Teknologi for dobbel tilkobling"
SOURCEDISK1                  = "Installasjonsplate for Intel(R) Wireless"
UHB_BAND_SUPPORTED_STR       = "Ultra High Band (6GHz)"
HUMAN_PRESENCE_DETECTION_STR = "Deteksjon av menneskelig tilstedeværelse"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Polish (Poland)
[Strings.0415]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Sterownik karty Intel(R) Wireless dla systemu Windows 10 64 Bit"
RECOMMENDED_CHANNEL24_STR    = "Kanał Ad Hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Kanał Ad Hoc 802.11a"
RECOMMENDED_BAND             = "Domyślny tryb sieci bezprzewodowej Ad Hoc"
IBSS_TX_POWER_STR            = "Moc transmisji"
ROAMING_AGGRESSIVENESS_STR   = "Agresywność mobilności"
ADHOC_POWER_MANAGEMENT_STR   = "Zarządzanie energią w sieci Ad Hoc"
ADHOC_QOS_MODE_STR           = "Tryb Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR    = "Ochrona trybu mieszanego"
THROUGHPUT_ENHANCEMENT_STR   = "Rozszerzenie przepływności"
WIRELESS_MODE_STR            = "Tryb bezprzewodowy 802.11a/b/g"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2,4 GHz 802.11b"
WIRELESS_MODE_G              = "2,4 GHz 802.11g"
WIRELESS_MODE_BG             = "2,4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Dual Band 802.11a/g"
WIRELESS_MODE_ABG            = "Dual Band 802.11a/b/g"
PREFERRED_BAND_STR           = "Pasmo preferowane"
CHANNELWIDTH52               = "Szerokość kanału dla 5 GHz"
CHANNELWIDTH6                = "Szerokość kanału dla 6 GHz"
CHANNELWIDTH24               = "Szerokość kanału dla 2,4 GHz"
TGnMode                      = "Tryb bezprzewodowy 802.11n"
11N_AC_MODE                  = "Tryb bezprzewodowy 802.11n/ac"
11N_AX_MODE                  = "Tryb bezprzewodowy 802.11n/ac/ax"
11N_BE_MODE                  = "Tryb bezprzewodowy 802.11n/ac/ax/be"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Brak tolerancji dla kanału 40 MHz"
LOWEST_STR                   = "Najniższa"
MEDIUM_LOW_STR               = "Średnio-niska"
MEDIUM_STR                   = "Średnia"
MEDIUM_HIGH_STR              = "Średnio-wysoka"
HIGHEST_STR                  = "Najwyższa"
DISABLED_STR                 = "Wyłączono"
ENABLED_STR                  = "Włączono"
MAXIMUM_POWER_SAVING_STR     = "Maks. oszczędność energii"
NOISY_ENVIRONMENT_STR        = "Środowisko z zakłóceniami"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "Włączony zwrotny CTS"
RTS_CTS_ENABLED_STR          = "Włączony RTS/CTS"
AUTO_STR                     = "Automatyczny"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "Automatyczny"
WMM_DISABLED_STR             = "Wyłączono WMM"
WMM_ENABLED_STR              = "Włączono WMM"
NO_PREFERECE_STR             = "Bez preferencji"
PREFER_24_BAND_STR           = "Preferowany pasmo 2,4 GHz"
PREFER_52_BAND_STR           = "Preferuj Pasmo 5 GHz"
PREFER_6_BAND_STR            = "Preferuj Pasmo 6 GHz"
PREFER_52_6_BAND_STR         = "Preferuj pasmo 5 GHz + 6 GHz"
WAKE_ON_MAGIC_PACKET         = "Wznawianie na podstawie pakietu Magic"
WAKE_ON_PATTERN_MATCH        = "Wznawianie na podstawie dopasowania do wzorca"
PM_WIFI_REKEY_OFFLOAD        = "GTK tworzy klucze ponowne dla WoWLAN"
PM_ARP_OFFLOAD               = "Odciążanie ARP dla WoWLAN"
PM_NS_OFFLOAD                = "Odciążanie NS dla WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Uśpienie WoWLAN Disconnect"
PACKET_COALESCING            = "Łączenie pakietów"
U_APSD_SUPPORT               = "Obsługa funkcji U-APSD"
THROUGHPUTBOOSTER_STR        = "Przyśpieszacz przepustowości"
MIMO_POWER_SAVE_MODE_STR     = "Tryb oszczędzania energii MIMO"
MIMO_AUTO_STR                = "Automatyczna funkcja SMPS"
NO_MIMO_STR                  = "Statyczna funkcja SMPS"
RTS_BEFORE_MIMO_STR          = "Dynamiczna funkcja SMPS"
NO_RTS_BEFORE_MIMO_STR       = "Brak funkcji SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "Technologia podwójnego połączenia"
SOURCEDISK1                  = "Dysk instalacyjny Intel(R) Wireless"
UHB_BAND_SUPPORTED_STR       = "Ultrawysokie pasmo (6 GHz)"
HUMAN_PRESENCE_DETECTION_STR = "Wykrywanie obecności człowieka"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Portuguese (Brazil)
[Strings.0416]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Driver do adaptador Intel(R) Wireless para Windows 10 64 bits"
RECOMMENDED_CHANNEL24_STR    = "Canal ad-hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Canal ad-hoc 802.11a"
RECOMMENDED_BAND             = "Modo sem fio padrão ad-hoc"
IBSS_TX_POWER_STR            = "Potência de transmissão"
ROAMING_AGGRESSIVENESS_STR   = "Agressividade de roaming"
ADHOC_POWER_MANAGEMENT_STR   = "Gerenciamento de energia ad-hoc"
ADHOC_QOS_MODE_STR           = "Modo QoS Ad-hoc"
MIXED_MODE_PROTECTION_STR    = "Proteção de modo misto"
THROUGHPUT_ENHANCEMENT_STR   = "Aumento da taxa de transferência"
WIRELESS_MODE_STR            = "Modo sem fio 802.11a/b/g"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2,4 GHz 802.11b"
WIRELESS_MODE_G              = "2,4 GHz 802.11g"
WIRELESS_MODE_BG             = "2,4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Banda Dupla 802.11a/g"
WIRELESS_MODE_ABG            = "Banda Dupla 802.11a/b/g"
PREFERRED_BAND_STR           = "Banda preferencial"
CHANNELWIDTH52               = "Largura do canal para 5 GHz"
CHANNELWIDTH6                = "Largura do canal para 6 GHz"
CHANNELWIDTH24               = "Largura do canal para 2,4 GHz"
TGnMode                      = "Modo sem fio 802.11n"
11N_AC_MODE                  = "Modo sem fio 802.11n/ac"
11N_AX_MODE                  = "Modo sem fio 802.11n/ac/ax"
11N_BE_MODE                  = "Modo sem fio 802.11n/ac/ax/be"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Sem tolerância a canal FAT"
LOWEST_STR                   = "Mais baixo"
MEDIUM_LOW_STR               = "Média a baixa"
MEDIUM_STR                   = "Média"
MEDIUM_HIGH_STR              = "Média a alta"
HIGHEST_STR                  = "Mais alto"
DISABLED_STR                 = "Desabilitado"
ENABLED_STR                  = "Habilitado"
MAXIMUM_POWER_SAVING_STR     = "Economia máx. de energia"
NOISY_ENVIRONMENT_STR        = "Ambiente ruidoso"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "CTS auto-ativação ativado"
RTS_CTS_ENABLED_STR          = "RTS/CTS ativado"
AUTO_STR                     = "Auto"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "Auto"
WMM_DISABLED_STR             = "WMM Desativado"
WMM_ENABLED_STR              = "WMM Ativado"
NO_PREFERECE_STR             = "Sem preferência"
PREFER_24_BAND_STR           = "Preferir banda de 2,4 GHz"
PREFER_52_BAND_STR           = "Preferir banda de 5 GHz"
PREFER_6_BAND_STR            = "Preferir banda de 6 GHz"
PREFER_52_6_BAND_STR         = "Preferir banda de 5 GHz + 6 GHz"
WAKE_ON_MAGIC_PACKET         = "Pacote Mágico do Wake on"
WAKE_ON_PATTERN_MATCH        = "Correspondência de padrão do Wake on"
PM_WIFI_REKEY_OFFLOAD        = "Nova geração de chaves GTK para WoWLAN"
PM_ARP_OFFLOAD               = "Descarregamento ARP para WoWLAN"
PM_NS_OFFLOAD                = "Descarregamento NS para WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Suspender desconexão de WoWLAN"
PACKET_COALESCING            = "União de pacote"
U_APSD_SUPPORT               = "Suporte para U-APSD"
THROUGHPUTBOOSTER_STR        = "Impulsionador do throughput"
MIMO_POWER_SAVE_MODE_STR     = "MIMO - Modo de Economia de Energia"
MIMO_AUTO_STR                = "SMPS automático"
NO_MIMO_STR                  = "Estático SMPS"
RTS_BEFORE_MIMO_STR          = "SMPS dinâmico"
NO_RTS_BEFORE_MIMO_STR       = "Sem SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "Tecnologia de conexão dupla"
SOURCEDISK1                  = "Disco da instalação do Intel(R) Wireless"
UHB_BAND_SUPPORTED_STR       = "Banda Ultra Alta (6 GHz)"
HUMAN_PRESENCE_DETECTION_STR = "Detecção de presença humana"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Portuguese (Portugal)
[Strings.0816]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Controlador da placa Intel(R) Wireless para Windows 10 64 Bits"
RECOMMENDED_CHANNEL24_STR    = "Canal ad hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Canal ad hoc 802.11a"
RECOMMENDED_BAND             = "Modo ad hoc sem fios predefinido"
IBSS_TX_POWER_STR            = "Potência de transmissão"
ROAMING_AGGRESSIVENESS_STR   = "Agressividade do roaming"
ADHOC_POWER_MANAGEMENT_STR   = "Gestão de energia ad hoc"
ADHOC_QOS_MODE_STR           = "Modo Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR    = "Protecção do modo misto"
THROUGHPUT_ENHANCEMENT_STR   = "Melhoria da produtividade"
WIRELESS_MODE_STR            = "Modo sem fios 802.11a/b/g"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2,4 GHz 802.11b"
WIRELESS_MODE_G              = "2,4 GHz 802.11g"
WIRELESS_MODE_BG             = "2,4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Banda dupla de 802.11a/g"
WIRELESS_MODE_ABG            = "Banda dupla de 802.11a/b/g"
PREFERRED_BAND_STR           = "Banda preferida"
CHANNELWIDTH52               = "Largura do canal para 5 GHz"
CHANNELWIDTH6                = "Largura do canal para 6 GHz"
CHANNELWIDTH24               = "Largura do canal para 2,4 GHz"
TGnMode                      = "Modo sem fios 802.11n"
11N_AC_MODE                  = "Modo sem fios 802.11n/ac"
11N_AX_MODE                  = "Modo sem fios 802.11n/ac/ax"
11N_BE_MODE                  = "Modo sem fios 802.11n/ac/ax/be"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Canal de grandes volumes incompatível"
LOWEST_STR                   = "Menor"
MEDIUM_LOW_STR               = "Média-baixa"
MEDIUM_STR                   = "Média"
MEDIUM_HIGH_STR              = "Média-Elevada"
HIGHEST_STR                  = "Maior"
DISABLED_STR                 = "Desactivado"
ENABLED_STR                  = "Activado"
MAXIMUM_POWER_SAVING_STR     = "Máxima poupança de energia"
NOISY_ENVIRONMENT_STR        = "Ambiente ruidoso"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "CTS-to-self activado"
RTS_CTS_ENABLED_STR          = "RTS/CTS Activado"
AUTO_STR                     = "Auto"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "Auto"
WMM_DISABLED_STR             = "WMM desactivado"
WMM_ENABLED_STR              = "WMM activado"
NO_PREFERECE_STR             = "Sem Preferência"
PREFER_24_BAND_STR           = "Preferir banda de 2,4 GHz"
PREFER_52_BAND_STR           = "Preferir banda de 5 GHz"
PREFER_6_BAND_STR            = "Preferir banda de 6 GHz"
PREFER_52_6_BAND_STR         = "Preferir banda de 5 GHz e 6 GHz"
WAKE_ON_MAGIC_PACKET         = "Reactivação por Magic Packet"
WAKE_ON_PATTERN_MATCH        = "Correspondência de padrão do Wake on"
PM_WIFI_REKEY_OFFLOAD        = "Regeração de chaves GTK para WoWLAN"
PM_ARP_OFFLOAD               = "Descarga ARP para WoWLAN"
PM_NS_OFFLOAD                = "Descarga NS para WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Suspender quando a WoWLAN estiver desligada"
PACKET_COALESCING            = "União de pacote"
U_APSD_SUPPORT               = "Suporte de U-APSD"
THROUGHPUTBOOSTER_STR        = "Otimizador do rendimento"
MIMO_POWER_SAVE_MODE_STR     = "Modo de poupança de energia MIMO"
MIMO_AUTO_STR                = "SMPS automático"
NO_MIMO_STR                  = "SMPS estático"
RTS_BEFORE_MIMO_STR          = "SMPS dinâmico"
NO_RTS_BEFORE_MIMO_STR       = "Sem SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "Tecnologia de ligação dupla"
SOURCEDISK1                  = "Disco de Instalação da Intel(R) Wireless"
UHB_BAND_SUPPORTED_STR       = "Banda ultra-alta (6GHz)"
HUMAN_PRESENCE_DETECTION_STR = "Deteção de Presença Humana"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Russian (Russia)
[Strings.0419]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Драйвер адаптера Intel(R) Wireless для Windows 10 64 Bit "
RECOMMENDED_CHANNEL24_STR    = "Канал Ad Hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Канал Ad Hoc 802.11a"
RECOMMENDED_BAND             = "Режим сети Ad Hoc по умолчанию"
IBSS_TX_POWER_STR            = "Мощность передачи"
ROAMING_AGGRESSIVENESS_STR   = "Агрессивность роуминга"
ADHOC_POWER_MANAGEMENT_STR   = "Мощность передачи Ad Hoc"
ADHOC_QOS_MODE_STR           = "Режим Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR    = "Защита в смешанном режиме"
THROUGHPUT_ENHANCEMENT_STR   = "Повышенная пропуск. способность"
WIRELESS_MODE_STR            = "Режим беспроводной связи 802.11a/b/g"
WIRELESS_MODE_A              = "5 ГГц 802.11a"
WIRELESS_MODE_B              = "2,4 ГГц 802.11b"
WIRELESS_MODE_G              = "2,4 ГГц 802.11g"
WIRELESS_MODE_BG             = "2,4 ГГц 802.11b/g"
WIRELESS_MODE_AG             = "Двухдиапазонная сеть 802.11a/g"
WIRELESS_MODE_ABG            = "Двухдиапазонная сеть 802.11a/b/g"
PREFERRED_BAND_STR           = "Предпочитаемая частота"
CHANNELWIDTH52               = "Ширина канала для 5 ГГц"
CHANNELWIDTH6                = "Ширина канала для 6 ГГц"
CHANNELWIDTH24               = "Ширина канала для 2,4 ГГц"
TGnMode                      = "Режим беспроводной связи 802.11n"
11N_AC_MODE                  = "Режим беспроводной связи 802.11n/ac"
11N_AX_MODE                  = "Режим беспроводной связи 802.11n/ac/ax"
11N_BE_MODE                  = "Режим беспроводной связи 802.11n/ac/ax/be"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Несовместимость с каналом"
LOWEST_STR                   = "Мин."
MEDIUM_LOW_STR               = "Средн.-мин."
MEDIUM_STR                   = "Средн."
MEDIUM_HIGH_STR              = "Средн.-макс."
HIGHEST_STR                  = "Макс."
DISABLED_STR                 = "Выключено"
ENABLED_STR                  = "Включено"
MAXIMUM_POWER_SAVING_STR     = "Макс. экономия энергии"
NOISY_ENVIRONMENT_STR        = "Условия с помехами"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "CTS-to-self включено"
RTS_CTS_ENABLED_STR          = "RTS/CTS включено"
AUTO_STR                     = "Авто"
CHANNELWIDTH20ONLY           = "20 МГц"
CHANNELWIDTHAUTO             = "Авто"
WMM_DISABLED_STR             = "WMM Выключено"
WMM_ENABLED_STR              = "WMM Включено"
NO_PREFERECE_STR             = "Нет предпочтений"
PREFER_24_BAND_STR           = "Предпочитать частоту 2,4 ГГц"
PREFER_52_BAND_STR           = "диапазон 5 ГГц предпочтительней."
PREFER_6_BAND_STR            = "диапазон 6 ГГц предпочтительней."
PREFER_52_6_BAND_STR         = "Предпочитать диапазон 5 ГГц + 6 ГГц"
WAKE_ON_MAGIC_PACKET         = "Пробуждение пакетом Magic Packet"
WAKE_ON_PATTERN_MATCH        = "Пробуждение при соответствии шаблону"
PM_WIFI_REKEY_OFFLOAD        = "Повторный ввод ключа GTK для режима пробуждения Wake on Wireless LAN"
PM_ARP_OFFLOAD               = "Выгрузка ARP для режима пробуждения Wake on Wireless LAN"
PM_NS_OFFLOAD                = "Выгрузка NS для режима пробуждения Wake on Wireless LAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Переход в состояние сна при отключении режима пробуждения Wake on Wireless LAN"
PACKET_COALESCING            = "Объединение пакетов"
U_APSD_SUPPORT               = "Поддержка U-APSD"
THROUGHPUTBOOSTER_STR        = "Увеличение пропускной способности"
MIMO_POWER_SAVE_MODE_STR     = "Режим энергосбережения MIMO"
MIMO_AUTO_STR                = "Авто SMPS"
NO_MIMO_STR                  = "Статический SMPS"
RTS_BEFORE_MIMO_STR          = "Динамический SMPS"
NO_RTS_BEFORE_MIMO_STR       = "Нет SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "Технология двойного соединения"
SOURCEDISK1                  = "Установочный диск адаптера Intel(R) Wireless"
UHB_BAND_SUPPORTED_STR       = "Сверхвысокий диапазон частот (6 ГГц)"
HUMAN_PRESENCE_DETECTION_STR = "Обнаружение присутствия человека"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Swedish (Sweden)
[Strings.041D]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Kortdrivrutin för Windows 10 64-bitars Intel(R) Wireless"
RECOMMENDED_CHANNEL24_STR    = "Ad hoc-kanal 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Ad hoc-kanal 802.11a"
RECOMMENDED_BAND             = "Ad hoc Standard trådlöst läge"
IBSS_TX_POWER_STR            = "Överföringsenergi"
ROAMING_AGGRESSIVENESS_STR   = "Roaming-aggressivitet"
ADHOC_POWER_MANAGEMENT_STR   = "Energisparfunktioner för ad hoc"
ADHOC_QOS_MODE_STR           = "Ad Hoc QoS-läge"
MIXED_MODE_PROTECTION_STR    = "Skydd för blandat läge"
THROUGHPUT_ENHANCEMENT_STR   = "Genomflödesförbättring"
WIRELESS_MODE_STR            = "802.11a/b/g Trådlöst läge"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2,4 GHz 802.11b"
WIRELESS_MODE_G              = "2,4 GHz 802.11g"
WIRELESS_MODE_BG             = "2,4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Dual Band 802.11a/g"
WIRELESS_MODE_ABG            = "Dual Band 802.11a/b/g"
PREFERRED_BAND_STR           = "Förvalt band"
CHANNELWIDTH52               = "Kanalbredd för 5 GHz"
CHANNELWIDTH6                = "Kanalbredd för 6 GHz"
CHANNELWIDTH24               = "Kanalbredd för 2,4 GHz"
TGnMode                      = "802.11n Trådlöst läge"
11N_AC_MODE                  = "802.11n/ac Trådlöst läge"
11N_AX_MODE                  = "802.11n/ac/ax Trådlöst läge"
11N_BE_MODE                  = "802.11n/ac/ax/be Trådlöst läge"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Inkompatibel med 40 MHz-kanal"
LOWEST_STR                   = "Lägsta"
MEDIUM_LOW_STR               = "Medel-låg"
MEDIUM_STR                   = "Medel"
MEDIUM_HIGH_STR              = "Medel-hög"
HIGHEST_STR                  = "Högsta"
DISABLED_STR                 = "Inaktiverad"
ENABLED_STR                  = "Aktiverad"
MAXIMUM_POWER_SAVING_STR     = "Max. energibesparing"
NOISY_ENVIRONMENT_STR        = "Miljö med störningar"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "CTS-till-själv aktiverat"
RTS_CTS_ENABLED_STR          = "RTS/CTS aktiverat"
AUTO_STR                     = "Auto"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "Auto"
WMM_DISABLED_STR             = "WMM inaktiverad"
WMM_ENABLED_STR              = "WMM aktiverad"
NO_PREFERECE_STR             = "Ingen inställning"
PREFER_24_BAND_STR           = "Föredra 2,4 GHz-bandet"
PREFER_52_BAND_STR           = "Föredrar 5 GHz-bandet"
PREFER_6_BAND_STR            = "Föredrar 6 GHz-bandet"
PREFER_52_6_BAND_STR         = "5 GHz + 6 GHz-bandet föredras"
WAKE_ON_MAGIC_PACKET         = "Aktivera vid Magic Packet"
WAKE_ON_PATTERN_MATCH        = "Aktivering vid mönstermatchning"
PM_WIFI_REKEY_OFFLOAD        = "GTK-nyckeluppdatering för WoWLAN"
PM_ARP_OFFLOAD               = "ARP-avbelastning för WoWLAN"
PM_NS_OFFLOAD                = "NS-avbelastning för WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Viloläge vid WoWLAN-frånkoppling"
PACKET_COALESCING            = "Paketsammanslagning"
U_APSD_SUPPORT               = "Support för U-APSD"
THROUGHPUTBOOSTER_STR        = "Genomflödesbooster"
MIMO_POWER_SAVE_MODE_STR     = "MIMO - Energisparläge"
MIMO_AUTO_STR                = "Auto SMPS"
NO_MIMO_STR                  = "Statisk SMPS"
RTS_BEFORE_MIMO_STR          = "Dynamisk SMPS"
NO_RTS_BEFORE_MIMO_STR       = "Ingen SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "Teknologi för dubbla anslutningar"
SOURCEDISK1                  = "Installationsdisk Intel(R) Wireless"
UHB_BAND_SUPPORTED_STR       = "Ultrahögt band (6 GHz)"
HUMAN_PRESENCE_DETECTION_STR = "Detektering av mänsklig närvaro"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Thai (Thailand)
[Strings.041E]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "ไดรเวอร์อแด็ปเตอร์ Intel(R) Wireless สำหรับ Windows 10 64 บิต"
RECOMMENDED_CHANNEL24_STR    = "แชนแนลเฉพาะกิจ 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "แชนแนลเฉพาะกิจ 802.11a"
RECOMMENDED_BAND             = "โหมดไร้สายเริ่มต้นแบบเฉพาะกิจ"
IBSS_TX_POWER_STR            = "การส่งผ่านพลังงาน"
ROAMING_AGGRESSIVENESS_STR   = "ความแรงในการใช้งานข้ามเขต"
ADHOC_POWER_MANAGEMENT_STR   = "การจัดการพลังงานเฉพาะกิจ"
ADHOC_QOS_MODE_STR           = "โหมด QoS เฉพาะกิจ"
MIXED_MODE_PROTECTION_STR    = "การป้องกันโหมดผสม"
THROUGHPUT_ENHANCEMENT_STR   = "การเพิ่มประสิทธิภาพอัตรารับส่ง"
WIRELESS_MODE_STR            = "โหมดไร้สาย 802.11a/b/g"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2.4 GHz 802.11b"
WIRELESS_MODE_G              = "2.4 GHz 802.11g"
WIRELESS_MODE_BG             = "2.4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Dual Band 802.11a/g"
WIRELESS_MODE_ABG            = "Dual Band 802.11a/b/g"
PREFERRED_BAND_STR           = "แบนด์ที่ต้องการ"
CHANNELWIDTH52               = "ความกว้างช่องสัญญาณสำหรับ 5GHz"
CHANNELWIDTH6                = "ความกว้างช่องสัญญาณสำหรับ 6GHz"
CHANNELWIDTH24               = "ความกว้างช่องสัญญาณสำหรับ 2.4GHz"
TGnMode                      = "โหมดไร้สาย 802.11n"
11N_AC_MODE                  = "โหมดไร้สาย 802.11n/ac"
11N_AX_MODE                  = "โหมดไร้สาย 802.11n/ac/ax"
11N_BE_MODE                  = "โหมดไร้สาย 802.11n/ac/ax/be"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "ไม่สามารถใช้กับแชนแนลขนาดใหญ่"
LOWEST_STR                   = "ต่ำสุด"
MEDIUM_LOW_STR               = "ปานกลาง-ต่ำ"
MEDIUM_STR                   = "ปานกลาง"
MEDIUM_HIGH_STR              = "ปานกลาง-สูง"
HIGHEST_STR                  = "สูงสุด"
DISABLED_STR                 = "ยกเลิกใช้งาน"
ENABLED_STR                  = "เปิดการใช้งาน"
MAXIMUM_POWER_SAVING_STR     = "การประหยัดพลังงานสูงสุด"
NOISY_ENVIRONMENT_STR        = "สภาพแวดล้อมที่มีเสียงดัง"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "ใช้งาน CTS-to-self แล้ว"
RTS_CTS_ENABLED_STR          = "ใช้งาน RTS/CTS"
AUTO_STR                     = "อัตโนมัติ"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "อัตโนมัติ"
WMM_DISABLED_STR             = "ยกเลิกการใช้งาน WMM"
WMM_ENABLED_STR              = "เปิดการใช้งาน WMM"
NO_PREFERECE_STR             = "ไม่มีการกำหนด"
PREFER_24_BAND_STR           = "แบนด์ 2.4 GHz"
PREFER_52_BAND_STR           = "ชอบแบนด์ 5 GHz"
PREFER_6_BAND_STR            = "ชอบแบนด์ 6 GHz"
PREFER_52_6_BAND_STR         = "ต้องการแบนด์ 5 GHz + 6 GHz"
WAKE_ON_MAGIC_PACKET         = "Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH        = "Wake on Pattern Match"
PM_WIFI_REKEY_OFFLOAD        = "GTK กำลังกำหนดคีย์ใหม่สำหรับ WoWLAN"
PM_ARP_OFFLOAD               = "ARP ออฟโหลดสำหรับ WoWLAN"
PM_NS_OFFLOAD                = "NS ออฟโหลดสำหรับ WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "ยกเลิกการเชื่อมต่อสลีปบน WoWLAN"
PACKET_COALESCING            = "การรวมแพคเก็ต"
U_APSD_SUPPORT               = "การสนับสนุน U-APSD"
THROUGHPUTBOOSTER_STR        = "ตัวเพิ่มอัตรารับส่ง"
MIMO_POWER_SAVE_MODE_STR     = "โหมดประหยัดพลังงานMIMO"
MIMO_AUTO_STR                = "SMPSอัตโนมัติ"
NO_MIMO_STR                  = "SMPSค่าคงที่"
RTS_BEFORE_MIMO_STR          = "SMPSความเคลื่อนไหว"
NO_RTS_BEFORE_MIMO_STR       = "ไม่มีSMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "เทคโนโลยีการเชื่อมต่อในสองช่องทาง"
SOURCEDISK1                  = "ดิสก์ติดตั้ง Intel(R) Wireless"
UHB_BAND_SUPPORTED_STR       = "Ultra High Band (6GHz)"
HUMAN_PRESENCE_DETECTION_STR = "การตรวจจับเมื่อมีคนอยู่ใกล้"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Turkish (Türkiye)
[Strings.041F]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Windows 10 64 Bit için Intel(R) Wireless Bağdaştırıcı Sürücüsü "
RECOMMENDED_CHANNEL24_STR    = "Aygıttan Aygıta Kanal 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Aygıttan Aygıta Kanal 802.11a"
RECOMMENDED_BAND             = "Ad Hoc Varsayılan Bağlantı Modu"
IBSS_TX_POWER_STR            = "Yayın gücü"
ROAMING_AGGRESSIVENESS_STR   = "Gezinme Zorlaması"
ADHOC_POWER_MANAGEMENT_STR   = "Aygıttan Aygıta Güç Yönetimi"
ADHOC_QOS_MODE_STR           = "Aygıttan Aygıta QoS Modu"
MIXED_MODE_PROTECTION_STR    = "Karışık mod koruması"
THROUGHPUT_ENHANCEMENT_STR   = "Veri Aktarım Geliştirici"
WIRELESS_MODE_STR            = "802.11a/b/g Kablosuz Ağ Modu"
WIRELESS_MODE_A              = "5 GHz 802.11a"
WIRELESS_MODE_B              = "2,4 GHz 802.11b"
WIRELESS_MODE_G              = "2,4 GHz 802.11g"
WIRELESS_MODE_BG             = "2,4 GHz 802.11b/g"
WIRELESS_MODE_AG             = "Çift Bant 802.11a/g"
WIRELESS_MODE_ABG            = "Çift Bant 802.11a/b/g"
PREFERRED_BAND_STR           = "Yeğlenen Bant"
CHANNELWIDTH52               = "5 GHz İçin Kanal Genişliği"
CHANNELWIDTH6                = "6 GHz İçin Kanal Genişliği"
CHANNELWIDTH24               = "2,4 GHz İçin Kanal Genişliği"
TGnMode                      = "802.11n Kablosuz Ağ Modu"
11N_AC_MODE                  = "802.11n/ac Kablosuz Ağ Modu"
11N_AX_MODE                  = "802.11n/ac/ax Kablosuz Ağ Modu"
11N_BE_MODE                  = "802.11n/ac/ax/be Kablosuz Ağ Modu"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Geniş Kanal için Uyumsuz"
LOWEST_STR                   = "En düşük"
MEDIUM_LOW_STR               = "Düşük"
MEDIUM_STR                   = "Orta"
MEDIUM_HIGH_STR              = "Yüksek"
HIGHEST_STR                  = "En yüksek"
DISABLED_STR                 = "Devre dışı"
ENABLED_STR                  = "Etkin"
MAXIMUM_POWER_SAVING_STR     = "Azami Güç Tasarrufu"
NOISY_ENVIRONMENT_STR        = "Gürültülü Ortam"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "CTS-to-self etkin"
RTS_CTS_ENABLED_STR          = "RTS/CTS etkin"
AUTO_STR                     = "Otomatik"
CHANNELWIDTH20ONLY           = "20 MHz"
CHANNELWIDTHAUTO             = "Otomatik"
WMM_DISABLED_STR             = "WMM devre dışı"
WMM_ENABLED_STR              = "WMM etkin"
NO_PREFERECE_STR             = "Tercih yok"
PREFER_24_BAND_STR           = "2,4 GHz bant Tercih Et"
PREFER_52_BAND_STR           = "5 GHz bant Tercih Et"
PREFER_6_BAND_STR            = "6 GHz bant Tercih Et"
PREFER_52_6_BAND_STR         = "5 GHz + 6 GHz bandı tercih et"
WAKE_ON_MAGIC_PACKET         = "Sihirli Paket Uyanması"
WAKE_ON_PATTERN_MATCH        = "Desen eşleştirme uyanması"
PM_WIFI_REKEY_OFFLOAD        = "WoWLAN için GTK yeniden anahtarlama"
PM_ARP_OFFLOAD               = "WoWLAN için ARP yük boşaltma"
PM_NS_OFFLOAD                = "WoWLAN için NS yük boşaltma"
DEVICE_SLEEP_ON_DISCONNECT   = "WoWLAN Bağlantı Kesintisinde uyku durumuna geç"
PACKET_COALESCING            = "Paket Birleştirme"
U_APSD_SUPPORT               = "U-APSD Desteği"
THROUGHPUTBOOSTER_STR        = "Verimlilik Arttırıcı"
MIMO_POWER_SAVE_MODE_STR     = "MIMO Güç Tasarrufu Modu"
MIMO_AUTO_STR                = "Otomatik SMPS"
NO_MIMO_STR                  = "Statik SMPS"
RTS_BEFORE_MIMO_STR          = "Dinamik SMPS"
NO_RTS_BEFORE_MIMO_STR       = "SMPS Yok"
DOUBLECONNECTTECHNOLOGY_STR  = "Çift Bağlantı Teknolojisi"
SOURCEDISK1                  = "Intel(R) Wireless Yükleme Diski"
UHB_BAND_SUPPORTED_STR       = "Ultra Yüksek Bant Genişliği (6 GHz)"
HUMAN_PRESENCE_DETECTION_STR = "İnsan Varlığı Algılama"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"

; Ukrainian (Ukraine)
[Strings.0422]
NIC_1650i_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650i 160MHz Wireless Network Adapter (201NGW)"
NIC_1650s_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650s 160MHz Wireless Network Adapter (201D2W)"
NIC_203_2x2_AX_no_160        = "Intel(R) Wi-Fi 6 AX203"
NIC_101_1x1_AX_no_160        = "Intel(R) Wi-Fi 6 AX101"
NIC_201_2x2_AX               = "Intel(R) Wi-Fi 6 AX201 160MHz"
PROVIDER_NAME                = "Intel"
COMPANY_NAME                 = "Intel Corporation"
NIC_Service_DispName_WINT_64 = "Драйвер адаптера бездротового зв’язку Intel(R) для ОС Windows 10 (64-розрядна версія)"
RECOMMENDED_CHANNEL24_STR    = "Канал прямого мережевого підключення 802.11b/g"
RECOMMENDED_CHANNEL52_STR    = "Канал прямого мережевого підключення 802.11a"
RECOMMENDED_BAND             = "Стандартний режим бездротового зв’язку"
IBSS_TX_POWER_STR            = "Потужність передачі сигналу"
ROAMING_AGGRESSIVENESS_STR   = "Агресивність роумінгу"
ADHOC_POWER_MANAGEMENT_STR   = "Керування живленням прямого мережевого підключення"
ADHOC_QOS_MODE_STR           = "Режим QoS прямого мережевого підключення"
MIXED_MODE_PROTECTION_STR    = "Захист у змішаному режимі"
THROUGHPUT_ENHANCEMENT_STR   = "Покращення пропускної здатності"
WIRELESS_MODE_STR            = "Бездротовий режим 802.11a/b/g"
WIRELESS_MODE_A              = "5 ГГц 802.11a"
WIRELESS_MODE_B              = "2,4 ГГц 802.11b"
WIRELESS_MODE_G              = "2,4 ГГц 802.11g"
WIRELESS_MODE_BG             = "2,4 ГГц 802.11b/g"
WIRELESS_MODE_AG             = "Дводіапазонний зв’язок 802.11a/g"
WIRELESS_MODE_ABG            = "Дводіапазонний зв’язок 802.11a/b/g"
PREFERRED_BAND_STR           = "Бажаний діапазон"
CHANNELWIDTH6                = "Ширина каналу для 6 ГГц"
CHANNELWIDTH52               = "Ширина каналу для 5 ГГц"
CHANNELWIDTH24               = "Ширина каналу для 2,4 ГГц"
TGnMode                      = "Бездротовий режим 802.11n"
11N_AC_MODE                  = "Бездротовий режим 802.11n/ac"
11N_AX_MODE                  = "Бездротовий режим 802.11n/ac/ax"
11N_BE_MODE                  = "Бездротовий режим 802.11n/ac/ax/be"
11BE_ENABLED_STR             = "802.11be"
11AX_ENABLED_STR             = "802.11ax"
VHT_ENABLED_STR              = "802.11ac"
HT_ENABLED_STR               = "802.11n"
BTHSMode                     = "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT         = "Без переваги широкого каналу"
LOWEST_STR                   = "Найнижч."
MEDIUM_LOW_STR               = "Середньо-низьк."
MEDIUM_STR                   = "Середн."
MEDIUM_HIGH_STR              = "Середньо-висок."
HIGHEST_STR                  = "Найвищ."
DISABLED_STR                 = "Вимкнуто"
ENABLED_STR                  = "Увімкнено"
MAXIMUM_POWER_SAVING_STR     = "Максимальна економія енергії"
NOISY_ENVIRONMENT_STR        = "Середовище з перешкодами"
WMM_STR                      = "WMM"
CTS_TO_SELF_ENABLED_STR      = "Функцію CTS-to-self увімкнуто"
RTS_CTS_ENABLED_STR          = "Функцію RTS/CTS увімкнуто"
AUTO_STR                     = "Автоматично"
CHANNELWIDTH20ONLY           = "Тільки 20 МГц"
CHANNELWIDTHAUTO             = "Автоматично"
WMM_DISABLED_STR             = "Функцію WMM вимкнуто"
WMM_ENABLED_STR              = "Функцію WMM увімкнуто"
NO_PREFERECE_STR             = "Без пріоритету"
PREFER_24_BAND_STR           = "У пріоритеті діапазон 2,4 ГГц"
PREFER_52_BAND_STR           = "У пріоритеті діапазон 5 ГГц"
PREFER_6_BAND_STR            = "У пріоритеті діапазон 6 ГГц"
PREFER_52_6_BAND_STR         = "У пріоритеті діапазон 5 ГГц + 6 ГГц"
WAKE_ON_MAGIC_PACKET         = "Пробудження за сигналом з локальної мережі"
WAKE_ON_PATTERN_MATCH        = "Пробудження після отримання особливого шаблону"
PM_WIFI_REKEY_OFFLOAD        = "Зміна ключа GTK для WoWLAN"
PM_ARP_OFFLOAD               = "Вивантаження ARP для WoWLAN"
PM_NS_OFFLOAD                = "Вивантаження NS для WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT   = "Перехід у режим сну у разі вимкнення WoWLAN"
PACKET_COALESCING            = "Об’єднання пакетів"
U_APSD_SUPPORT               = "Підтримка U-APSD"
THROUGHPUTBOOSTER_STR        = "Підсилювач пропускної здатності"
MIMO_POWER_SAVE_MODE_STR     = "Режим збереження енергії MIMO"
MIMO_AUTO_STR                = "Автоматичний SMPS"
NO_MIMO_STR                  = "Статичний SMPS"
RTS_BEFORE_MIMO_STR          = "Динамічний SMPS"
NO_RTS_BEFORE_MIMO_STR       = "Без SMPS"
DOUBLECONNECTTECHNOLOGY_STR  = "Технологія подвійного підключення"
SOURCEDISK1                  = "Інсталяційний диск безпровідного адаптера Intel(R)"
UHB_BAND_SUPPORTED_STR       = "Ультрависокий діапазон (6 ГГц)"
HUMAN_PRESENCE_DETECTION_STR = "Виявлення присутності людини"

NIC_1650x_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650x 160MHz Wireless Network Adapter (200NGW)"
NIC_1650w_2x2_AX             = "Killer(R) Wi-Fi 6 AX1650w 160MHz Wireless Network Adapter (200D2W)"
NIC_200_2x2_AX               = "Intel(R) Wi-Fi 6 AX200 160MHz"
NIC_1550i_2x2_AC             = "Killer(R) Wireless-AC 1550i Wireless Network Adapter (9560NGW) 160MHz"
NIC_1550s_2x2_AC             = "Killer(R) Wireless-AC 1550s Wireless Network Adapter (9560D2W) 160MHz"
NIC_9462_1x1_AC_no_160       = "Intel(R) Wireless-AC 9462"
NIC_9461_1x1_AC_no_160       = "Intel(R) Wireless-AC 9461"
NIC_9560_2x2_AC_no_160       = "Intel(R) Wireless-AC 9560"
NIC_9462_1x1_AC              = "Intel(R) Wireless-AC 9462 160MHz"
NIC_9461_1x1_AC              = "Intel(R) Wireless-AC 9461 160MHz"
NIC_9560_2x2_AC              = "Intel(R) Wireless-AC 9560 160MHz"
NIC_1550_2x2_AC              = "Killer(R) Wireless-AC 1550 Wireless Network Adapter (9260NGW) 160MHz"
NIC_9260_2x2_AC_no_160       = "Intel(R) Wireless-AC 9260"
NIC_9260_2x2_AC              = "Intel(R) Wireless-AC 9260 160MHz"


