*********************************************************************************
                            GXxMxxx EC RELEASE NOTE
*********************************************************************************
---------------------------------------------------------------------------------
2026/03/31    		     EC Version 1.18.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.18.00.000.bin		CHKSUM:0x22CD135

PD Version: 0x83 (Disable UART debug)


[Modify]
1.Update PD FW to 0x83
2.Modify TypeC Adaptor Plug In DC to AC waiting PD ready
3.EC auto Plug out disable Adaptor if TypeC Adptor Outage over 2 sec

[FanTable]
IDG_GX5MRXG_Thermal_Fan Control Table_20240426_R06.pptx

[SAPC]
SAPC_ GX4MRXL_20240429.xlsx

[ROMID]
- IDL Standard US Membraine Keyboard (IDL_STD_US.bat)
  0xFF 0xFF 0x01 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard UK Membraine Keyboard (IDL_STD_UK.bat)
  0xFF 0xFF 0x02 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard JP Membraine Keyboard (IDL_STD_JP.bat)
  0xFF 0xFF 0x03 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL XMG DE Membraine Keyboard (IDL_XMG_DE.bat)
  0x0C 0xFF 0x04 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL XMG US Membraine Keyboard (IDL_XMG_US.bat)
  0x0C 0xFF 0x01 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

- IDG Standard US/UK Membraine Keyboard (IDG_STD.bat)
  0xFF 0xFF 0xFF 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG MCJ JP Membraine Keyboard (IDG_MCJ_JP.bat)
  0x04 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG ThirdWave JP Membraine Keyboard (IDG_THW_JP.bat)
  0x08 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG XMG DE Membraine Keyboard (IDG_XMG_DE.bat)
  0x0C 0xFF 0x04 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG XMG US Membraine Keyboard (IDG_XMG_DE.bat)
  0x0C 0xFF 0x01 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2025/12/09    		     EC Version 1.17.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.17.00.000.bin		CHKSUM:0x22B91A8

PD Version: 0x94


[Modify]
1.Modify XMG Power LED
2.Support Charge Limit for PCS

[FanTable]
IDG_GX5MRXG_Thermal_Fan Control Table_20240426_R06.pptx

[SAPC]
SAPC_ GX4MRXL_20240429.xlsx

[ROMID]
- IDL Standard US Membraine Keyboard (IDL_STD_US.bat)
  0xFF 0xFF 0x01 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard UK Membraine Keyboard (IDL_STD_UK.bat)
  0xFF 0xFF 0x02 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard JP Membraine Keyboard (IDL_STD_JP.bat)
  0xFF 0xFF 0x03 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL XMG DE Membraine Keyboard (IDL_XMG_DE.bat)
  0x0C 0xFF 0x04 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL XMG US Membraine Keyboard (IDL_XMG_US.bat)
  0x0C 0xFF 0x01 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

- IDG Standard US/UK Membraine Keyboard (IDG_STD.bat)
  0xFF 0xFF 0xFF 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG MCJ JP Membraine Keyboard (IDG_MCJ_JP.bat)
  0x04 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG ThirdWave JP Membraine Keyboard (IDG_THW_JP.bat)
  0x08 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG XMG DE Membraine Keyboard (IDG_XMG_DE.bat)
  0x0C 0xFF 0x04 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG XMG US Membraine Keyboard (IDG_XMG_DE.bat)
  0x0C 0xFF 0x01 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF


---------------------------------------------------------------------------------
2024/10/28    		     EC Version 1.16.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.16.00.000.bin		CHKSUM:0x22BEB36


[Modify]
1.Support ODM customer ALTYK KB
2.Modify STD Copilot key to Copilot/Menu
3.Fix RSOC 2x calculate

[FanTable]
IDG_GX5MRXG_Thermal_Fan Control Table_20240426_R06.pptx

[SAPC]
SAPC_ GX4MRXL_20240429.xlsx

[ROMID]
- IDL Standard US Membraine Keyboard (IDL_STD_US.bat)
  0xFF 0xFF 0x01 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard UK Membraine Keyboard (IDL_STD_UK.bat)
  0xFF 0xFF 0x02 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard JP Membraine Keyboard (IDL_STD_JP.bat)
  0xFF 0xFF 0x03 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL XMG DE Membraine Keyboard (IDL_XMG_DE.bat)
  0x0C 0xFF 0x04 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL XMG US Membraine Keyboard (IDL_XMG_US.bat)
  0x0C 0xFF 0x01 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

- IDG Standard US/UK Membraine Keyboard (IDG_STD.bat)
  0xFF 0xFF 0xFF 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG MCJ JP Membraine Keyboard (IDG_MCJ_JP.bat)
  0x04 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG ThirdWave JP Membraine Keyboard (IDG_THW_JP.bat)
  0x08 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG XMG DE Membraine Keyboard (IDG_XMG_DE.bat)
  0x0C 0xFF 0x04 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG XMG US Membraine Keyboard (IDG_XMG_DE.bat)
  0x0C 0xFF 0x01 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2024/10/07    		     EC Version 1.15.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.15.00.000.bin		CHKSUM:0x22C1968


[Modify]
1.Update PD FW to 0x94 (Fix TypeC device no power @TypeC AC in)

[FanTable]
IDG_GX5MRXG_Thermal_Fan Control Table_20240426_R06.pptx

[SAPC]
SAPC_ GX4MRXL_20240429.xlsx

[ROMID]
- IDL Standard US Membraine Keyboard (IDL_STD_US.bat)
  0xFF 0xFF 0x01 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard UK Membraine Keyboard (IDL_STD_UK.bat)
  0xFF 0xFF 0x02 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard JP Membraine Keyboard (IDL_STD_JP.bat)
  0xFF 0xFF 0x03 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL XMG DE Membraine Keyboard (IDL_XMG_DE.bat)
  0x0C 0xFF 0x04 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL XMG US Membraine Keyboard (IDL_XMG_US.bat)
  0x0C 0xFF 0x01 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

- IDG Standard US/UK Membraine Keyboard (IDG_STD.bat)
  0xFF 0xFF 0xFF 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG MCJ JP Membraine Keyboard (IDG_MCJ_JP.bat)
  0x04 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG ThirdWave JP Membraine Keyboard (IDG_THW_JP.bat)
  0x08 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG XMG DE Membraine Keyboard (IDG_XMG_DE.bat)
  0x0C 0xFF 0x04 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG XMG US Membraine Keyboard (IDG_XMG_DE.bat)
  0x0C 0xFF 0x01 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF


---------------------------------------------------------------------------------
2024/09/23    		     EC Version 1.14.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.14.00.000.bin		CHKSUM:0x22BE5C4


[Modify]
1.Update PD FW to 0x93
2.Modify Safety Protect in TypeC Adaptor
3.Modify Smart APC table renew
4.Modify XMG Charge Led @S5 Low Battery

[FanTable]
IDG_GX5MRXG_Thermal_Fan Control Table_20240426_R06.pptx

[SAPC]
SAPC_ GX4MRXL_20240429.xlsx

[ROMID]
- IDL Standard US Membraine Keyboard (IDL_STD_US.bat)
  0xFF 0xFF 0x01 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard UK Membraine Keyboard (IDL_STD_UK.bat)
  0xFF 0xFF 0x02 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard JP Membraine Keyboard (IDL_STD_JP.bat)
  0xFF 0xFF 0x03 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL XMG DE Membraine Keyboard (IDL_XMG_DE.bat)
  0x0C 0xFF 0x04 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL XMG US Membraine Keyboard (IDL_XMG_US.bat)
  0x0C 0xFF 0x01 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

- IDG Standard US/UK Membraine Keyboard (IDG_STD.bat)
  0xFF 0xFF 0xFF 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG MCJ JP Membraine Keyboard (IDG_MCJ_JP.bat)
  0x04 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG ThirdWave JP Membraine Keyboard (IDG_THW_JP.bat)
  0x08 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG XMG DE Membraine Keyboard (IDG_XMG_DE.bat)
  0x0C 0xFF 0x04 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG XMG US Membraine Keyboard (IDG_XMG_DE.bat)
  0x0C 0xFF 0x01 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2024/08/19    		     EC Version 1.13.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.13.00.000.bin		CHKSUM:0x225C026


[Modify]
1.Modify IDL US Copilot Keyboard F12/PrtScr -> F12/Insert & Insert -> PrtScr
2.Modify Copilot Keyboard CoPilot/CoPilot -> CoPilot/RCtrl

[FanTable]
IDG_GX5MRXG_Thermal_Fan Control Table_20240426_R06.pptx

[SAPC]
SAPC_ GX4MRXL_20240429.xlsx

[ROMID]
- IDL Standard US Membraine Keyboard (IDL_STD_US.bat)
  0xFF 0xFF 0x01 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard UK Membraine Keyboard (IDL_STD_UK.bat)
  0xFF 0xFF 0x02 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard JP Membraine Keyboard (IDL_STD_JP.bat)
  0xFF 0xFF 0x03 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL XMG DE Membraine Keyboard (IDL_XMG_DE.bat)
  0x0C 0xFF 0x04 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL XMG US Membraine Keyboard (IDL_XMG_US.bat)
  0x0C 0xFF 0x01 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

- IDG Standard US/UK Membraine Keyboard (IDG_STD.bat)
  0xFF 0xFF 0xFF 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG MCJ JP Membraine Keyboard (IDG_MCJ_JP.bat)
  0x04 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG ThirdWave JP Membraine Keyboard (IDG_THW_JP.bat)
  0x08 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG XMG DE Membraine Keyboard (IDG_XMG_DE.bat)
  0x0C 0xFF 0x04 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG XMG US Membraine Keyboard (IDG_XMG_DE.bat)
  0x0C 0xFF 0x01 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2024/08/15    		     EC Version 1.12.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.12.00.000.bin		CHKSUM:0x225E6BA



[Modify]
1.Support XMG US Keyboard

[FanTable]
IDG_GX5MRXG_Thermal_Fan Control Table_20240426_R06.pptx

[SAPC]
SAPC_ GX4MRXL_20240429.xlsx

[ROMID]
- IDL Standard US Membraine Keyboard (IDL_STD_US.bat)
  0xFF 0xFF 0x01 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard UK Membraine Keyboard (IDL_STD_UK.bat)
  0xFF 0xFF 0x02 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard JP Membraine Keyboard (IDL_STD_JP.bat)
  0xFF 0xFF 0x03 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL XMG DE Membraine Keyboard (IDL_XMG_DE.bat)
  0x0C 0xFF 0x04 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL XMG US Membraine Keyboard (IDL_XMG_US.bat)
  0x0C 0xFF 0x01 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

- IDG Standard US/UK Membraine Keyboard (IDG_STD.bat)
  0xFF 0xFF 0xFF 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG MCJ JP Membraine Keyboard (IDG_MCJ_JP.bat)
  0x04 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG ThirdWave JP Membraine Keyboard (IDG_THW_JP.bat)
  0x08 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG XMG DE Membraine Keyboard (IDG_XMG_DE.bat)
  0x0C 0xFF 0x04 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG XMG US Membraine Keyboard (IDG_XMG_DE.bat)
  0x0C 0xFF 0x01 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2024/07/31    		     EC Version 1.11.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.11.00.000.bin		CHKSUM:0x225E0E5


[Modify]
1.Modify Smart APC release power budget
2.Modify LCD Backlight On
3.Modify Power LED
4.Modify Keyboard Back Light for XMG

[FanTable]
IDG_GX5MRXG_Thermal_Fan Control Table_20240426_R06.pptx

[SAPC]
SAPC_ GX4MRXL_20240429.xlsx

[ROMID]
- IDL Standard US Membraine Keyboard (IDL_STD_US.bat)
  0xFF 0xFF 0x01 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard UK Membraine Keyboard (IDL_STD_UK.bat)
  0xFF 0xFF 0x02 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard JP Membraine Keyboard (IDL_STD_JP.bat)
  0xFF 0xFF 0x03 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL XMG DE Membraine Keyboard (IDL_XMG_DE.bat)
  0x0C 0xFF 0x04 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

- IDG Standard US/UK Membraine Keyboard (IDG_STD.bat)
  0xFF 0xFF 0xFF 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG MCJ JP Membraine Keyboard (IDG_MCJ_JP.bat)
  0x04 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG ThirdWave JP Membraine Keyboard (IDG_THW_JP.bat)
  0x08 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG XMG DE Membraine Keyboard (IDG_XMG_DE.bat)
  0x0C 0xFF 0x04 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2024/07/05    		     EC Version 1.10.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.10.00.000.bin		CHKSUM:0x2252261


[Modify]
1.Modify CoPilot key
2.Modify Fan Control
3.Modify TccOffset
4.Support Moving Average Cpu temperature (XMG Only)
5.Fix XMG Keyboard

[FanTable]
IDG_GX5MRXG_Thermal_Fan Control Table_20240426_R06.pptx

[SAPC]
SAPC_ GX4MRXL_20240429.xlsx

[ROMID]
- IDL Standard US Membraine Keyboard (IDL_STD_US.bat)
  0xFF 0xFF 0x01 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard UK Membraine Keyboard (IDL_STD_UK.bat)
  0xFF 0xFF 0x02 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL Standard JP Membraine Keyboard (IDL_STD_JP.bat)
  0xFF 0xFF 0x03 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDL XMG DE Membraine Keyboard (IDL_XMG_DE.bat)
  0x0C 0xFF 0x04 0x14 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

- IDG Standard US/UK Membraine Keyboard (IDG_STD.bat)
  0xFF 0xFF 0xFF 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG MCJ JP Membraine Keyboard (IDG_MCJ_JP.bat)
  0x04 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG ThirdWave JP Membraine Keyboard (IDG_THW_JP.bat)
  0x08 0xFF 0x03 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF
- IDG XMG DE Membraine Keyboard (IDG_XMG_DE.bat)
  0x0C 0xFF 0x04 0x12 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2024/05/20    		     EC Version 1.09.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.09.00.000.bin		CHKSUM:0x22413BD

1.Modify CoPilot key
2.Fix TccOffset App default

---------------------------------------------------------------------------------
2024/05/03    		     EC Version 1.08.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.08.00.000.bin		CHKSUM:0x224BBEA

1.Support non-Uniwill 100W Type-C adaptor profile
2.Support 100W/85W switch by BIOS setup menu option
3.Modify XMG turbo mode TccOffset

---------------------------------------------------------------------------------
2024/04/26    		     EC Version 1.07.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.07.00.000.bin		CHKSUM:0x225406F

1.Modify Skin temperatureprote protection
2.Modify SAPC Standley Hybrid re-Charge
3.Reset Charg 10Hr timer after Hybrid re-Charge

---------------------------------------------------------------------------------
2024/04/19    		     EC Version 1.06.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.06.00.000.bin		CHKSUM:0x2256EC8

1.Delay power on after NonSpec turn On Vs for MPS read while Init state @Battery mode
2.Support NV OVRM check for GPU connection
3.Add PD flash retry to avoid dead loop
4.Modify P80 initial RAM
5.Modify Oemservice jack adaptor power setting

---------------------------------------------------------------------------------
2024/04/12    		     EC Version 1.05.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.05.00.000.bin		CHKSUM:0x22497A2

1.Support RGB KB Back light Level Single area 0,1,2,3,4, Single Color 0,2,4
2.Support Co-Pilot Key for XMG

---------------------------------------------------------------------------------
2024/04/03    		     EC Version 1.04.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.04.00.000.bin		CHKSUM:0x2253336

1.Modify KB Back Light 4Level(0,1,2,3,4) -> 2Level(0,2,4)
2.Modify Default KB Matrix be IDL-US for SMT request
3.Modify LCtrl+Space+QAZX block by Ghost Key prevent
4.Modify MCJ DC battery boot @ low temperature(6'C) & low RSOC(30%)

---------------------------------------------------------------------------------
2024/03/28    		     EC Version 1.03.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.03.00.000.bin		CHKSUM:0x2262374

1.Update PD FW to 006

---------------------------------------------------------------------------------
2024/03/26    		     EC Version 1.02.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.02.00.000.bin		CHKSUM:0x2260E46

1.Support XMG KB (with ROMID)
2.Delay Type C PD Adaptor Warning LED after power boot

---------------------------------------------------------------------------------
2024/03/20    		     EC Version 1.01.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.01.00.000.bin		CHKSUM:0x22762D4

1.Update PD FW to 058
2.Modify Charger Adaptor current limit 5.1A @Uniwill 100W
3.Modify 99W Battery charge current to 5.5A @Uniwill 100W Adaptor S5
4.Modify Ivan Hybrid re-Charge RSOC>100% -> RSOC>94% for meet Self-Discharge rule <=93% re-Charge
5.Modify SAPC Standley Hybrid re-Charge
6.Modify SAPC (PL & Battery current calculate & trigger current)
7.Modify DC boot post PL 40 40 80
8.Modify IDG MCJ KB 
9.Modify ZeroI High loading condition
10.Workaround force pseudo G3 after Shiiping mode first Wake Up 
11.Disable USB Nkey KB support

---------------------------------------------------------------------------------
2024/03/08    		     EC Version 1.00.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_1.00.00.000.bin		CHKSUM:0x22594E9

1.Update PD FW to 054
2.Modify SAPC for Hybrid re-Charge
3.Modify PL1/2 70W @Turbo 
4.Modify GPU ModuleID (0x7D2)
5.Modify TP SAT GPIO release @S0

---------------------------------------------------------------------------------
2024/03/01    		     EC Version 0.22.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.22.00.000.bin		CHKSUM:0x2259851

1.Update PD FW to 053
2.Workaround for IDL US KB Ghost Key Win+Fn+F12(PrtSC) -> Win+F12(PrtSC)
3.Modify SAPC for Hybrid re-Charge

---------------------------------------------------------------------------------
2024/02/22    		     EC Version 0.21.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.21.00.000.bin		CHKSUM:0x22646CF

1.Update PD FW to 050
2.Support OZ Charger 1.5V Gap WA (Enable)

---------------------------------------------------------------------------------
2024/02/21    		     EC Version 0.20.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.20.00.000.bin		CHKSUM:0x2268536

1.Update PD FW to 069
2.Modify GX Project ID for AP
3.Fix Plug In/Out rapidly will cause RSOC=0% @Shipping mode resume

---------------------------------------------------------------------------------
2024/02/19    		     EC Version 0.19.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.19.00.000.bin		CHKSUM:0x22AE345

1.Modify Plug In Init Power Sequence
2.Modify Pseudo G3 VA on/off delay
3.Modify PD Modern Standby command 03->02
4.Modify PD Adaptor VID/PID check to PID Only
5.Modify CPU temperature protect shutdown point (Thermal Fan table R05)
6.Modify Type C Adaptor (Port1 TBT4 <45W, Port2 NoTBT4 <60W) disable @S0
7.Modify DC JACK plug in check

---------------------------------------------------------------------------------
2024/02/07    		     EC Version 0.18.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.18.00.000.bin		CHKSUM:0x22ADA05

1.Modify Smart APC
2.Modify CPU temperature protect shutdown point
3.Modify Charger Adaptor current limit
4.Modify CPU temperature calculate
5.Modify Fan table
6.Modify PD version reading
7.Support Charger 1.5V Gap WA (disable)

---------------------------------------------------------------------------------
2024/02/02    		     EC Version 0.17.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.17.00.000.bin		CHKSUM:0x22AFACC

1.Update PD FW to 005
2.Support Type-C Adaptor VID/PID identify with PD FW
3.Modify Charging current @S5
4.Modify SAPC PL4 @Balance mode

---------------------------------------------------------------------------------
2024/01/26    		     EC Version 0.16.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.16.00.000.bin		CHKSUM:0x22E4357

1.Update PD FW to 060
2.Modify Workaround for ADAP_IN Glitch 
3.Modify OOB Scan time (CpuTemp/PLx)
4.Modify Thermal Test Mode release
5.Modify IDG STD KB
6.Fix "Win Lock/Unloc" OSD while KB Backlight cycle to Maximum
7.Disable OC Control/Memory OC

---------------------------------------------------------------------------------
2024/01/19    		     EC Version 0.15.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.15.00.000.bin		CHKSUM:0x22DDDFA

1.Update PD FW to 077
2.Modify Turbo mode PL4=217
3.Modify Battery Hybrid boost current Limit 8A->14A
4.Modify Thermal Remote temperature protect point
5.Modify CPU temperature protect shutdown Lastest High point.
6.Modify Adaptor current setting scan
7.Workaround for ADAP_IN Glitch
8.Fix first AC in detect delay
9.Fix Battery Low LED
10.Support Retimer Update with BIOS

---------------------------------------------------------------------------------
2024/01/12    		     EC Version 0.14.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.14.00.000.bin		CHKSUM:0x22F217F

1.Update PD FW to 076
2.Modify Cpu temperature Throttling
3.Modify UCSI for WHQL
4.Modify PD power state command
5.Modify Tcc offset
6.Modify Thermal Remote temperature protect
7.Modify SAPC turbo mode PL124
8.Support PD declare source output current down while Battery Discharge Current Throttling
9.Support Display Change status
10.Support IDG STD JP KB

---------------------------------------------------------------------------------
2024/01/05    		     EC Version 0.13.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.13.00.000.bin		CHKSUM:0x22FD267

1.Modify Smart APC PD AC3 Mode >45W ~ <60W
2.Modify Battery Charge Current >45W ~ <60W 1A @S0
3.Modify Battery Discharge Current Throttling
4.Support Enable/Disable PD source port @BatI Throttling
5.Fix Battery Healthy 4.0 age issue

---------------------------------------------------------------------------------
2023/12/29    		     EC Version 0.12.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.12.00.000.bin		CHKSUM:0x230763A

1.Modify KB Map IDL/IDG
2.Modify Type C Adaptor Change indicate
3.Modify Thermal Safety protect PROCHOT->PL12=10

---------------------------------------------------------------------------------
2023/12/25    		     EC Version 0.11.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.11.00.000.bin		CHKSUM:0x230DC8F

1.Update PD FW to 073
2.Support FanLock protect
3.Support Thermistor temperature protect
4.Modify Smart APC trig condition
5.Modify Smart APC Charging current for performance priority
6.Modify Charge IC Adaptor current Limit @DC
7.Modify Wake On Lan Power on/off
8.Modify power USB charging @S5
9.Modify PseudoG3 condition
10.Modify Battery discharge current protect 7.5A

---------------------------------------------------------------------------------
2023/12/18    		     EC Version 0.10.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.10.00.000.bin		CHKSUM:0x2361ACC

1.Update PD FW to 089
2.Support Pseudo G3 Enable/Disable by BIOS setup
3.Modify Battery low RSOC<4% shutdown @NoOS
4.Modify Charge current down @SAPC for performance priority
5.Modify Fan kick off 3sec->10sec
6.Modify SAPC
7.Modify KB back Light @NoAPP
8.Modify Zero I Calculate
9.Modify Shipping mode indicate
10.Fix IDL KB "del" key
11.Battery coefficient work around

---------------------------------------------------------------------------------
2023/12/08    		     EC Version 0.09.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.09.00.000.bin		CHKSUM:0x22EC4C0

1.Modify Pseudo G3 detect
2.Modify Type C Adaptor Uniwill 100W VID/PID detection (no work now)
3.Modify Adaptor setting by OEM service
4.Modify USB power @Power Off
5.Modify Smart APC table structure
6.Modify diode keyboard 850 scan table
7.Modify Fn Key function for IDL US/UK/JP (depends on ROMID)
8.Fix Fn Key repeat while Fn release first
9.Fix preCharge stop @low tempature
10.Support EShutter controll

---------------------------------------------------------------------------------
2023/12/01    		     EC Version 0.08.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.08.00.000.bin		CHKSUM:0x2315EBA

1.Enable LID switch
2.Enable Pseudo G3 detect @S5
3.Modify Cpu Tempature calculate
4.Modify KB US/UK
5.Modify Battery Boost mode
6.Modify MPS update password
7.Modify PD System State command @S5
8.Modify Battery mode S5 suicide
9.Fix Audio crack @Power On mute

---------------------------------------------------------------------------------
2023/11/21    		     EC Version 0.07.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.07.00.000.bin		CHKSUM:0x22FCFE7

1.Support Battery Shipping mode (disable)
2.Support PD Compliance mode (disable)
3.Support MPS update password/checksum (disable)
4.Modify Adaptor current limit
5.Modify Adaptor power calculate
6.Modify WK3081 
7.Modify USB power @Power Off

---------------------------------------------------------------------------------
2023/11/17    		     EC Version 0.06.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.06.00.000.bin		CHKSUM:0x22F84A4

1.Update PD FW to 003
2.Modify Fan table
3.Modify Smart APC
4.Modify Charge current
5.Modify Fan control/Fan boost (step out)
6.Modify Tcc offset
7.Modify Lan Power 
8.Modify Adaptor power calculate
9.Modify PD power level check (U100W)
10.Modify EC service password
11.Modify power button long push shutdown 4.8sec->12sec
12.Modify WK3081 power on/off sequence
13.Enable WK3081
14.Swap membrane KB 'U' & 'K'
15.Support PD Compliance Mode (disable)

---------------------------------------------------------------------------------
2023/11/03    		     EC Version 0.05.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.05.00.000.bin		CHKSUM:0x22B023D

1.Update PD FW to 097
2.Support Mode LED
3.Modify Charging current
4.Modify Smart APC
5.Modify Adaptor Watt calculate
6.Disable Workaround 3000
7.Disable LID switch for temporary
8.Fix Discharge to S4 and restart RSOC be 0%->5%

---------------------------------------------------------------------------------
2023/10/25    		     EC Version 0.04.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.04.00.000.bin		CHKSUM:0x232E5AE

1.Update PD FW to 093
2.Modify Charging LED
3.Modify Modern standby LED
4.Modify Tcc Offset
5.Modify App set PL124 @TypeC Adaptor
6.Support MPS read temperature
7.Support Thermistor temperature
8.Set Charge IC Max boost current 8A@10mOhm
9.Disable GPU exist
10.Support AbNormal LED

---------------------------------------------------------------------------------
2023/10/16    		     EC Version 0.03.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.02.00.000.bin		CHKSUM:0x231EAF0

1.Update PD FW to 091
2.Modify Type C Loading switch (with DC IN FDS switch)
3.Modify battery S5 suicide resume reset
4.Modify Adaptor/TypeC current sense resistor switch (10mOhm/2.5mOhm)
5.Modify Power On sequence S5->S0
6.Support Membranes/Diode Keyboard (with ROM ID)
7.Add Caps/Num Lock LED
8.Fix ACover LED power

---------------------------------------------------------------------------------
2023/10/06    		     EC Version 0.02.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.02.00.000.bin		CHKSUM:0x23C2178

1.Modify EDP GPIO & Sequence
2.Modify Mute GPIO
3.Modify MPS ReadVer/Update
4.Modify EC Init G3 Sequence
5.Modify Power On/Off Sequence
6.Modify Power Sw overwrite bug
7.Modify 66DC Flash end power off Sequence
8.Modify OOB write package
9.Modify PD read bin @PD2
10.Enable PD update FW 0.01
11.Enable MPS ReadVer
12/Disable SUS PWRDN G3
13.Disable Thermo safety (PROCHOT by FanLock)
14.Set Battery Charge current 2A @All situation

---------------------------------------------------------------------------------
2023/09/12    		     EC Version 0.01.00.000	      Owner: Ryan Luo
---------------------------------------------------------------------------------
File name: GXxMxxx_0.01.00.bin		CHKSUM:0x2437811

1.First release for Phase-A SMT (W/O PD FW)


