# Supported Adapters

Intel® iSCSI Remote Boot is designed to operate with PCI-Express* based Intel® Server Adapters. Intel® iSCSI Remote Boot is supported on the following devices:

Product Name | Controller
--- | ---
Intel® PRO/1000 PT Quad Port Server Adapter | 82571EB
Intel® PRO/1000 PT Quad Port LP Server Adapter | 82571EB
Intel® PRO/1000 PF Quad Port Server Adapter | 82571EB
Intel® PRO/1000 PT Dual Port Network Connection1 | 82571EB
Intel® PRO/1000 PT Dual Port Server Adapter | 82571EB
Intel® PRO/1000 PB Dual Port Server Connection1 | 82571EB
Intel® PRO/1000 PF Dual Port Server Connection1 | 82571EB
Intel® PRO/1000 PF Dual Port Server Adapter | 82571EB
Intel® PRO/1000 PT Network Connection1 | 82572EI
Intel® PRO/1000 PT Server Adapter | 82572EI
Intel® PRO/1000 PF Network Connection1 | 82572EI
Intel® PRO/1000 PF Server Adapter | 82572EI
Intel® PRO/1000 PB Server Connection1 | 82572EI
Intel® PRO/1000 EB Network Connection with I/O Acceleration1 | 80003ES2LAN
Intel® PRO/1000 EB Backplane Connection with I/O Acceleration1 | 80003ES2LAN
Intel® PRO/1000 EB1 Network Connection with I/O Acceleration1 | 80003ES2LAN
Intel® PRO/1000 EB1 Backplane Connection with I/O Acceleration1 | 80003ES2LAN
Intel® 82575EB Gigabit Network Connection1 | 82575EB
Intel® 82575EB Gigabit Backplane Connection1 | 82575EB
Intel® Gigabit VT Quad Port Server Adapter | 82575
Intel® Gigabit PT Quad Port Server ExpressModule | 82571
Intel® 82598EB 10 Gigabit AF Dual Port Network Connection1 | 82598
Intel® 82598EB 10 Gigabit AF Network Connection1 | 82598
Intel® 82598EB 10 Gigabit AT CX4 Network Connection1 | 82598
Intel® 10 Gigabit XF SR Server Adapter | 82598
Intel® 10 Gigabit XF LR Server Adapter | 82598
Intel® 10 Gigabit XF SR Dual Port Server Adapter | 82598
Intel® 82566DM-2 Gigabit Network Connection | 82566DM-2
Intel® 10 Gigabit CX4 Dual Port Server Adapter | 82598EB

1Requires iSCSI remote boot support in the system BIOS.

`Last modified on 2/14/08 3:56p Revision 16`